;
; VAG-COM Measuring Block Labels Template file.; TDi 1.9 ( 1Z engine) ECU 028 906 021 xxx
;
; 
; thank's  Mike Sauve www.alientech.net
; testing and modification Claudio Gonella www.mectronik.com
; (31/03/2001)

1,0,Injected Quantity
1,1,Engine speed,861-945
1,2,Injection Quantity,3-9
1,3,Mod. Piston Displ.,1.35-2.10
1,4,Coolant Temp.,80-110

2,0,Idle display
2,1,Engine speed,861-945
2,2,Throttle Position,0
2,3,Operating Cond/AC,speed/throttle/AC
;xxx
;1   Idle speed increased because compressor is on
; 1  Throttle Position switch closed
;  1 Air Cond. compressor on
2,4,Coolant Temp,80-110

3,0,EGR
3,1,Engine speed,861-945
3,2,MAF (specified),240-340
3,3,MAF (actual),240-340
3,4,EGR duty cycle,4-84

4,0,Start of Injection
4,1,Engine speed,861-945
4,2,Specified start,2 to -3
4,3,Actual start,2 to -3
4,4,Cold Start Valve,3-70

5,0,Starting conditions
5,1,Engine speed,
5,2,Start Inj Qty,
5,3,Actual Start of Inj,
5,4,Coolant temp,

6,0,Switch positions
6,1,Speed,
6,2,Brake Pedal,F/F47/F36 
; xxx 
; 1    switch F closed
;  1   switch F47 open (Brake switch)
;   1  switch F36 open (Clutch vacuum vent valve)

6,3,Cruise Control,Cl/Br/Re/Ac/on/on
; xxxxxx
; 1      Clutch pedal operated
;  1     Brake pedal operated
;   1    Resume/acceleration
;    1   Acceleration
;     0  CC switched off (momentary)
;      0 CC switched off (permanent)
6,4,Cruise present?,
;1.0 = normal?
;17.0 = brake pressed?

7,0,Temperatures
7,1,Fuel Temp,
7,2,n/a
7,3,Intake Air Temp,
7,4,Coolant Temp,

8,0,Injection Quantities? (undocumented)
8,1,Engine speed
8,2,Inj qty,?
8,3,Inj qty,?
8,4,Inj qty,?

9,0,Injected quantity limitation
9,1,Engine speed,
9,2,Injection Quantity,CC active
9,3,Inj limit,during a/t shift
9,4,,

10,0,Air system
10,1,Mass Air Flow,
10,2,Barometric,Pressure
10,3,Manifold ,Pressure
10,4,Position,Throttle

11,0,Manifold Air Pressure
11,1,Engine speed,
11,2,Specified MAP,
11,3,Actual MAP,
11,4,Duty cycle,Boost Valvle

12,0,Glow plugs (see label file for #1)
12,1,Glow status,all 1's=off
; xxxxxxxx
; 11111111 Glowing off
; 00010000 Pre-glow
; 01110000 Start of glow
; 11110000 Interim glow
; 10110000 Post-glow
; 00110000 Readiness glowing
12,2,Pre-glow period,
12,3,Supply Voltage,
12,4,Coolant Temp,

13,0, Idle speed smooth running adjustments
13,1,Cyl 1,-2 to +2
13,2,Cyl 2,-2 to +2
13,3,Cyl 3,-2 to +2
13,4,Cyl 4,-2 to +2

15,0,Fuel consumption
15,1,Engine speed,
15,2,Inj Qty (actual),
15,3,Fuel Consumption,
15,4,Inj Qty requested,(accelerator)

16,0,Auxiliary heater
16,1,Generator loading,
16,2,Aux. heat,(see label file)
; xxxxxxxx
; 1        Not relevant
;  1       Not relevant
;   1      Coolant Temp. sensor G62 or IAT sensor G72 faulty
;    1     Engine start in last 10 seconds
;     1    Engine below 760 RPM
;      1   Battery below 9 volts
;       1  Generator faulty
;        1 Coolant temp > 70-80C or IAT > 5C
16,3,Activation,Hi/Lo
; xx
; 1  High heat output,J360 on
;  1 Low heat output,J459 on
16,4,Voltage supply,
;
;end



