;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Audi A4 (8EC/8ED)
;
; Component: J285 - Instrument cluster (#17)
;
; P/N: 8E0-920-9??-??
;
; includes measuring blocks, adaptation, coding,
;          security access and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8E-17.LBL
; 8E0-920-9xx-8E2.LBL
; 8E0-920-9xx-8EC.LBL
;
; created on 07/Sep/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 21/Sep/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Remote Clock,Receiver Status,Range: OK/not OK
002,3,Comfort-CAN,Information,xx0 - Left-Hand-Drive (LHD)\nxx1 - Right-Hand-Drive (RHD)\nx1x - 4-Door\n1xx - Temperature Display in °F
002,4,Outside,Temperature
;
003,0,General
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
004,0,Fuel Level Sensor
004,1,Fuel Display,(1st Sensor)
004,2,Fuel Sensor,(1st Sensor)
004,3,Fuel Display,(2nd sensor),All-Wheel-Drive only
004,4,Fuel Sensor,(2nd sensor),All-Wheel-Drive only
;
005,0,Service Reminder
005,1,Distance,before/after Service,Unit: 100 km
005,2,Time,before/after Service,Unit: 1 day(s)
005,3,Engine Hood,Contact,Range: Open/Closed
005,4,Calculated,Service Interval
;
006,0,Oil Level I
006,1,Min. Oil Level,in Service Interval
006,2,Max. Oil Level,in Service Interval
006,3,100 km Average,Oil Level Dif.
;
007,0,Oil Level II
007,1,Current,Oil Level
007,2,Oil Level,Threshold,Current Value from ECU
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...8
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)
; 4 - New Customer Service / Delivery Condition (Replacement Instrument Cluster)
; 5 - Customer Service locked / Adaptation Data Programmed in Customer Service
; 6 - Immobilizer adapted / Normal Function Condition
; 7 - Key Adaptation active
;
024,0,Immobilizer III
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Identification Number (VIN) & Serial Number
;
082,0,Advanced Control Module Identification III
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nRange: Engine 0/Engine 1
125,2,Transmission
125,3,Brake Electronics,(J104),Specification: ABS 1\nRange: ABS 0/ABS 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Airbag,(J234),Specification: Airbag 1\nRange: Airbag 0/Airbag 1
126,2,Headlight Range,,Specification: HdLtRange 1\nRange: HdLtRange 0/HdLtRange 1
;
130,0,CAN-Databus Communication (Comfort)
130,3,Comfort System,(J393),Specification: Central 1\nRange: Central 0/Central 1
;
131,0,CAN-Databus Communication (Comfort)
131,1,Central Electronics,(J519),Specification: Cent Elec 1\nRange: Cent Elec 0/Cent Elec 1
131,2,Steering Column,Electronics (J527),Specification: St. Wheel 1\nRange: St. Wheel 0/St. Wheel 1
131,3,Climate Control,(J255),Specification: A/C 1\nRange: A/C 0/A/C 1
131,4,Status,CAN-Comfort,Specification: 2-Wire\nRange: 1-Wire/2-Wire
;
132,0,CAN-Databus Communication (Comfort)
132,1,Convertible Top
;
140,0,CAN-Databus Communication (Infotainment)
140,1,Radio,,Specification: Radio 1\nRange: Radio 0/Radio 1
;
141,0,CAN-Databus Communication (Infotainment)
141,4,Status,CAN-Infotainment,Specification: 2-Wire\nRange: 1-Wire/2-Wire
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??xxx: Options I
C02,+01 = Smaller Fuel Tank Volume (All-Wheel-Drive)
C03,+02 = Side Marker Lights Indicator Lamp inactive
C04,+04 = 3. K-Number (Rental Cars)
C05,+08 = 2. K-Number (Australia)
C06,+16 = Clutch Pedal Switch Operation in FIS Display
C07,00xx?xx: Country
C08,0 = Germany (D) / 1 = Rest of World (RoW) / 2 = USA (US)
C09,3 = Canada (CAN) / 4 = Great Britain (GB) / 5 = Japan (JP)
C10,6 = Saudi Arabia / 7 = Australia (AUS)
C11,00xxx?x: Seatbelt Warning
C12,0 = No Seatbelt Warning
C13,1 = Seatbelt Warning Europe-NCAP
C14,2 = Seatbelt Warning USA and Canada (NAR old)
C15,3 = Seatbelt Warning USA and Canada (NAR new)
C16,4 = Seatbelt Warning Europe-NCAP (incl. passenger)
C17,5 = Seatbelt Warning USA and Canada old (incl. passenger)
C18,6 = Seatbelt Warning USA and Canada NAR new (incl. passenger)
C19,00xxxx?: Options II
C20,1 = Standard (< 11/2006)
C21,4 = Washer Fluid Warning inactive (11/2006 >)
C22,8 = Washer Fluid Warning active (11/2006 >)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S0,Instrument Cluster (J285) Security Access
S1,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 5 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,8 = Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
A009,11, 
A009,12,NOTE: Perform Security Access with "13861" first.
;
A018,0,Auxiliary Heating
A018,5,Auxiliary Heating
A018,6,000?x: Engine pre-warm-up
A018,7,0 = without Engine pre-warm-up
A018,8,1 = with Engine pre-warm-up
A018,9, 
A018,10,000x?: Auxiliary Heating
A018,11,0 = No Auxiliary Heating installed
A018,12,1 = Auxiliary Heating installed
A018,13,2 = Auxiliary Heating installed but OFF when turning engine OFF
A018,14,3 = Only Auxiliary Ventilation installed
A018,15,4 = Only Auxiliary Ventilation but OFF when turning engine OFF
;
A019,0,Additional Features
A019,5,Additional Features
A019,6,?xxxx: Illumination
A019,7,0 = Needle and Scale only active at "Light ON"
A019,8,1 = Needle already active at "Ignition ON"
A019,9,2 = Scale already active at "Ignition ON"
A019,10,3 = Scale (2nd Map) and Needle at "Ignition ON" active
A019,11,x?xxx: Board computer
A019,12,0 = only Level 2 (Long Time Memory)
A019,13,1 = Level 1 and 2
A019,14,xx?xx: Driver Information System (DIS)
A019,15,0 = DIS
A019,16,1 = Highline without DIS
A019,17,2 = DIS with Menu Guide
A019,18,3 = DIS with Menu Guide and Unit Changing
A019,19,xxx?x: Lap Timer
A019,20,+1 = Lap Timer active (RS4 only)
A019,21,xxxx?: Remote Clock
A019,22,+1 = Remote Clock active
A019,23,+2 = Sport Seats installed (RS4 only)
;
A021,0,Immobilizer (Key Adaptation)
;
A029,0,Tank Characteristic (Fuel Level Sensor 2)
A029,5,Tank Characteristic (Fuel Level Sensor 2)
A029,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A029,7, 
A029,8,Standard Value: 128
A029,9,Value Range: 96...160 (-8.0...+8.0 l)
A029,10,Increments: 1 = 1 Ohm = 1/4 l
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A030,7, 
A030,8,Standard Value: 128
A030,9,Value Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A032,0,Tank Characteristic (Not detactable Tank Volume)
A032,5,Tank Characteristic (Not detactable Tank Volume)
A032,6,The tank volume which is not recordable by the fuel gauge sender(s).
;
A033,0,Tank Characteristic (Full Calibration)
A033,5,Tank Characteristic (Full Calibration)
A033,6,Non-parallel shift of the tank characterictic above a readout of 1/2.
A033,7,To start the adaptation enter '65535' as new value.
A033,8, 
A033,9,Standard Value: 128
A033,10,Value Range: 112...144 (-4.0...+4.0 l)
A033,11,Increments: 1 = 1 Ohm = 1/4 l
;
A034,0,Tank Characteristic (Dry Calibration)
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold for the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
A038,8,0 = Oil Minimum Detection not activated
A038,9,1 = Oil Minimum Detection activated
A038,10, 
A038,11,NOTE: Perform Security Access first.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
A039,7,0 = TOG Evaluation from the Instrument Cluster not activated
A039,8,1 = TOG Evaluation from the Instrument Cluster activated
A039,9, 
A039,10,NOTE: Perform Security Access first.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km/mi
A040,7, 
A040,8,NOTE: Adaptation channels 040-049 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 040-049 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km/mi
A042,7,00080 = fixed Service Intervals (8.000 km - w/o Longlife)
A042,8,00150 = flexible Service Intervals (15.000 km - with Longlife)
A042,9,or (if coded to miles)
A042,10,00050 = fixed Service Intervals (5.000 mi - w/o Longlife)
A042,11,00090 = flexible Service Intervals (9.000 mi - with Longlife)
A042,12, 
A042,13,NOTE: Adaptation channels 040-049 must be
A042,14,entered and stored in the following order:
A042,15,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,00080 = fixed Service Intervals (8.000 km - w/o Longlife)
A043,8,00300 = flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00050 = fixed Service Intervals (5.000 mi - w/o Longlife)
A043,11,00190 = flexible Service Intervals (19.000 mi - with Longlife)
; 00186 = flexible Service Intervals (19.000 mi - with Longlife - Seat Exeo Diesel Engines)
; 00190 = flexible Service Intervals (19.000 mi - with Longlife - Seat Exeo Gasoline Engines)
A043,12, 
A043,13,NOTE: Adaptation channels 040-049 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 040-049 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
A045,8,3 = Diesel Engines with Immobilizer III
A045,9, 
A045,10,NOTE: Adaptation channels 040-049 must be
A045,11,entered and stored in the following order:
A045,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
A046,8, 
A046,9,NOTE: Adaptation channels 040-049 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 040-049 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 040-049 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 = fixed Service Intervals (w/o Longlife)
A049,8,00365 = flexible Service Intervals (Gasoline Engines with Longlife)
A049,9,00730 = flexible Service Intervals (Diesel Engines with Longlife)
A049,10, 
A049,11,NOTE: Adaptation channels 040-049 must be
A049,12,entered and stored in the following order:
A049,13,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A060,0,CAN-Databus Powertrain (Installation List)
A060,5,CAN-Databus Powertrain (Installation List)
A060,6,+00001 = Engine (Standard)
A060,7,+00002 = Automatic Transmission OR Shift Indicator (Optional)
A060,8,+00004 = Brake (Standard)
A060,9,+00016 = Airbag (Standard)
A060,10,+00064 = Headlight Leveling
A060,11,+00128 = Headlight Leveling with Curve Light (AFS)
A060,12,+01024 = Instrument Cluster (Standard)
;
A061,0,CAN-Databus Comfort (Installation List)
A061,5,CAN-Databus Comfort (Installation List)
A061,6,+00001 = Central Electronics (Standard)
A061,7,+00002 = Comfort System (Standard)
A061,8,+00064 = Trailer (Optional)
A061,9,+00128 = Convertible Top (Optional)
A061,10,+00256 = Instrument Cluster (Standard)
A061,11,+00512 = Tire Pressure Control (Optional)
A061,12,+01024 = Steering Column Electronics (Standard)
A061,13,+02048 = Climate Control (Standard)
A061,14,+32768 = Auxiliary Heating (Optional)
;
A062,0,CAN-Databus Infotainment (Installation List)
A062,5,CAN-Databus Infotainment (Installation List)
A062,6,+00001 = Radio (Optional)
A062,7,+00002 = Telephone OR US-Telematics (Optional)
A062,8,+00004 = Navigation (Optional)
A062,9,+00008 = Telematics (Optional)
A062,10,+00016 = Intrument Cluster (Standard - only coded with 2nd Component)
;
A099,0,Transport Mode
A099,5,Transport Mode
A099,6,0 = inactive
A099,7,1 = active
A099,8, 
A099,9,Some Head units require a seperate transport mode
A099,10,deactivation (Adress 56 - Adaptation channel 099).
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,100,DIST
RD,43,Max Mileage to Service,100,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
RD,46,Total Consumption,100,DIST
RD,47,Soot Quantity,100,DIST
RD,48,Thermal Load,100,DIST
RD,49,Min Time to Service,1,Days
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
