;
; VCDS Label File
;
; Copyright © 2007-2010 Ross-Tech, LLC
;
; VW Polo (6N)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6N0-919-???-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6N-17.LBL
; 6N0-919-xxx-17.LBL
; 6N0-920-xxx-17.LBL
;
; created on 05/Nov/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 22/Jan/2010
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
;
003,0,General
003,1,Coolant,Temperature
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+02 = Seatbelt Warning active
C03,xx?xx: Country
C04,1 = Europe
C05,4 = Great Britain (GB)
C06,xxx?x: Cylinders
C07,4 = 4-Cylinders
C08,xxxxx?: Distance Impulse Number (K-Value)
C09,1 = Standard
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A005,0,Maximum Distance to Oil Service (OEL)
A005,5,Maximum Distance to Oil Service (OEL)
A005,6,15 = 15.000 km (Standard)
A005,7,or (if coded to miles)
A005,8,10 = 10.000 mi (Standard)
A005,9, 
A005,10,Resolution: 1 = 1000 km/mi
;
A006,0,Maximum Distance to Inspection (IN1)
A006,5,Maximum Distance to Inspection (IN1)
A006,6,30 = 30.000 km (Standard)
A006,7,or (if coded to miles)
A006,8,20 = 20.000 mi (Standard)
A006,9, 
A006,10,Resolution: 1 = 1000 km/mi
;
A007,0,Maximum Time to Inspection (IN2)
A007,5,Maximum Time to Inspection (IN2)
A007,6,12 = 12 Month (Standard)
A007,7, 
A007,8,Resolution: 1 = 1 Month
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Resolution: 1 = 10 km/mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
;
A010,0,Distance to Oil Service (OEL)
A010,5,Distance to Oil Service (OEL)
A010,6,150 = 15.000 km (Standard)
A010,7,or (if coded to miles)
A010,8,100 = 10.000 mi (Standard)
A010,7, 
A010,8,Resolution: 1 = 100 km/mi
;
A011,0,Distance to Inspection (IN1)
A011,5,Distance to Inspection (IN1)
A011,6,300 = 30.000 km (Standard)
A011,7,or (if coded to miles)
A011,8,200 = 20.000 mi (Standard)
A011,9, 
A011,10,Resolution: 1 = 100 km/mi
;
A012,0,Time to Inspection (IN2)
A012,5,Time to Inspection (IN2)
A012,6,360 = 360 Days (Standard)
A012,7, 
A012,8,Resolution: 1 = 1 Days
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Maximum Distance to Oil Service (OEL),1000,DIST
RD,6,Maximum Distance to Inspection (IN1),1000,DIST
RD,7,Maximum Time to Inspection (IN2),1,Month
RD,10,Distance to Oil Service (OEL),100,DIST
RD,11,Distance to Inspection (IN1),100,DIST
RD,12,Time to Inspection (IN2),1,Days
;
RJ,0,0,Service Reset (OIL / Kilometers),,
RJ,0,1,10,150
;
RJ,1,0,Service Reset (INSP / Kilometers),,
RJ,1,1,10,150
RJ,1,2,11,300
;
RJ,2,0,Service Reset (OIL &  INSP / Kilometers),,
RJ,2,1,10,150
RJ,2,2,11,300
RJ,2,3,12,360
;
RJ,3,0,Service Reset (OIL / Miles),,
RJ,3,1,10,100
;
RJ,4,0,Service Reset (INSP / Miles),,
RJ,4,1,10,100
RJ,4,2,11,200
;
RJ,5,0,Service Reset (OIL &  INSP / Miles),,
RJ,5,1,10,100
RJ,5,2,11,200
RJ,5,3,12,360
;
