;
; VCDS Label File
;
; Copyright © 2010 Ross-Tech, LLC
;
; Seat Leon/Toledo (1M)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 1M0-919-???-???
;
; includes measuring blocks, adaptation, coding, login
;          and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1M-17.LBL
; 1M0-919-xxx.LBL
; 1M0-920-xx0.LBL
; 1M0-920-xx2.LBL
;
; created on 12/Aug/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Aug/2010
;
; requires VCDS 10.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
020,0,Immobilizer - ID Block 1
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer - ID Block 2
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,7 = No Text
A004,13,8 = Czech
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
;
A010,0,Service Reminder: Distance to Oil Service "OIL"
A010,5,Service Reminder: Distance to Oil Service "OIL" (in 1000 km)
A010,6,15 = 15.000 km (Standard)
;
A011,0,Service Reminder: Distance to Inspection "INSP 01"
A011,5,Service Reminder: Distance to Inspection "INSP 01" (in 1000 km)
A011,6,30 = 30.000 km (Standard)
;
A012,0,Service Reminder: Time to Inspection "INSP 02"
A012,5,Service Reminder: Time to Inspection "INSP 02" (in 10 Days)
A012,6,37 = 370 Days (Standard)
;
A016,0,Distance Impulse Number
A016,5,Distance Impulse Number
A016,6,The displayed value cannot be modified.
;
A021,0,Immobilizer (Key Adaptation)
A021,3,Key Count
A021,5,Immobilizer (Key Adaptation)
A021,6,Prior to Adapting new Keys the Adaptation has to be enabled by
A021,7,logging in using the Immobilizer PIN/SKC. The Adaptation Value
A021,8,is the number of all Keys to be adapted (Maximum 8).
A021,9,After Saving the Adaptation Value the first Key is adapted.
A021,10,Proceed until all Keys are adapted:
A021,11,- Switch the Ingnition OFF and take out the Key.
A021,12,- Switch the Ignition ON using the next Key.
A021,13,- The Immobilizer Lamp should light up for 2 Seconds and then switch OFF.
A021,14,- The Key is now adapted.
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,Standard: 0
A035,11,Range: 0...1000 U/min
A035,12,Increments: 250 U/min
;
;
;---------------------------------------------------
;
; Codierung
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,+01 = Brake Pad Warning installed
C03,+02 = Seatbelt Warning installed
C04,+04 = Washer Fluid Warning installed
C05,+16 = Secondary Display (Radio/Navigation) installed
C06,xx?xx: Country
C07,1 = Europe (EU)
C08,4 = Great Britain (GB)
C09,xxx?x: Engine
C10,4 = 4-Cylinder Engine
C11,5 = 5-Cylinder Engine
C12,6 = 6-Cylinder Engine
C13,xxxx?: Distance Impulse Number
C14,1 = 4358 (AHW/APE/AEH/AKL/AGZ/AGN with Manual Transmission)
C15,2 = 3538 (AGP/AGR/AHF with Manual Transmission and Midline Instrument Cluster)
C16,2 = 3538 (all Engines with Automatic Transmission)
C17,3 = 4146 (ALH/AGR/AHF with Manual Transmission and Lowline Instrument Cluster)
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
L02, 
L03,Prior to Key Learning or adapting a used replacement
L04,Instrument Cluster the Vehicle specific PIN/SKC (Login)
L05,of the replacement Instrument Cluster has to be used
L06,to enable the adaptation.
L07,You'll find the PIN/SKC on the Key Tag of the additional
L08,Key (of the Donor Car) or you can acquire it through your
L09,responsible Distribution Center or Importer.
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Maximum Distance to Next Oil Change (OIL),1000,km
RD,6,Maximum Distance to Inspection (IN1),1000,km
RD,7,Maximum Time to Inspection (IN2),10,DAYS
RD,10,ST_DNOC,1000,km
RD,11,ST_DTI,1000,km
RD,12,ST_TTI,10,DAYS
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Service Reset (Oil Service - Indivdual Channels),,
RJ,1,1,10,15
;
RJ,2,0,Service Reset (Inspection - Indivdual Channels),,
RJ,2,1,10,15
RJ,2,1,11,30
;
RJ,3,0,Service Reset (Oil Service & Inspection - Indivdual Channels),,
RJ,3,1,10,15
RJ,3,1,11,30
RJ,3,1,12,37
;
