;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A3 (8L) / Audi A4 (8D) / Audi A6 (4B) / Audi A8 (4D)
;
; Component: J347 - Interior Monitoring (#45) w/o Head Airbags
;
; P/N: 4B0-951-173-??? / 8L0-951-173-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8L-45.LBL
; 4B0-951-173.LBL
;
; includes measuring blocks, adaptation and coding
;
; created on 07/Jun/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 21/Feb/2013
;
; requires VCDS 11.11.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Input Signals,,?xxx = Switch for Int. Monitoring operated\nx?xx = Driver's Door Contact Switch open\nxx?x = Anti-Theft Warning System active\nxxx? = Glass Breakage recognized (Avant/Wagon only)
; ?xxx = Switch for Int. Monitoring operated
; x?xx = Driver's Door Contact Switch open
; xx?x = Anti-Theft Warning System active
; xxx? = Glass Breakage recognized (Avant/Wagon only)
001,2,Sensor,Sensitivity,Specification: 50...100 % (see Adaptation Channel 001)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Sensitivity
A001,5,Sensitivity
A001,6,Sensitivity of the Ultra-Sound Sensors can be lowered/raised.
A001,7, 
A001,8,Range: 50...100 %
A001,9,Standard: 100 (= 100 %)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Interior Monitoring (J247) Coding
C01,00?0x: Type
C02,0 = Audi A3 (8L) / Audi A6 (4B)
C03,1 = Audi A4 (8D) / Audi A8 (4D)
C04,00x0?: Chassis Type
C05,1 = Limousine/Sedan
C06,2 = Avant/Wagon
;
