;
; VAG-COM Label File
;
; Seat Ibiza (6L)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6L0-920-??3-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6L-17.LBL
; 6L0-920-xx0-17.LBL  (< MY 2006)
; 6L0-920-xx3-17.LBL  (MY 2007 >)
;
; created on 22/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
005,0,Service Reminder
005,1,Distance since,Service exceeded,Unit: 100 km
005,2,Time since,Service exceeded,Unit: 1 day(s)
005,3,Remaining dist.,until Service,Unit: 100 km
005,4,Remaining time,until Service,Unit: 1 day(s)
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time,to Service,See Adaptation Channel 049
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nRange: Engine 0/Engine 1
125,2,Transmission,,Range: Transm. 0/Transm. 1
125,3,Brake Electronics,(J104),Specification: ABS 1\nRange: ABS 0/ABS 1
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbags,(J234),Specification: Airbag 1\nRange: Airbag 0/Airbag 1
126,3,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nRange: Steer. ang. 0/Steer. ang. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,1,Central Electronics,(J519),Specification: E.Load.Crtl 1\nDisplay Range: E.Load.Crtl 1/E.Load.Crtl 0
;
201,1,Distance Impulse,Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??x0x: Options
C02,+01 = Brakepad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,xx?0x: Country
C06,0 = Germany / 1 = Europe
C07,4 = Great Britain (GB)
C08,6 = Saudi Arabia
C09,7 = Australia (AUS)
C10,xxxxx?: Distance Impulse Number (K-Value)
C11,1 = Engine Code BPX/BUK/BBU/BLZ/BJX/BKV
C12,2 = Engine Code ATD/AXR/BMT/BNV/BMS
C13,5 = Engine Code BBY/BKY/BBZ/BBX/BAH/ASZ/BLT/BNM/BTS/BXV/BXW
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Resolution: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
;
;A025,0,
;0
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km/mi
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,00150 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,or (if coded to miles)
A043,9,00093 = fixed Service Intervals (9.300 mi - w/o Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,100,DIST
RD,43,Max Mileage to Service,100,DIST
RD,44,Max Time to Service,1,Days
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
