;
; VCDS Label File
;
; Copyright © 2004-2012 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J197 - Level Control (#34)
;
; P/N: 4E0-910-553-???
;
; includes measuring blocks, coding, adaptation and security access
;
; created on 24/Sep/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated by "Frans"
; updated on 23/Feb/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 23/Feb/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,terminal 15
001,2,Voltage,terminal 30
001,3,Vehicle speed,[km/h]
001,4,Status,Term. 50,starting/starter active
;
002,1,Door,Status,Display range: door closed/door open/door locked
002,2,Rear lid,status,Display range: Rear lid open/rear lid closed
002,3,Voltage supply,right,Specified value: 0...10 V
002,4,Voltage supply,left,Specified value: 0...10 V
;
003,1,High level,selected,Display range: Pressed/not operated
003,2,[N/A]
003,3,Lower level,selected,Display range: Pressed/not operated
003,4,Compressor,Status,Display range: relay on/relay off
;
004,0,Deviation from standard level
004,1,Front,Left
004,2,Front,Right
004,3,Rear,Left
004,4,Rear,Right
;
005,0,Absolute vehicle height (mirror image of installation position)
005,1,Front,Left
005,2,Front,Right
005,3,Rear,Left
005,4,Rear,Right
;
006,1,Compressor,temperature
006,2,Pressure,sensor signal
006,3,Drain valve,Status
006,4,Pressure,accu. valve
;
007,0,Transverse lock-up (air spring valve status) 
007,1,Front,Left
007,2,Front,Right
007,3,Rear,Left
007,4,Rear,Right
;
008,1,Pitch,angle,in increments
008,2,Pitch angle,duty cycle,signal from headlight range control
008,3,Workshop,code
008,4,System,status
;
009,1,System,status
009,2,longitudinal,acceleration
009,3,deviation from,def. pos. front
009,4,deviation from,def. pos. rear
;
010,0,Vehicle level deviation (mm)
010,1,Front,Left
010,2,Front,Right
010,3,Rear,Left
010,4,Rear,Right
;
011,0,Damper valve current (mA)
011,1,Front,Left
011,2,Front,Right
011,3,Rear,Left
011,4,Rear,Right
;
012,0,Signal for body acceleration
012,1,front left,[V]
012,2,front right,[V]
012,3,rear,[V]
012,4,[N/A]
;
013,0,Damper velocity from height sensor (no-load level 2.5 Volts)
013,1,front left,[dm/s]
013,2,front right,[dm/s]
013,3,rear left,[dm/s]
013,4,rear right,[dm/s]
;
014,1,actuation,status button
014,2,Current damper,recognition,Display range: comfort=0/normal=1/sport1=2/sport2=3
014,3,CDC function LED,display status
014,4,[N/A]
;
015,1,Steering,angle
015,2,Vehicle,speed
015,3,Weighted,braking signal
015,4,CDC emergency,running,see labelfile
; 32 = CDC emergency running A
; 16 = CDC emergency running B
;  8 = CDC emergency running C
;  4 = CDC emergency running D
;  2 = CDC emergency running E
;  1 = no emergency running
;
016,1,Failsafe,temperature
016,2,Calculated,compressor,temperature
016,3,Measured,temperature value
016,4,Temperature,signal raw value
;
017,1,Standard,demand
017,2,Extreme,level
017,3,Bend
017,4,Vehicle skew
;
018,1,Heavy vehicle,distortion,Display range: 0 = not recognised / 1= recognised
018,2,[N/A]
018,3,[N/A]
018,4,Slight vehicle,distortion,Display range: 0 = not recognised / 1= recognised
;
019,1,[N/A]
019,2,Level,button,Display range: Not pressed/pressed
019,3,[N/A]
019,4,CDC button,,Display range: not pressed/pressed
;
020,1,Emergency,running A 
020,2,Emergency,running B
020,3,Emergency,running C
020,4,Emergency,running D
;
021,1,Emergency,running E
021,2,Emergency,running F
021,3,Emergency,running G
021,4,Emergency,running H
;
022,1,Pressure sensor,signal [V]
022,2,Pressure sensor,signal
022,3,Pressure sensor,signal [bar]
022,4,Accumulator,status,compressor actuation
;
023,1,Pressure in,accumulator
023,2,Pressure,level
023,3,Level,,Powertrain CAN-Databus
023,4,Gateway,,Fiber Optic MOST Data Bus
;
024,0,see lebelfile
;Digits 1-13 = part no., antenna FL
;Digits 13-15 = blank
;Digits 16-29 = part no., antenna FR
;
025,0,see labelfile
;Digits 1-13 = part no., antenna RL
;Digits 13-15 = blank
;Digits 16-29 = part no., antenna RR
;
026,0,see labelfile
;0.0 - 180 s (countdown for BE active; end at 0.0 seconds)
;
027,0,see labelfile
;Digits 1-8	= reception FL
;Digits 9-16	= reception FR
;Digits 17-24	= reception RL
;Digits 25-32	= reception RR
;Digits 33-40	= reception r
;
028,0,see labelfile
;Digits 1-8     = non-reception FL
;Digits 9-16     = non-reception FR
;Digits 17-24     = non-reception RL
;Digits 25-32     = non-reception RR
;Digits 33-40     = non-reception RR
;
031,1,Warning,lamp
031,2,LED for manual,operation
031,3,LED for,up-adjust
031,4,LED for,lowering
;
036,0,Air spring pressure
036,1,Front,Left [bar]
036,2,Front,Right [bar]
036,3,Rear,Left [bar]
036,4,Rear,Right [bar]
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
125,0,CAN-Databus communication (Powertrain)
125,1,brake,control module
125,2,engine,control module
125,3,steering angle,sensor
125,4,electrical,ignition lock
;
126,0,CAN-Databus communication (Powertrain)
126,1,CAN-Gateway
126,2,CAN-Gateway,(diagnosis)
126,3,[N/A]
126,4,[N/A]
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Level Control System (J197) Coding
C01,00?xxxx: Headlight Leveling
C02,1 = Internal = Level Sensor Information via Level Control System (J197)
C03,2 = External = Level Sensor Information partially via Headlight Leveling
C04,00x?xxx: Front Axle Height (Standard ~416 mm from Wheel Center to Fender)
C05,0 = -25 mm / 1 = -20 mm / 2 = -15 mm / 3 = -10 mm / 4 = -5 mm
C06,5 = 0 mm (No Change) / 6 = +5 mm / 7 = +10 mm / 8 = +15 mm / 9 = +20 mm
C07,00xx?xx: Rear Axle Height (Standard 398 mm from Wheel Center to Fender)
C08,0 = -25 mm / 1 = -20 mm / 2 = -15 mm / 3 = -10 mm / 4 = -5 mm
C09,5 = 0 mm (No Change) / 6 = +5 mm / 7 = +10 mm / 8 = +15 mm / 9 = +20 mm
C10,00xxx?x: Trailer Hitch
C11,0 = Standard (ONLY 4E0-910-533-C & 4E0-910-533-D)
C12,1 = Trailer Hitch NOT installed (without Trailer Control Module)
C13,2 = Trailer Hitch installed (with Trailer Control Module)
C14,00xxxx?: Country
C15,0 = Rest of World (RoW/Standard)
C16,1 = North American Region (NAR)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
; Login with security access code (function 16) first when calibrating suspension - the security code code is 31564
;
; NOTE: Transport mode activation code: 10273 Transport mode deactivation code: 41172
;
; See detailed instructions posted on the Ross-Tech website for suspension calibration
;
;
A01,0,Starting point for suspension calibration, and data entry for front left wheel
A01,1,Status,WAIT or VALUE
A01,2,Wheel position,or VALID message
A01,3,ENTER means,enter new measurement
A01,5,How to calibrate the level control system for each wheel
A01,6,Measure the distance from exact wheel center to the lower edge of the fender
A01,7,then enter the measurement (in millimeters) and press TEST. If the measurement
A01,8,is accepted, the words VALUE VALID will appear in the boxes above. Once you see
A01,9,VALUE VALID move up to the next adaptation channel and repeat the process for 
A01,10,the next wheel.  You CANNOT move backwards - the process must be completed
A01,11,in the exact sequence of channel 01 - 02 - 03 - 04 then confirmed in channel 05.
A01,12,  
A01,13,If you screw up or quit out of this process without confirming your work in channel 05
A01,14,you must enter the security code 31564 again and start again from channel 01.
A01,15,  
A01,16,Your work will not be saved until you confirm it in channel 05 by entering and saving a value of 1.
A01,17,You cannot calibrate just one wheel - you have to do all 4 wheels. Once your actual measurements are
A01,18,within 5mm of the stored values - you can consider the process to be finished.
;
A02,0,Data entry for front right wheel
A02,1,Status,WAIT or VALUE
A02,2,Wheel position,or VALID message
A02,3,ENTER means,enter new measurement
;
A03,0,Data entry for rear left wheel
A03,1,Status,WAIT or VALUE
A03,2,Wheel position,or VALID message
A03,3,ENTER means,enter new measurement
;
A04,0,Data entry for rear right wheel
A04,1,Status,WAIT or VALUE
A04,2,Wheel position,or VALID message
A04,3,ENTER means,enter new measurement
;
A05,0,This is where you confirm you want to save your measurements by entering a new value of 1.
A05,5,Confirmation of the work you did in the previous 4 channels
A05,6,In order for the car to save the entries you just made you must enter and save
A05,7,a value of 1 (one) in the NEW VALUE box. If you do not do this, all the measurements
A05,8,that you entered in the previous 4 channels will be discarded and the car will
A05,9,revert to whatever measurements were previously stored, with no changes made.
;
A10,0,Here you can turn the level control system on or off.
A10,5,Enter the appropriate number to turn the level control system on or off
A10,6,There are two possible choices - enabled or disabled. Be aware that simply clicking
A10,7,up or down on the arrow beside the NEW VALUE or entering a number in the NEW VALUE
A10,8,box will cause the instriction to be executed without any need to press the SAVE button.
A10,9,The fact that you have entered a security code to get here puts you in 'live fire' mode - so
A10,10,don't mess with the number in NEW VALUE unless you are prepared to recalibrate the level control
A10,11,system (via channels 01 to 05 inclusive) all over again.
;
;
;
;---------------------------------------------------
;
; Security Access Code Information
;
;---------------------------------------------------
;
S00,Security Access Codes for Audi Suspension System
S01,To begin Adaptation (calibration) Process - 31564
S02,To activate Transport Mode (for car carrier shipping) - 10273
S03,To deactivate Transport Mode (for normal operations) - 41172
;