;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; VW Touran (1T)
;
; Component: J234 - Airbag (#15) - VW62/VW7/VW71
;
; P/N: 1T0-909-605-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6Q-15.LBL
; 1T0-909-605.LBL      (VW71)
; 6Q0-909-605-VW5.LBL  (VW5/VW51/VW6/VW61)
; 6Q0-909-605-VW52.LBL (VW52)
;
; includes measuring blocks, adaptation, security access and misc
;
; created on 10/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 02/Feb/2012
;
; requires VCDS 11.2.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1, , , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Display Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
006,0,Seat Occupation (Rear)
006,1,Seat Occupation,Rear Driver Side,Display Range: Not Installed
006,2,Seat Occupation,Rear Pass. Side,Display Range: Not Installed
;
007,0,Igniters IV (Head Airbags)
007,1,Head-Level Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Head-Level Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
008,0,Crash Sensor I (Version)
008,1,Driver Side,Front
008,2,Passenger Side,Front
008,3,Driver Side,Rear
008,4,Passenger Side,Rear
;
009,0,Crash Sensor I (Identification)
009,1,Driver Side,Front
009,2,Passenger Side,Front
009,3,Driver Side,Rear
009,4,Passenger Side,Rear
;
010,0,Key Switch
010,1,Passenger,Airbag Status,Display Range: ON/OFF
010,2,Key Switch,Logic Contact 1,Display Range: too small/to Ground/to B+/on/off/not installed
010,3,Key Switch,Logic Contact 2,Display Range: too small/to Ground/to B+/on/off/not installed
;
011,0,Igniters IV (Head Airbags)
011,1,Head-Level Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Head-Level Airbag,Rear Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Pyrotechnic Igniter,Battery Separating,Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
012,0,Ingniters VI (Roll-Over Bars)
012,1,Roll-Over Bar,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
012,2,Roll-Over Bar,Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
012,3,Roll-Over Bar,Trigger Counter
012,4,Work Shop Code,Counter Reset
;
013,0,Ingniters VII (Front Airbags Stage 2)
013,1,Airbag (Stage 2),Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
013,2,Airbag (Stage 2),Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
014,0,Crash Sensors II (Version)
014,1,Driver Front,Airbag Sensor
014,2,Passengers Front,Airbag Sensor
;
015,0,Crash Sensors II (Identification)
015,1,Driver Front,Airbag Sensor
015,2,Passengers Front,Airbag Sensor
;
016,0,Seat Occupied Recognition Control Module (J706) I
016,1,Serial Number,(1/2)
016,2,Serial Number,(3/4)
016,3,Serial Number,(5)
016,4,Calibration Status
;
018,0,Seat Occupied Recognition Control Module (J706) II
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration,Sensor
;
019,0,Seat Occupied Recognition Control Module (J706) III
019,1,Workshop Code,(Last Coding)
019,2,Workshop Code,(Last 0-Balance)
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Brake Electronics,(J104),Specification: ABS 1\Range: ABS 1/ABS 0
;
225,0,CAN-Databus Powertrain (TimeOut)
225,1,Instrument Cluster
225,2,Brake Electronics,(J104)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
S01,11063 = Seat Occupied Recognition Basic Setting/Zero Balancing
S02,13731 = Seat Occupied Recognition Adaptation/Reset
S03,31415 = Extended Output Test Enabling
S04,53069 = Roll-Over Bars Trigger Counter Reset/Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 = Airbag Disabled
A001,7,1 = Airbag Enabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,5,Front Driver Airbag Deactivation
A002,6,0 = Airbag Disabled
A002,7,1 = Airbag Enabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 = Airbag Disabled
A003,7,1 = Airbag Enabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 = Airbag Disabled
A004,7,1 = Airbag Enabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
A005,0,Front Passenger Belt Tensioner Deactivation
A005,1,Front Passenger,Belt Tensioner
A005,2,Current Status
A005,5,Front Passenger Belt Tensioner Deactivation
A005,6,0 = Belt Tensioner Disabled
A005,7,1 = Belt Tensioner Enabled
A005,8, 
A005,9,Note: Refer to Service Manual!
;
A006,0,Front Driver Belt Tensioner Deactivation
A006,1,Front Driver,Belt Tensioner
A006,2,Current Status
A006,5,Front Driver Belt Tensioner Deactivation
A006,6,0 = Belt Tensioner Disabled
A006,7,1 = Belt Tensioner Enabled
A006,8, 
A006,9,Note: Refer to Service Manual!
;
A017,0,Roll-Over Bars Deactivation
A017,1,Roll-Over Bars
A017,2,Current Status
A017,5,Roll-Over Bars Deactivation
A017,6,0 = Roll-Over Bars Disabled
A017,7,1 = Roll-Over Bars Enabled
A017,8, 
A017,9,Note: Refer to Service Manual!
;
A018,0,Roll-Over Bars Trigger Counter Reset
A018,5,Roll-Over Bars Trigger Counter Reset
A018,6,To reset the trigger counter save "0" as new value.
A018,7, 
A018,8,Note: Refer to Service Manual!
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
I,
;
