;
; VCDS Label File
;
; Copyright © 2007-2011 Ross-Tech, LLC
;
; Audi A3 (8P) / Audi R8 (42) / Audi TT (8J)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 8P0-919-283-???
;
; includes measuring blocks, coding and adaptation
;
; created on 11/Jun/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 28/Apr/2011
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Distance (Rear)
001,1,Rear Left,Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
001,2,Rear Left,Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Rear Right,Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
001,4,Rear Right,Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
;
002,0,Distance (Front)
002,1,Front Left (G255),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
002,2,Front Left (G254),Center Sensor,Specification: 10...120 cm (255 cm = no obstacle recognized)
002,3,Front Right (G253),Center Sensor,Specification: 10...120 cm (255 cm = no obstacle recognized)
002,4,Front Right (G252),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
;
003,0,Resulting Distance / Vehicle Speed && Voltage
003,1,Resulting,Distance Front,Specification: 10...120 cm (255 cm = no obstacle recognized)
003,2,Resulting,Distance Rear,Specification: 10...160 cm (255 cm = no obstacle recognized)
003,3,Vehicle Speed,,Display Range: 0.0...255.0 km/h
003,4,Sensor,Voltage Supply,Specification: 10.0...14.5 V
;
004,0,External Information
004,1,Reverese Gear,engaged,Display Range: Reverse: Yes/Reverse: No
004,2,Trailer hitched,,Display Range: YES/NO/Not Installed
004,3,Sound Output,Suppressed (Park),Display Range: OFF/ON
004,4,Parking Aid,Button (E266),Display Range: ON/OFF/Not Oper./Not Installed
;
005,0,Volume && Frequency
005,1,Rear Buzzer,Volume,Display Range: 1...9
005,2,Rear Buzzer,Frequency,Display Range: 1...9
005,3,Front Buzzer,Volume,Display Range: 1...9
005,4,Front Buzzer,Frequency,Display Range: 1...9
;
006,0,Oscillation Time (Rear)
006,1,Rear Left,Sensor,Specification: 0.8...1.5 ms
006,2,Rear Left,Center Sensor,Specification: 0.8...1.5 ms
006,3,Rear Right,Center Sensor,Specification: 0.8...1.5 ms
006,4,Rear Right,Sensor,Specification: 0.8...1.5 ms
;
007,0,Oscillation Time (Front)
007,1,Front Left,Sensor,Specification: 0.8...1.5 ms
007,2,Front Left,Center Sensor,Specification: 0.8...1.5 ms
007,3,Front Right,Center Sensor,Specification: 0.8...1.5 ms
007,4,Front Right,Sensor,Specification: 0.8...1.5 ms
;
008,0,Confirmation Sound
008,1,Confirm. Sound,(Reverse Gear),Display Range: ON/OFF
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,00?xxxx: Trailer Hitch
C02,0 = Trailer Hitch not installed
C03,1 = Trailer Hitch installed
C04,00x?xxx: Transmission
C05,0 = Manual Transmission
C06,1 = Automatic Transmission
C07,00xx?xx: Specification
C08,0 = Rest of World (RoW)
C09,1 = Rest of World (RoW) S/RS
C10,2 = North America (NAR)
C11,3 = North America (NAR) S/RS
C12,00xxx?x: Chassis
C13,0 = Sedan
C14,1 = Avant (Wagon)
C15,2 = Cabriolet
C16,3 = Coupé
C17,5 = Sports Car (R8 only)
C18,00xxxx?: Model
C19,1 = Audi TT (8J) / Audi R8 (42)
C20,3 = Audi A3 (8P)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Rear Buzzer Volume
A001,5,Rear Buzzer Volume
A001,6,Adaptation of the rear warning buzzer volume.
A001,7, 
A001,8,Display Range: 1...9
;
A002,0,Rear Buzzer Frequency
A002,5,Rear Buzzer Frequency
A002,6,Adaptation of the rear warning buzzer frequency.
A002,7, 
A002,8,Display Range: 1...9
;
A005,0,Confirmation Sound
A005,5,Confirmation Sound
A005,6,Adaptation of confirmation sound when
A005,7,switching into reverse gear.
A005,8, 
A005,9,0 = without confirmation sound
A005,10,1 = with confirmation sound
;
A003,0,Front Buzzer Volume
A003,1,Current Value
A003,5,Front Buzzer Volume
A003,6,Adaptation of the front warning buzzer volume.
A003,7, 
A003,8,Display Range: 1...9
;
A004,0,Front Buzzer Frequency
A004,1,Current Value
A004,5,Front Buzzer Frequency
A004,6,Adaptation of the front warning buzzer frequency.
A004,7, 
A004,8,Display Range: 1...9
;
A005,0,Confirmation Sound
A005,2,Current Status
A005,5,Confirmation Sound
A005,6,Adaptation of confirmation sound when
A005,7,switching into reverse gear.
A005,8, 
A005,9,0 = with confirmation sound
A005,10,1 = without confirmation sound
;
A006,0,Reset Factory Default
A006,5,Reset Factory Default
A006,6,To reset all adaptation channels to their
A006,7,standard settings save "0" as new value.
;
