;
; VAG-COM Label File
;
; VW Golf/Jetta (1J)
;
; Component: Engine (#01) - AJQ/APP/ARY/AUQ
;
; P/N: 06A 906 032 ??
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 06-01.LBL
; 8L-01.LBL
; 8N-01.LBL
; 06A-906-032-AJQ.LBL (1.8l TE  @ 180 HP - AJQ/APP/ARY/AUQ)
;
; created on 24/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 05/Jan/2007
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed,,Specification (ilde): 700...820 RPM
001,2,Coolant,Temperature,Specifiation: 80.0...110.0 °C
001,3,Lambda,Controller,Specification: -10.0...+10.0 %
001,4,Basic Setting,Requirements,see labelfile
; 1xxxxxxx - Coolant temperature above 80 °C
; x1xxxxxx - Engine speed below 2000 RPM
; xx1xxxxx - Throttle valve closed
; xxx1xxxx - Lambda regulation correct
; xxxx1xxx - State of idle
; xxxxx1xx - A/C system compressor deactivated
; xxxxxxx1 - No malfunction detected by Self-Diagnosis
;
002,0,Basic Functions
002,1,Engine Speed,,Specification (ilde): 700...820 RPM
002,2,Engine Load,,Specification: 15...25 %
002,3,Injection,Timing,Specification: 2.0...4.0 ms
002,4,Intake Air Mass,,Specification: 2.0...4.5 g/s
;
003,0,Basic Functions
003,1,Engine Speed,,Specification (ilde): 700...820 RPM
003,2,Intake Air Mass,,Specification: 2.0...4.5 g/s
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.2...4.0 %
003,4,Ignition,Timing Angle,Specification: 6.0...12.0 °BDTC
;
004,0,Basic Functions
004,1,Engine Speed,,Specification (ilde): 700...820 RPM
004,2,Voltage Supply,,Specification: 12.0...15.0 V
004,3,Coolant,Temperature,Specifiation: 80.0...110.0 °C
004,4,Intake Air,Temperature,Specification: -48.0...+110.0 °C
;
005,0,Basic Functions
005,1,Engine Speed,,Specification (ilde): 700...820 RPM
005,2,Engine Load,,Specification: 15...25 %
005,3,Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed,,Specification (ilde): 700...820 RPM
006,2,Engine Load,,Specification: 15...25 %
006,3,Intake Air,Temperature,Specification: -48.0...+110.0 °C
006,4,Heights Correction,Factor
;
010,0,Ignition
010,1,Engine Speed,,Specification (ilde): 700...820 RPM
010,2,Engine Load,,Specification: 15...25 %
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.2...4.0 %
010,4,Ignition,Timing Angle,Specification: 5.0...15.0 °BDTC
;
020,0,Ignition Timing Angle  Retardation
020,1,Cylinder 1 Ignition,Angle Delay,Specification: 0.0...12.7 °
020,2,Cylinder 2 Ignition,Angle Delay,Specification: 0.0...12.7 °
020,3,Cylinder 3 Ignition,Angle Delay,Specification: 0.0...12.7 °
020,4,Cylinder 4 Ignition,Angle Delay,Specification: 0.0...12.7 °
;
022,0,Ignition Timing Angle  Retardation
022,1,Engine Speed,,Specification: 700...6800 RPM
022,2,Engine Load,,Specification: 16...175.0 %
022,3,Cylinder 1 Ignition,Angle Delay,Specification: 0.0...12.0 °
022,4,Cylinder 2 Ignition,Angle Delay,Specification: 0.0...12.8
;
023,0,Ignition Timing Angle  Retardation
023,1,Engine Speed,,Specification: 700...6800 RPM
023,2,Engine Load,,Specification: 16...175.0 %
023,3,Cylinder 3 Ignition,Angle Delay,Specification: 0.0...12.0 °
023,4,Cylinder 4 Ignition,Angle Delay,Specification: 0.0...12.8 °
;
026,0,Knock Sensor Voltage
026,1,Voltage Cyl. 1,Knock Sensor,Specification: 0.0...31.25 V
026,2,Voltage Cyl. 2,Knock Sensor,Specification: 0.0...31.25 V
026,3,Voltage Cyl. 3,Knock Sensor,Specification: 0.0...31.25 V
026,4,Voltage Cyl. 4,Knock Sensor,Specification: 0.0...31.25 V
;
028,1,Engine Speed,,Specification: 2200...6800 RPM
028,2,Engine Load,,Specification: 15.0...175.0 %
028,3,Coolant,Temperature,Specification: 40.0...110.0 °C
028,4,Result,Knock Sensor Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,see labelfile (Specification: 111)
; 1xx - Sensor heater
; x1x - Oxygen sensor ready
; xx1 - Lambda regulation active
;
031,1,Lambda Sensor,Current Value,Specification: 0.00...1.00 V
031,2,Lambda Sensor,Specified Value
;
032,1,Lambda (add.),Self-Adaptation,Specification: -10.0...+10.0 %
032,2,Lambda (mult.),Self-Adaptation,Specification: -10.0...+10.0 &
;
033,1,Bank 1,Lambda Control,Specification: -10.0...+10.0 %
033,2,Bank 1 Voltage,of Oxygen Sensors,Specification: 0.00...1.00 V
;
036,1,Bank 1 Sensor 2,Voltage,Specification: 0.00...1.00 V
036,2,Result,Lambda Availability,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK
;
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition
;
050,0,Speed Regulation
050,1,Engine Speed,,Specification (ilde): 700...820 RPM
050,2,Engine Speed,(Specified)
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
053,0,Speed Regulation
053,1,Engine Speed,,Specification (ilde): 700...820 RPM
053,2,Engine Speed,(Specified)
053,3,Voltage Supply,,Specification: 12.0...15.0 V
053,4,Current,Consumption,Display Range: 0...100 %
;
054,0,Speed Regulation
054,1,Engine Speed,,Specification (ilde): 700...820 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Display Range 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed,,Specification (ilde): 700...820 RPM
055,2,Idle Regulator,,Specification: -4.30...12.20 %
055,3,Idle Stabilization,Self-Adaptation,Specification (A/C-High): -6.0...+6.0 % | Specification (A/C-Low): -3.0...+3.0 %
055,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed,,Specification (ilde): 700...820 RPM
056,2,Engine Speed,(Specified)
056,3,Idle Regulator,,Specification: -4.30...12.20 %
056,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
060,0,Speed Regulation (EPC Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
060,3,Self-Adaptation,Steps Counter,Specification: 0...8
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
061,0,Speed Regulation (EPC System)
061,1,Engine Speed,,Specification: 700...6800 RPM
061,2,Voltage Supply,,Specification: 12.0...15.0 V
061,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
061,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
062,3,Throttle Position,Sensor (G79),Specification: 12...97 %
062,4,Accelerator Pedal,Position Sensor 2,G185 (Specification: 4...49 %)
;
066,1,Speed
066,2,Brake switch,clutch and CCS,see labelfile
; ----1xxx - Cruise control system active
; ----x1xx - Clutch depressed (always 1 in automatic transmission)
; ----xx1x - Brake depressed (brake pedal switch)
; ----xxx1 - Brake depressed (brake light switch)
066,3,Specified Speed
066,4,CCS Control,Positions,see labelfile
; ----1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; ----x1xx - SET button pressed
; ----xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; ----xxx1 - CCS slide handle on OFF
;
113,0,Charge Pressure Control
113,1,Engine Speed,,Specification: 700...6800 RPM
113,2,Engine Load,,Specification: 15.0...175.0 %
113,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
113,4,Athmospheric,Pressure,Specification: 500...1200 mbar
;
114,0,Charge Pressure Control
114,1,Engine Load,(specified),Specification: < 175.0 %
114,2,Engine Load,(spec. corrected),Specification: < 175.0 %
114,3,Engine Load,(actual Value),Specification: 15.0...175.0 %
114,4,Charge Pressure,Solenoid Valve,Display Range: 0.0...100.0 %
;
115,0,Charge Pressure Control
115,1,Engine Speed,,Specification: 700...6800 RPM
115,2,Engine Load,,Specification: 15.0...175.0 %
115,3,Charge Pressure,(specified Value),Specification: 990...2200 mbar
115,4,Charge Pressure,(actual Value),Specification: < 2000 mbar
;
117,0,Charge Pressure Control
117,1,Engine Speed,,Specification: 700...6800 RPM
117,2,Throttle Position,Sensor (G79),Display Range: 0...100 %
117,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
117,4,Charge Pressure,(specified Value),Specification: 990...2200 mbar
;
118,0,Charge Pressure Control
118,1,Engine Speed,,Specification: 700...6800 RPM
118,2,Intake Air,Temperature,Specification: -48.0...+110.0 °C
118,3,Charge Pressure,Solenoid Valve,Display Range: 0.0...100.0 %
118,4,Charge Pressure,(actual Value),Specification: < 2000 mbar
;
120,0,Traction Control System (ASR/TCS)
120,1,Engine Speed,,Specification: 700...6800 RPM
120,2,Engine Torque,specified by ASR,Specification: 0...399 Nm
120,3,Current,Engine Torque,Specification: 0...260 Nm
120,4,ASR Condition,,Display Range: ASR active/ASR not active
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
;
126,0,CAN-Databus Powertrain (Communication)
126,3,Airbag
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine (J220) Coding
C01,??xxx: Country/Emission
C02,05 = Emissions (EURO3)
C03,11 = Emissions (EURO4)
C04,xx?xx: Additional Functions
C05,0 = Front-Wheel-Drive (FWD) w/o ASR/ESP and Databus
C06,5 = Front-Wheel-Drive (FWD) with ASR/ESP and Databus
C07,6 = All-Wheel-Drive (AWD) w/o ASR/ESP and Databus
C08,7 = All-Wheel-Drive (AWD) with ASR/ESP and Databus
C09,xxx?x: Transmission
C10,0 = 5-Speed Manual Transmission
C11,1 = 6-Speed Manual Transmission
C12,3 = 4-Speed Automatic Transmission (01M)
C13,5 = 5-Speed Automatic Transmission
C14,7 = 6-Speed Automatic Transmission (09G)
C15,xxxx?: Vehicle Type
C16,0 = A Class (Seat Leon/Audi A3/Audi TT)
;
