;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; Porsche Cayenne (9P) / VW Touareg (7L) / VW Phaeton (3D)
;
; Component: J234 - Airbag (#15) 8.4+
;
; P/N: 3D0-909-601-???
;
; includes measuring blocks, basic settings, security access, adaptation and misc
;
; created on 30/Aug/2005 by Michael Moore (Moore@ross-tech.com)
; updated on 08/Feb/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 02/Feb/2012
;
; requires VCDS 11.2.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Belt Tensioner,Rear Center,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Pyrotechnic Igniter,Battery Separating,Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
006,0,Igniter Status (Side Airbag)
006,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
008,0,Igniter Status (Head Airbag)
008,1,Airbag (Stage 2),Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
008,2,Airbag (Stage 2),Passenger Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
008,3,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
008,4,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
009,0,Key Switch Status
009,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
009,2,Key Switch,(HW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
009,3,Key Switch,(SW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
;011,1,
;zu gross
;011,2,
;zu gross
;011,3,
;zu gross
;011,4,
;zu gross
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Brake Electronics,(J104),Specification: ABS 1\nRange: ABS 1/ABS 0
125,2,Instrument Cluster,(J285),Specification: Instruments 1\nRange: Instruments 1/Instruments 0
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Brake Electronics,(J104)
225,2,Instrument Cluster,(J285)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
S01,20324 = Seat Occupied Recognition Basic Setting/Zero Balancing
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
I,
;
