;
; VAG-COM label file
;
; Ford Galaxy (7M) / Seat Alhambra (7M) / VW Sharan (7M)
;
; component: Engine (#01) - AYL
;
; p/n: 022 906 032 ??
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 02-01.LBL
; 022-906-032-AYL.LBL (2.8l E   @ 204 HP - AYL)
;
; created on 20/Apr/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 20/Apr/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed,,Specification: 650...750 RPM
001,2,Coolant,Temperature,Specification: 80.0...110.0 °C
001,3,Lambda,Controller,Specification: -10.0...+10.0
001,4,Basic Setting,Requirements,Specification: 11111111
; xxxxxxx1 - Coolant temperature below 80 °C
; xxxxxx1x - Engine speed below 2000 RPM
; xxxxx1xx - Throttle valve closed
; xxxx1xxx - Lambda regulation correct
; xxx1xxxx - State of idle
; xx1xxxxx - A/C system compressor deactivated
; x1xxxxxx - Catalyst temperature over 350 °C
; 1xxxxxxx - No malfunctions detected
;
002,0,Basic Functions (Mass Air Flow)
002,1,Engine Speed,,Specification: 650...750 RPM
002,2,Engine Load,,Specification: 12.0...26.0 %
002,3,Injection,Timing,Specification: 1.0...4.0 ms
002,4,Intake Air Mass,,Specification: 2.5...5.0 g/s
;
003,0,Basic Functions (Mass Air Flow)
003,1,Engine Speed,,Specification: 650...750 RPM
003,2,Intake Air Mass,,Specification: 2.5...5.0 g/s
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.2....4.0 %
003,4,Ignition,Timing Angle,Specification: 6...15 °BTDC
;
004,0,Basic Functions
004,1,Engine Speed,,Specification: 650...750 RPM
004,2,Voltage Supply,,Specification: 12.0...15.0 V
004,3,Coolant,Temperature,Specification: 80...110 °C
004,4,Intake Air,Temperature,Specification: -48.0...+1430.0 °C
;
005,0,Basic Functions
005,1,Engine Speed,,Specification: 650...750 RPM
005,2,Engine Load,,Specification: 12.0...26.0 %
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed,,Specification: 650...750 RPM
006,2,Engine Load,,Specification: 12.0...26.0 %
006,3,Intake Air,Temperature,Specification: -48.0...+143.0 °C
006,4,Altitude,Correction Factor,Specification: -50.0...+10.0 %
;
010,0,Ignition
010,1,Engine Speed,,Specification: 650...750 RPM
010,2,Engine Load,,Specification: 12.0...26.0 %
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.2...4.0 %
010,4,Ignition,Timing Angle,Specification: 6..15 °BTDC
;
014,0,Ignition (Misfire Recognition)
014,1,Engine Speed,,Specification: 650...750 RPM
014,2,Engine Load,,Specification: 15.0...25.0 %
014,3,Misfire,(total),Specification: 0...6
014,4,Misfire,recognition,Specification: active | Display Range: active/inactive
;
015,0,Misfire Recognition
015,1,Cylinder 1,,Specification: 0...1
015,2,Cylinder 2,,Specification: 0...1
015,3,Cylinder 3,,Specification: 0...1
015,4,Malfunction,Recognition,Display Range: activated/blocked
;
016,0,Misfire Recognition
016,1,Cylinder 4,,Specification: 0...1
016,2,Cylinder 5,,Specification: 0...1
016,3,Cylinder 6,,Specification: 0...1
016,4,Malfunction,Recognition,Display Range: activated/blocked
;
022,0,Ignition (Knock Control - Cyl 1 && 2)
022,1,Engine Speed,,Specification: 630...6800 RPM
022,2,Engine Load,,Specification: 10.0...100.0 %
022,3,Cylinder 1 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
022,4,Cylinder 2 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
;
023,0,Ignition (Knock Control - Cyl 3 && 4)
023,1,Engine Speed,,Specification: 630...6800 RPM
023,2,Engine Load,,Specification: 10.0...100.0 %
023,3,Cylinder 3 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
023,4,Cylinder 4 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
;
024,0,Ignition (Knock Control)
024,1,Engine Speed,,Specification: 630...6800 RPM
024,2,Engine Load,,Specification: 10.0...100.0 %
024,3,Cylinder 5 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
024,4,Cylinder 6 Ignition,Angle Delay,Specification: 0.0...12.0 °CA
;
028,0,Knock Sensor Test (Short Trip)
028,1,Engine Speed,,Specification: 2200...6800 RPM
028,2,Engine Load,,Specification: 15.0...100.0 %
028,3,Engine Coolant,Temperature,Specification: 40.0...110.0 °C
028,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,Specification: 111
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
030,2,Bank 1,Sensor 2,Specification: 111
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
;
032,0,Lambda Regulation
032,1,Lambda (Idle),Self-Adaptation,Specification: -5.4...+5.4 %
032,2,Lambda (Partial),Self-Adaptation,Specification: -10.0...+10.0 %
;
033,0,Lambda Regulation (befor Catalyst)
033,1,Bank 1,Lambda Control,Specification: -10.0...+10.0 %
033,2,Bank 1 Voltage,of Oxygen Sensors,Specification: 1.40...1.60 V
;
034,0,Lambda Regulation (befor Catalyst - Basic Setting: Aging Check)
034,1,Engine Speed,,Specification: ~2300 RPM
034,2,Catalytic Converter,Temperature,Specification: min. 350 °C
034,3,Lambda Sensor,Dynamic Factor,Specification: 0.5...2.0
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK
;
036,0,Lambda Regulation (after Catalyst)
036,1,Bank 1 Sensor 2,Voltage,Specification: 0.10...0.90 V
036,2,Result,Lambda Availability,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK
;
041,0,Lambda Regulation (Lambda Probe Heating)
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition,,Specification: Htg.bC.ON
041,3,Resistance,Bank 1 Sensor 2,Specification: 0.0...25.0 kOhm
041,4,Heater Condition,,Specification: Htg.aC.ON
;
043,0,Oxygen Sensor Control (Basic Setting: Sensor After Catalyst - Aging Check)
043,1,Engine Speed,,Specification: ~2300 RPM
043,2,Catalyst,Temperature,Specification: min. 350 °C
043,3,Lambda Sensor,Voltage (B1-S1),Specification: 0.0...1.0 V
043,4,Result,Aging Check,Specification: B1-S2 OK | Display Range: Test OFF/Test ON/B1-S2 OK/B1-S2 nOK
;
050,0,Speed Regulation
050,1,Engine Speed,,Specification: 650...750 RPM
050,2,Engine Speed,(specified),Specification: 700 RPM
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
054,0,Speed Regulation
054,1,Engine Speed,,Specification: 650...2520 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Specification: 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed,,Specification: 650...750 RPM
055,2,Idle Regulator,,Specification: -5.0...+10.0 %
055,3,Idle Stabilization,Self-Adaptation,Specification: -5.0...+5.0 %
055,4,Operating Mode
; ---1x - Gear engaged
; ---x1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed,,Specification: 650...750 RPM
056,2,Engine Speed,(specified),Specification: 700 RPM
056,3,Idle Regulator,,Specification: -5.0...+10.0 %
056,4,Operating Mode
; ---1x - Gear engaged
; ---x1 - Air conditioner compressor switched on
;
060,0,Speed Regulation (Basic Setting: Throttle Body Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
060,3,Learn Step,Counter,Specification: 0...8
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
061,0,Speed Regulation (EPC)
061,1,Engine Speed,,Specification: 650...6500 RPM
061,2,Voltage Supply,,Specification: 12.0...15.0 V
061,3,Activation Throttle,Position Actuator,G186 (Specification: 0...100 %)
061,4,Operating,Condition
; ---1x - Gear engaged
; ---x1 - Air conditioner compressor switched on
;
062,0,Speed Regulation (Basic Setting: EPC Adaptation)
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...93 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
062,3,Throttle Position,Sensor (G79),Specification: 12...97 %
062,4,Accelerator Pedal,Position Sensor 2,G185 (Specification: 4...49 %)
;
063,0,Speed Regulation (Basic Setting: Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79),Display Range: 0...100 % | Specification: 70...97 %
063,2,Throttle Position,Sensor (learned),G79 (Specification: 80...100 %)
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP runs/ADP OK/ADP ERROR
;
066,1,Cruise Cntrol System
066,2,Brake switch,clutch and CCS,Specification: ----1000
; ----1xxx - Cruise control system active
; ----x1xx - Clutch depressed (always 1 in automatic transmission)
; ----xx1x - Brake depressed (brake pedal switch)
; ----xxx1 - Brake depressed (brake light switch)
066,3,Specified Speed
066,4,CCS Control,Positions,Specification: ----0011
; ----1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; ----x1xx - SET button pressed
; ----xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; ----xxx1 - CCS slide handle on OFF
;
090,0,Performance Increase (Exhaust Camshaft)
090,1,Engine Speed,,Specification: 650...6500 RPM
090,2,Operating Mode,Camshaft Adj.,Display Range: ON/OFF
090,3,Actual Camshaft,Adjustment Angle,Specification: 0.0...12.0 °CA
;
091,0,Performance Increase (Camshaft Adjustment)
091,1,Engine Speed,,Specification: 650...6500 RPM
091,2,Engine Load,,Specification: 10...100 %
091,3,Spec. Camshaft,Adjustment Angle,Specification: 0.0...52.0 °CA
091,4,Actual Camshaft,Adjustment Angle,Specification: 0.0...52.0 °CA
;
095,0,Performance Increase (Intake Manifold Change Over)
095,1,Engine Speed,,Specification: 650...6500 RPM
095,2,Engine Load,,Specification: 0...100 %
095,3,Coolant,Temperature,Specification: 80.0...110.0 °C
095,4,Switch-Over,Staus,Display Range: IMC-V ON/IMC-V OFF
;
099,0,Oxygen Sensor Control (Basic Setting: Oxygen Sensor Operating Condition)
099,1,Engine Speed,,Specification: 650...750 RPM
099,2,Coolant,Temperature,Specification: 80.0...110.0 °C
099,3,Lambda Sensor,Control,Specification: -10.0...+10.0 %
099,4,Lambda Sensor,Condition,Specification: Lambda ON/OFF
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
;
