;
; VCDS Label File
;
; Audi TT (8J)
;
; Component: J502 - Tire Pressure Monitoring (#65)
;
; P/N: 8J0-907-273-???
;
; includes measuring blocks and coding
;
; created on 29/Oct/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 15/Mar/2008
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Wheel 1 Wheel Status I
001,1,Wheel,Position,No Display = Not yet recognized
001,2,Wheel,Temperature
001,3,Wheel Pressure,(actual)
001,4,Wheel Pressure,(specified)
;
002,0,Wheel 1 Status II
002,1,Wheel,Position,No Display = Not yet recognized
002,2,Wheel,Acceleration,Range: 0.0...127.5
;
003,0,Wheel 1 Status III
003,1,Wheel Sensor,Position / Identification
;
004,0,Wheel 2 Status I
004,1,Wheel,Position,No Display = Not yet recognized
004,2,Wheel,Temperature
004,3,Wheel Pressure,(actual)
004,4,Wheel Pressure,(specified)
;
005,0,Wheel 2 Status II
005,1,Wheel,Position,No Display = Not yet recognized
005,2,Wheel,Acceleration,Range: 0.0...127.5
;
006,0,Wheel 2 Status III
006,1,Wheel Sensor,Position / Identification
;
007,0,Wheel 3 Status I
007,1,Wheel,Position,No Display = Not yet recognized
007,2,Wheel,Temperature
007,3,Wheel Pressure,(actual)
007,4,Wheel Pressure,(specified)
;
008,0,Wheel 3 Status II
008,1,Wheel,Position,No Display = Not yet recognized
008,2,Wheel,Acceleration,Range: 0.0...127.5
;
009,0,Wheel 3 Status III
009,1,Wheel Sensor,Position / Identification
;
010,0,Wheel 4 Status I
010,1,Wheel,Position,No Display = Not yet recognized
010,2,Wheel,Temperature
010,3,Wheel Pressure,(actual)
010,4,Wheel Pressure,(specified)
;
011,0,Wheel 4 Status II
011,1,Wheel,Position,No Display = Not yet recognized
011,2,Wheel,Acceleration,Range: 0.0...127.5
;
012,0,Wheel 4 Status III
012,1,Wheel Sensor,Position / Identification
;
016,0,Wheel Sensor Status (from last Received Wheel ID) I
016,1,Wheel Sensor,Identification
;
17,0,Status
17,1,System Status
; 000xxxxx xxxxxxx1 = System ready
; 000xxxxx xxxxxx1x = Automatic Learning active
; 000xxxxx xxxxx1xx = Automatic Learning successful
; 000xxxxx xxxx1xxx = Automatic Learning not successful
; 000xxxxx xxx1xxxx = Specified Pressure saving active
; 000xxxxx xx1xxxxx = Specified Pressure saved
; 000xxxxx x1xxxxxx = Specified Pressure not saved
; 000xxxxx 1xxxxxxx = Unspecified Warning
; 000xxxx1 xxxxxxxx = Wheel Electronics overheated
; 000xxx1x xxxxxxxx = Radio Interference
; 000xx1xx xxxxxxxx = Radio Receiver Diagnostics active
; 000x1xxx xxxxxxxx = Fault stored
; 0001xxxx xxxxxxxx = Button active
17,2,Vehicle Status
; 000000xx xxxxxxx1 = Terminal 15 ON
; 000000xx xxxxxx1x = Vehicle Speed > 25km/h
; 000000xx xxxxx1xx = CAN-Signal Ambient Temperature OK
; 000000xx xxxx1xxx = CAN-Signal Terminal 15 OK
; 000000xx xxx1xxxx = CAN-Signal Vehicle Speed OK
; 000000xx xx1xxxxx = CAN-Signal Date/Time OK
; 000000xx x1xxxxxx = Standing Information available
; 000000xx 1xxxxxxx = End of Line Mode active
; 000000x1 xxxxxxxx = End of Line Mode OK
; 0000001x xxxxxxxx = MIL active
;
021,0,Wheel Temperatures
021,1,Wheel 1,Temperature
021,2,Wheel 2,Temperature
021,3,Wheel 3,Temperature
021,4,Wheel 4,Temperature
;
022,0,Pressure Deviation (Actual vs. Specified)
022,1,Wheel 1,Pressure Deviation
022,2,Wheel 2,Pressure Deviation
022,3,Wheel 3,Pressure Deviation
022,4,Wheel 4,Pressure Deviation
;
124,0,CAN-Databus Communication
124,1,Voltage,(Terminal 30)
124,2,Vehicle Speed
124,3,Speed Signal,from ABS received,Range: ABS 1/ABS 0
124,4,Status,Terminal 15,Range: Term 15 On/Term 15 Off
;
125,0,CAN-Databus Communication
125,1,Ambient,Temperature
125,2,Temp. Signal,from A/C received,Range: A/C 1 / A/C 0
;
126,0,CAN-Databus Communication
126,1,TPMS Button,(E226),Range: Operated/Not Oper.
126,2,TPMS Warning,Lamp,Range: Lamp OFF/Lamp ON
;
127,0,CAN-Databus Communication
127,1,Date
127,2,Time
127,3,Standing Time
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Tire Pressure Monitoring (J502) Coding
C01,0?x00xx: Data Carrier
C02,8 = 1 Antenna + 4 Trigger @ 315 MHz (PR-7K8)
C03,0x?00xx: Type
C04,4 = USA
C05,0xx00?x: Specified Pressure I
C06,1 = 1.x bar (Standard)
C07,2 = 2.x bar
C08,3 = 3.x bar
C09,0xx00x?: Specified Pressure II
C10,0 = x.0 bar / 1 = x.1 bar
C11,2 = x.2 bar / 3 = x.3 bar
C12,4 = x.4 bar / 5 = x.5 bar
C13,6 = x.6 bar / 7 = x.7 bar
C14,8 = x.8 bar / 9 = x.9 bar (Standard)
;
