;
; VCDS Label File
;
; Copyright © 2007-2011 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia (1Z)
;
; Component: J412/R36 - Telephone Preperation (#77)
;
; P/N: 1Z0-862-335-??? / 5P0-862-335-???
;
; includes measuring blocks, adaptation, coding and selective output test
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1Z-77.LBL
; 5P0-862-335.LBL
;
; created on 31/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 01/Sep/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltage
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
;
005,0,Input Signals
005,1,Input Signals,,1xxx = Communication to Mobile Phone active\nx1xx = Mobile Phone Switched ON\nxx1x = Mobile Phone inserted\nxxx1 = Push-To-Talk (PTT) Button pressed
;
010,0,Signal Strengths
010,1,Signal Strengths
010,2,Reception,Signal Strengths,Display Range: -113.0...33.0 dBm\n128.0 dBM = No Communication with Mobile Phone
;
011,0,Main Antenna
011,1,Main Antenna
011,2,Main Antenna,Status,Display Range: OK/Short Circuit/Open Circuit/Not Possible
;
014,0,Bluetooth Devices
014,1,Bluetooth Devices
014,2,Connected,Bluetooth Devices
;
019,0,Microphone Input
019,1,Microphone Input,Voltage
019,2,Microphone Input,Status
;
020,0,Connected Bluetooth Devices && Reception Signal Strength
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
082,0,Advanced Control Module Identification III
;
133,0,Bluetooth Antenna
133,1,Bluetooth Antenna
133,2,Bluetooth Antenna,Status
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A128,0,Output Volume
A128,5,Output Volume
A128,6,Basic Output Volume Adjustment
A128,7,Range: -6...+6 dB
A128,8, 
A128,9,0 = ±0 dB / 1 = +1 dB / 2 = +2 dB
A128,10,3 = +3 dB / 4 = +4 dB / 5 = +5 dB / 6 = +6 dB
A128,11,128 = -1 dB / 129 = -2 dB / 130 = -3 dB
A128,12,131 = -4 dB / 132 = -5 dB / 133 = -6 dB
;
A129,0,Afterrun Time
A129,5,Afterrun Time
A129,6,The time the mobile phone plate is active after "Ignition OFF".
A129,7, 
A129,8,Range: 0...6 (30 Seconds to 30 Minutes)
A129,9,Increments: 1 = 5 Minutes (0 = 30 Seconds)
;
A130,0,Delay Time
A130,5,Delay Time
A130,6,Adjustment of the delay times to compensate the
A130,7,audio component delay and acoustic running times.
A130,8, 
A130,9,Range: 0...12 ms
;
A131,0,Microphone Sensitivity
A131,5,Microphone Sensitivity
A131,6,Microphone Sensitivity Adjustment
A131,7,Range: -6...+6 dB
A131,8, 
A131,9,0 = ±0 dB / 1 = +1 dB / 2 = +2 dB
A131,10,3 = +3 dB / 4 = +4 dB / 5 = +5 dB / 6 = +6 dB
A131,11,128 = -1 dB / 129 = -2 dB / 130 = -3 dB
A131,12,131 = -4 dB / 132 = -5 dB / 133 = -6 dB
;
A132,0,Speed Dependent Volume Adjustment (GALA)
;
A133,0,Bluetooth
A133,5,Bluetooth
A133,6,0 = Bluetooth OFF
A133,7,1 = Bluetooth ON
;
A134,0,Hands Free Function
A134,5,Hands Free Function
A134,6,0 = Hands-free active while Bluetooth connection is active but without cell phone engaged
A134,7,1 = Hands-free only active with cell phone engaged
;
A135,0,Bluetooth Pass Key
A135,5,Bluetooth Pass Key
A135,6,Set the 4-digit Bluetooth pass key using this channel.
;
A136,0,Delay Time (Voice Control)
A136,5,Delay Time (Voice Control)
A136,6,Adjustment of the delay time between mute signal
A136,7,and start of the voice control recognition.
A136,8, 
A136,9,Standard: 5 (= 0.5 Seconds)
;
A137,0,Bluetooth Visibility Time
A137,5,Bluetooth Visibility Time
A137,6,Time for which the Bluetooth Telephone Preparation
A137,7,stays visible for other Bluetooth Devices. After
A137,8,this time only previously connected Devices can
A137,9,connect to the Bluetooth Telephone Preparation.
A137,10, 
A137,11,Range: 0/1...30 Minutes
A137,12,Standard: 0 (always visible)
;
A138,0,Voice Control Volume
A138,5,Voice Control Volume
A138,6,This Channel allows to alter
A138,7,the Maximum Voice Control Volume.
;
A139,0,Call Volume
A139,5,Call Volume
A139,6,This Channel allows to alter
A139,7,the Maximum Call Volume.
;
A141,0,Bluetooth Confirmation Tone
A141,5,Bluetooth Confirmation Tone
A141,6,The Bluetooth Confirmation Tone can be activated/deactivated.
A141,7, 
A141,8,0 = Confirmation Tone inactive
A141,9,1 = Confirmation Tone active
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Telephone Preperation (R36) Coding
C01,00?0xxx: Communication Type
C02,0 = Display-Data-Protocol (DDP)
C03,1 = Operating and Display Protocol (BAP)
C01,00x0?xx: Installation List
C02,3 = Radio or Radio/Navigation System
C03,4 = Multi-Function Steering Wheel and Radio or Radio/Navigation System
C04,00x0x?x: Language (Voice Control)
C05,0 = Voice Control OFF OR via external Device (e.g. Radio/Navigation System)
C06,1 = German / 2 = English (UK) / 3 = French
C07,4 = Italian / 5 = Spanish / 6 = Czech
C08,7 = English (US)
C09,9 = Speaker dependent (Voice Commands inactive & Acoustic Name Selection active) 
C10,00x0xx?: Language (Display)
C11,0 = No Display / 1 = German / 2 = English (UK) / 3 = French
C12,4 = Italian / 5 = Spanish / 7 = English (US)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T851,Speaker
T1530,Radio Mute
T2502,Signal Telephone ON
T2612,Audio Wire (only with Test Adapter)
T2619,Communication Wire (only with Test Adapter)
;
