;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; VW Passat (3B)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 3B?-920-??7-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3B-17.LBL
; 3Bx-920-xx5.LBL
;
; created on 25/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 24/May/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Speed / Engine speed / Oil pressure / Time
001,1,Speed
001,2,Engine Speed
001,3,Oil pressure, 0.9 bar
001,4,Time
;
002,0,Distance / Fuel / Ambient temperature
002,1,Mileage
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature,MFD only
;
003,0,Coolant and Oil
003,1,Coolant,Temperature
003,2,Oil Level,,Display Range: Ok/n.Ok
003,3,Oil,Temperature
;
022,0,Immobilizer
022,1,Starting,permitted
022,2,Engine (ECM),responds
022,3,Key condition,OK
022,4,Number of,keys coded
;
023,0,Immobilizer
023,1,Variable code,authorized
023,2,Key status,(transponder)
023,3,Fixed code,authorized
023,4,Immobilizer,status,see labelfile
; 4 - new customer service - delivery condition (replacement part instrument cluster)
; 5 - customer service locked - adaptation data programmed in customer service
; 6 - immobilizer adapted - normal function condition
; 7 - key adaptation active - key adaptation via tester
;
024,0,Immobilizer - locking periods
024,1,Instrument,cluster
024,2,Engine control, module (ECM)
024,3,Emergency,release
024,4,Transponder,recognition
;
025,0,Immobilizer Communication
025,1,Immobilizer,Communication,1 = via CAN-Databus / 2 = via W-Line
;
050,0,Main Information
050,1,Mileage
050,2,Engine Speed
050,3,Oil,Temperature
050,4,Coolant,Temperature
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Steering,sensor
126,2,Airbag
;
130,0,CAN-Databus Communication (Comfort)
130,1,CAN-Databus,Status
130,2,Comfort System
130,3,Door electronics,driver
130,4,Door electronics,passenger
;
131,0,CAN-Databus Communication (Comfort)
131,1,Door electronics,rear left
131,2,Door electronics,rear right
;
132,0,CAN-Databus Communication (Comfort)
;
140,0,CAN-Databus Communication (Infotainment)
140,1,CAN-Databus,Status
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A2,0,Service reminder
A2,5,Service reminder reset
A2,6,displayed values:
A2,7,0 - no service
A2,8,1 - service
A2,9, 
A2,10,reset:
A2,11,0 - Service reminder reset
;
A4,0,Language for error messages and navigation (MFD only)
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Czech
;
A9,0,Dinstance (in 10km)
A9,1,Distance
A9,2,in 10
A9,3,km
A9,5,Distance changing
A9,6,Before the cluster accepts the new
A9,7,distance you have to login using 13861.
A9,8, 
A9,9,The distance can only be changed until
A9,10,the current value is not over 100km.
;
A21,0,Key count (Immobilizer)
A21,1,Old Key
A21,2,count
A21,3,[count]
;
A30,0,Fuel gauge adaption
A30,1,Current,value
A30,5,Fuel gauge adaption
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A35,0,Engine speed threshold
A35,5,Engine speed threshold adaption
A35,6,Basic value: 0
A35,7,Range: 0 - 1000
A35,8,Unit: 250 U/min
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 1000 km/mi
A042,7,00015 = Standard (15.000 km)
A042,8,or (if coded to miles)
A042,9,00009 = Standard (9.000 mi)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 1000 km/mi
A043,7,00015 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,00030 = Gasoline Engines with flexible Service Intervals (30.000 km - with Longlife)
A043,9,00050 = Diesel Engines with flexible Service Intervals (50.000 km - with Longlife)
A043,10,or (if coded to miles)
A043,11,00009 = fixed Service Intervals (9.000 mi - Great Britain - w/o Longlife)
A043,12,00019 = Gasoline Engines with flexible Service Intervals (19.000 mi - with Longlife)
A043,13,00031 = Diesel Engines with flexible Service Intervals (31.000 mi - with Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = Gasoline Engines with flexible Service Intervals (with Longlife)
A045,8,4 = Diesel Engines with flexible Service Intervals (with Longlife)
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
;
A050,0,Immobilizer (Vehicle Data learning)
A050,1,Status
A050,5,Immobilizer (Vehicle Data learning)
A050,6,Please enter the Immobilizer PIN/SKC of the Engine Control Module (OLD PIN/SKC).
A050,7,After that the Learning Process is being initiated the new Immobilizer Control
A050,8,Module adopts the Vehicle-Identification-Number (VIN) and Immobilizer
A050,9,Identification (IMMO-ID) of the Vehicle (from the OLD Engine Control Module).
A050,10,Once the Adaptation is done switch the Ignition OFF for about 2 Minutes.
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = Brake Pad Wear Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Level Warning active
C05,+16 = Secondary Display (Radio/Navigation) active
C06,xx?xx: Country
C07,0 = Germany | 1 = Europe | 2 = USA
C08,3 = Canada/Mexico/Latin America | 4 = England
C09,5 = Japan | 6 = Saudi Arabia | 7 = Australia
C10,xxx?x: Service Intervals
C11,0 = Fixed Service Interval w/o Oil Level & Temperature Sensor (PR-QG0)
C12,1 = Flexible Service Interval with Oil Level & Temperature Sensor (PR-QG1)
C13,2 = Fixed Service Interval with Oil Level & Temperature Sensor (PR-QG2)
C14,3 = Service Interval Reminder inactive (USA/Canada)
C15,xxxx?: Distance Impulse Number (K-Value)
C16,1 = Speed Signal via CAN (23400)
C17,3 = 6-Cylinder Light Armored Vehicle (4134)
C18,5 = All other Engine Variants (4182)
C19,6 = 8-Cylinder (W8 - 4128)
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,1000,DIST
RD,43,ST_MADTS,1000,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Change to flexible Intervals (Great Britain/Gasoline)
RJ,1,1,42,9
RJ,1,2,43,19
RJ,1,3,44,730
RJ,1,4,45,2
;
RJ,2,0,Change to flexible Intervals (Great Britain/Diesel)
RJ,2,1,42,9
RJ,2,2,43,31
RJ,2,3,44,730
RJ,2,4,45,4
;
RJ,3,0,Change to fixed Intervals (Great Britain)
RJ,3,1,42,9
RJ,3,2,43,9
RJ,3,3,44,365
RJ,3,4,45,1
;
RJ,4,0,Change to flexible Intervals (Rest of World/Gasoline)
RJ,4,1,42,15
RJ,4,2,43,30
RJ,4,3,44,730
RJ,4,4,45,2
;
RJ,5,0,Change to flexible Intervals (Rest of World/Diesel)
RJ,5,1,42,15
RJ,5,2,43,50
RJ,5,3,44,730
RJ,5,4,45,4
;
RJ,6,0,Change to fixed Intervals (Rest of World)
RJ,6,1,42,15
RJ,6,2,43,15
RJ,6,3,44,365
RJ,6,4,45,1
;
