;
; VCDS Label File
;
; Copyright © 2011 Ross-Tech, LLC
;
; Audi V8 (4C) / Audi 100 (4A)
;
; Component: J220 - Engine (#01) - ABH
;
; P/N: 441-907-557-??? / 4A0-907-557-???
;
; includes measuring blocks, basic setting and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 44-01.LBL
; 4A-01.LBL
; 077-907-557-ABH.LBL  (4.2l SR     @ 280 HP - ABH)
;
; created on 15/Mar/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 15/Mar/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
000,0,Decimal Measuring Values
000,1,Coolant Temperature,Specification: 189...210 (85.0...100.0 °C)
000,2,Engine Load,Specification: 32...46
000,3,Engine Speed,Specification: 49...75 (690...750 RPM)
000,4,Idle Speed Stabilization (Operating Range),Specification: 123...140
000,5,Idle Speed Stabilization (Characteristic Curve Zero Point),Specification: 80...128
000,6,Idle Speed Stabilization (Load Adaptation),Specification: 120...138
000,7,Idle Speed Stabilization (Characteristic Curve Control),Specification: 42...53
000,8,Lambda Control,Specification: 121...135
000,9,Lambda Adaptation,Specification: 78...178
000,10,Ignition Timing,Specification: 42...47 (3.8...10.4 °BDTC)
;
B000,0,Active Charcoal Valve closing
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine Control Unit (J220) Coding
C01,Coding is being done via Coding Bridges in the Wiring.
C02,Please refer to the Factory Repair Manual for Details.
;
