;
; VCDS Label File
;
; Copyright © 2009+ Ross-Tech, LLC
;
; VW Eos (1F) / VW Golf/Jetta (1K) / VW Passat (35/3C) / VW Touareg (7L) / VW Touran (1T)
;
; Component: J650 - Multimedia System (#2E)
;
; P/N: 5N0-035-342-??? / 6J0-035-342-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6J-2E.LBL
; 5N0-035-342.LBL
;
; includes measuring blocks, long coding, adaptation, and selective output test
;
; created on 01/Nov/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 02/Jan/2013
;
; requires VCDS 805.0 / LCode 910.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,Terminal 30,Range: 0.0...20.0 V\nSpecification: 9.0...15.0 V
001,2,Status,S-Contact,Range: ON/OFF
001,3,Status,Terminal 15,Range: ON/OFF
;
002,0,Driver
002,1,Driver,(actual),,00000000 xxxxxxx1 = AUX-IN (3.5mm Connector-Driver active)\n00000000 xxxxxx1x = DAP UART (iPod-Driver active)\n00000000 xxxxx1xx = DAP USB-MSC (USB-Driver active)
;
003,0,Adapter Cable
003,1,Adapter Cable,(actual),00000000 xxxxxxx1 = Adapter Cable not connected\n00000000 xxxxxx1x = AUX-IN (3.5mm Adapter connected)\n00000000 xxxxx1xx = DAP UART (iPod-Adapter connected)\n00000000 xxxx1xxx = DAP USB-MC (USB-Adapter connected)
;
004,0,Codec
004,1,Codec,(actual),00000000 00xxxxx1 = No Codec active\n00000000 00xxxx1x = MP3\n00000000 00xxx1xx = MP3-Pro\n00000000 00xx1xxx = WMA\n00000000 00x1xxxx = OGG\n00000000 001xxxxx = AAC
;
005,0,Power Supply for external Devices
005,1,Power Supply,Status
005,2,Power Supply,Voltage,Range: 0.0..25.5 V\nStandard: ~5.0 V
;
006,0,Analoger Input (AUX-IN)
006,1,Analoger Input,(AUX-IN) recognized,Range: recognized/n. recognized
;
007,0,ucMedia Software Level
007,1,ucMedia,Software Level
;
008,0,External Connection
008,1,Ext. Connect.,recognized,Range: recognized/n. recognized
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,0~4,00,Control Module NOT coded
LC,00,0~4,01,Analoger Input (AUX-IN) istalled
LC,00,0~4,02,Analoger Input (AUX-IN) NOT installed
LC,00,0~4,03,Analoger Input (AUX-IN) AND Rear-Seat-Entertainment (RSE) installed
;
LC,01,0~4,00,Codepage: Standard (not changeable)
LC,01,0~4,01,Codepage: Latin
LC,01,0~4,02,Codepage: Chinese
LC,01,0~4,03,Codepage: Changeable (VW Phaeton (3D) only)
; Reversible only for VW Phaeton (3D) via ZAB
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T3376,Activation Left Audio Channel
T3377,Activation Right Audio Channel
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
;A016,0,
;1
;
;A017,0,
;1
;
