;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Audi A3 (8P) / Audi TT (8N) / Seat Altea (5P) / Seat Toledo (5P)
; Skoda Octavia (1Z) / VW Golf/Jetta (1K/5K/AJ) / VW New Beetle (1C) / VW Touran (1T)
;
; Component: J217 - Transmission Electronic (#02) - 6-Speed Automatic Transmission (09G)
;
; P/N: 09G-927-750-??? / 09G-997-750-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 09-02.LBL
; 09G-927-750.LBL
;
; includes measuring blocks, basic settings and coding
;
; created on 27/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 13/Dec/2010
;
; requires VCDS 10.5.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,1,Engine speed,,Specification: 0...7650 RPM
001,2,Transmission,RPM (from G182),Specification: 0...7650 RPM
001,3,Transmission,Output RPM,from G195 (Specification: 0...7650 RPM)
001,4,Driving Mode,,0 = Neutral\nR = Reverse Gear\nN = Neutral\n1H = 1st Gear Hydraulic\n1M = 1st Gear Mechanic\n2H = 2nd Gear Hydraulic\n2M = 2nd Gear Mechanic\n3H = 3rd Gear Hydraulic\n3M = 3rd Gear Mechanic\n4H = 4th Gear Hydraulic\n4M = 4th Gear Mechanic\n5H = 5th Gear Hydraulic\n5M = 5th Gear Mechanic\n6H = 6th Gear Hydraulic\n6M = 6th Gear Mechanic
;
B001,0,Kick-Down Adjustment
B001,1,Basic Setting,Status, 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,1,Transmission RPM,(from G182),Specification: 0...1650 RPM
002,2,G182 Voltage,Transmission RPM,Specification: 0...5.00 V
002,3,Transmission,output RPM,from G195 (Specification: 0...7650 RPM)
002,4,G195 Voltage,Transmission RPM,Output (Specififcation: 0...5.00 V)
;
003,1,Driving Manner,,Specification: DS/SO/WU/TT/AS/AC
003,2,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
003,3,Vehicle Speed,,Specification: 0...255 km/h
003,4,Driving Mode,,0 = Neutral\nR = Reverse Gear\nN = Neutral\n1H = 1st Gear Hydraulic\n1M = 1st Gear Mechanic\n2H = 2nd Gear Hydraulic\n2M = 2nd Gear Mechanic\n3H = 3rd Gear Hydraulic\n3M = 3rd Gear Mechanic\n4H = 4th Gear Hydraulic\n4M = 4th Gear Mechanic\n5H = 5th Gear Hydraulic\n5M = 5th Gear Mechanic\n6H = 6th Gear Hydraulic\n6M = 6th Gear Mechanic
;
004,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
004,2,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
004,3,Declination,Recognition,Specification: UP = upward / LEVEL = no declination / DW = downward
004,4,Driving Mode,,0 = Neutral\nR = Reverse Gear\nN = Neutral\n1H = 1st Gear Hydraulic\n1M = 1st Gear Mechanic\n2H = 2nd Gear Hydraulic\n2M = 2nd Gear Mechanic\n3H = 3rd Gear Hydraulic\n3M = 3rd Gear Mechanic\n4H = 4th Gear Hydraulic\n4M = 4th Gear Mechanic\n5H = 5th Gear Hydraulic\n5M = 5th Gear Mechanic\n6H = 6th Gear Hydraulic\n6M = 6th Gear Mechanic
;
005,1,Hill Driving,Factor,Specification: -32...+31.6
005,2,Throttle valve,factor,Specification: 0...100 %
005,3,Dynamic Index,,Specification: 0...100 %
005,4,Accelerator pedal,position,Specification: 0...100 % / Kick-Down / Error
;
006,1,ATF Temperature,(G93),Specification: -50...+171 °C
006,2,Specified Current,Solenoid Valve 4,N91 (Specification: 0...1.000)
006,3,Lock-Up Clutch,Slip Condition,Specification: 0 = open / 1 = closed / 2 = slipped
006,4,Lock-Up Clutch,Slip Condition,Specification: -1250...+1250 RPM
;
007,1,Solenoid Valve 5,(N92),Specification: 0...1.000 A
007,2,Solenoid Valve 9,(N282),Specification: 0...1.000 A
007,3,Solenoid Valve 3,(N90),Specification: 0...1.000 A
007,4,Solenoid Valve 10,(N283),Specification: 0...1.000 A
;
008,1,Solenoid Valve 6,(N93),Specification: 0...1.000 A
008,2,Solenoid Valve 4,(N91),Specification: 0...1.000 A
008,3,Solenoid Valve 1,Solenoid Valve 2,N88/N89 (Specification: 0 = inactive / 1 = active)
008,4,Battery,Voltage,Specification: 0...25.5 V
;
009,1,Brake Pedal,Switch,Specification: 0 = not operated / 1 = operated
009,2,Kick-Down,Switch,Specification:  = not operated / 1 = operated
009,3,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
009,4,Multi-Function,Switch
;
010,1,ATF Temperature,,Specification: -50...+171 °C
010,2,ATF Temperature,Sensor Voltage
010,3,Transmission,Condition
010,4,Voltage Supply,,Specification: 0...25.5 V
;
011,1,Brake Pedal Switch,Condition (F47),Specification: ON = switch operated / OFF = switch not operated
011,2,Locking in P/N,Condition
011,3,Speed,,Specififcation: 0...255 km/h
011,4,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
;
012,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
012,2,Tiptronic,Recognition
012,3,Driving Mode,,0 = Neutral\nR = Reverse Gear\nN = Neutral\n1H = 1st Gear Hydraulic\n1M = 1st Gear Mechanic\n2H = 2nd Gear Hydraulic\n2M = 2nd Gear Mechanic\n3H = 3rd Gear Hydraulic\n3M = 3rd Gear Mechanic\n4H = 4th Gear Hydraulic\n4M = 4th Gear Mechanic\n5H = 5th Gear Hydraulic\n5M = 5th Gear Mechanic\n6H = 6th Gear Hydraulic\n6M = 6th Gear Mechanic
012,4,Transferrable,Torque,Specification: 0...100
;
013,1,Selector Lever,Position,Specification: P/R/N/D/S/Manual/Error
013,2,Multi-Function,Switch Position
013,3,Tiptronic,Recognition
013,4,Tiptronic (F189) &&,Tiptronic (E389),\n000xxxx1 = Tiptronic Button on Steering Wheel (E389): Down\n000xxx1x = Tiptronic Button on Steering Wheel (E389): Up\n000xx1xx = Tiptronic Button on Selector Lever (F189): Down\n000x1xxx = Tiptronic Button on Selector Lever (F189): Recognition\n0001xxxx = Tiptronic Button on Selector Lever (F189): Up
;
014,1,Accelerator pedal,position,Specification: 0...100 %
014,3,Idle Switch,Condition,Specification: 0 = not operated / 1 = operated
014,4,Accelerator Pedal,Condition,Specification: 0 = not depressed / 1 = depressed
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Brake Electronics
125,3,Instrument Cluster
125,4,All-Wheel-Drive
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,6-Speed Automatic Transmission (J217/09G) Coding
C01,0000008 = Audi A3 (8P | < MY 2005)
C02,0008201 = Audi TT (8N)
C03,0000008 = Skoda Octavia (1Z | < MY 2005)
C04,0000072 = Skoda Octavia (1Z | MY 2006 >)
C05,0000072 = VW Golf (1K) / VW Golf Plus (5M)
C06,0000328 = VW Golf (5K) / VW Golf Plus (52)
C07,0000008 = VW New Beetle (1C/1Y/9C)
C08,0000072 = VW Passat (35/3C) / VW Rabbit (5K)
C09,0000072 = VW Polo (9N)
C10,0000328 = VW Tiguan (5N) Rest of World (RoW)
C11,0000840 = VW Tiguan (5N) North American Region (NAR)
C12,0000008 = VW Touran (1T | < MY 2005)
C13,0000072 = VW Touran (1T | MY 2006 >)
C14, 
C15,If the old Control Module is still accessible read/copy it's
C16,Coding to the new Module. In case this is not possible or the
C17,Model you are working on is not listed please contact us directly
C18,and we will assist you with the Coding Process.
C19, 
C20,http://www.Ross-Tech.com/contact.html
;
