;
; VCDS Label File
;
; Copyright © 2012 Ross-Tech, LLC
;
; Audi A8 (4D)
;
; Component: J234 - Airbag (#15) AIRBAG7
;
; P/N: 4D0-959-655-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4D-15.LBL
; 8A0-959-655.LBL      (Airbag 3)
; 4D0-959-655-AI5.LBL  (Airbag 5)
; 4D0-959-655-AI7.LBL  (Airbag 7)
; 4D0-959-655-AI8.LBL  (Airbag 8)
;
; includes measuring blocks, coding and adaptation
;
; created on 27/Mar/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 27/Mar/2012
;
; requires VCDS 11.11.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags && Front Belt Tensioners)
001,1,Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
001,2,Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
002,3,Belt Tensioner,Rear Center,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Display Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Belt Yes/Belt No\nDisplay Range: Too Low/Too High/Trig.Ground/Trig.Plus/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Belt Yes/Belt No\nDisplay Range: Too Low/Too High/Trig.Ground/Trig.Plus/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Belt Yes/Belt No\nDisplay Range: Too Low/Too High/Trig.Ground/Trig.Plus/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Belt Yes/Belt No\nDisplay Range: Too Low/Too High/Trig.Ground/Trig.Plus/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Specification: Belt Yes/Belt No\nDisplay Range: Too Low/Too High/Trig.Ground/Trig.Plus/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Too Low/Too High/Trig.Ground/Trig.Plus
;
006,0,Seat Occupation (Rear)
006,1,Seat Occupation,Rear Driver Side,Display Range: Too High
006,2,Seat Occupation,Rear Pass. Side,Display Range: Too High
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 = Airbag Enabled (Standard)
A001,7,1 = Airbag Disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Airbag 7 (J234) Coding
C01,Standard: Front Airbags/Front Belt Tensioners
C02,00?2x: Side/Head Airbags
C03,0 = Side/Head Airbags NOT installed
C04,1 = Front Side Airbags installed
C05,2 = Front & Rear Side Airbags installed
C06,00x2?: Rear Belt Tensioner
C07,4 = Model Year 1997 (07/1996 > 06/1997)
C08,5 = Model Year 1998 (07/1997 > 09/1998)
;
