;
; VAG-COM Measuring Block Labels file.
; S8 HVAC System
; Filename: 4d0-820-043-q.lbl
; 
; from 2001 Audi S8
;   Controller: 4D0 820 043 Q 
;       Module: 08
;    Component: A8-Klimavollautomat D13
;       Coding: 00081
;
; **Modification History**
; Created:  Dave Eaton, 3rd February 2004
; Modified: Dave Eaton, 4th February: Test & Corrections
; Corrections to: Dave.Eaton@clear.net.nz
;
; *********************************************************************
;
1,0,Compressor Shut-off Conditions
1,1,Switch-off status,0=On 1-15=off
1,2,Voltage AC Clutch,V (>9.5 w/comp off)
1,3,Voltage at,Terminal 15 (>12)
1,4,Air Quality Sensor,G238
;
2,0,Defroster Flap Motor V107 Position Sensor G135
2,1,Actual Position,20 < 230
2,2,Specified Position,(as #1) 20 < 230
2,3,Basic Setting,Closed (20<60)
2,4,Basic Setting,Open (190<230)
;
3,0,Center Air Flap Motor (V110) Position Sensor Motor G136
3,1,Actual Position,60 < 230
3,2,Specified Position,(as #1) 60 < 230
3,3,Basic Setting,Closed (60<100)
3,4,Basic Setting,Open (190<230)
;
4,0,Right Center Air Flap Motor (V111) Position Sensor Motor G137
4,1,Actual Position,20 < 190
4,2,Specified Position,(as #1) 20 < 190
4,3,Basic Setting,Closed (20<60)
4,4,Basic Setting,Open (150<190)
;
5,0,Center Vent Motor (V102) Position Sensor Motor G138
5,1,Actual Position,60 < 230
5,2,Specified Position,(as #1) 60 < 230
5,3,Basic Setting,Closed (60<100)
5,4,Basic Setting,Open (190<230)
;
6,0,Temperature Flap Motor (V68) Position Sensor Motor G92
6,1,Actual Position,20 < 185
6,2,Specified Position,(as #1) 20 < 185
6,3,Basic Setting,Closed (20<75)
6,4,Basic Setting,Open (135<185)
;
7,0,Center Footwell Flap Motor (V108) Position Sensor Motor G139
7,1,Actual Position,20 < 190
7,2,Specified Position,(as #1) 20 < 190
7,3,Basic Setting,Closed (20<60)
7,4,Basic Setting,Open (150<190)
;
8,0,Right Footwell Flap Motor (V109) Position Sensor Motor G140
8,1,Actual Position,60 < 240
8,2,Specified Position,(as #1) 60 < 240
8,3,Basic Setting,Closed (60<100)
8,4,Basic Setting,Open (200<240)
;
9,0,Rear Footwell Vent Motor (V112) Position Sensor Motor G141
9,1,Actual Position,60 < 230
9,2,Specified Position,(as #1) 60 < 230
9,3,Basic Setting,Closed (60<100)
9,4,Basic Setting,Open (190<230)
;
10,0,Air-flow Flap Motor (V71) Position Sensor Motor G113
10,1,Actual Position,50 < 215
10,2,Specified Position,(as #1) 50 < 215
10,3,Basic Setting,Closed (50<100)
10,4,Basic Setting,Open (165<215)
;
11,0,Recirculation Flap Motor (V113) Position Sensor Motor G143
11,1,Actual Position,10 < 210
11,2,Specified Position,(as #1) 10 < 210
11,3,Basic Setting,Closed (10<50)
11,4,Basic Setting,Open (170<210)
;
12,0,CAN Information
12,1,ECM Messages,0=Not Rec 1=Rec
12,2,Instr. Clstr,0=Not Rec 1=Rec
12,3,N/A
12,4,N/A
;
13,0,Recirculation Flap Motor (V183) Position Sensor Motor G184
13,1,Left Centre Vent,0=Cl 1=Mid 2=Op
13,2,Right Centre Vent,0=Cl 1=Mid 2=Op
13,3,Centre Vent,Cold>5 Warm<250
13,4,N/A
;
14,0,Air Temperature Sensors
14,1,Outside Air Temp,G17 Celsius
14,2,Fresh Air Duct,G89 Celsius
14,3,LF Vent Temp,G150 Celsius
14,4,RF Vent Temp,G151 Celsius
;
15,0,Instrument Panel Interior Temp Sensor G56, Coolant Temp G107
15,1,G56 Value,Celsius
15,2,Trans. Coolant,Temp Celsius
15,3,Sun Sensor,Left G107 %
15,4,Sun Sensor,Right G107 %
;
16,0,Voltage & Fresh Air Blower V2 Parking Light 58D
16,1,V2 Specified,Volts (3.5 < 12.5)
16,2,V2 Actual,Volts
16,3,% of Max Volts,% <10 Light Off
16,4,Panel Dimmer Sw,% Permissable
;
17,0,Engine and Vehicle Speed
17,1,Engine,Speed RPM
17,2,Vehicle Speed,Km/h
17,3,Parking Light,0=Off 1=On
17,4,Aux Heater,0=No 1=Yes
;
18,0,Kick-down, Coolant temp.
18,1,Rear Wind. Defrost,0=Off 1=On
18,2,Over Temp Switch,0=<118C 1=OvTmp
18,3,Compr. Cutin,0=Open 1=Closed
18,4,High Pr.Sw F118,0=Closed 1=Open
;
19,0,Coolant Pump V50 -Heat Reg Valve N175 Right -Heat Reg Valve N176
19,1,N175,1=Open 0=Closed
19,2,N176,1=Open 0=Closed
19,3,V50,0=Off 1=On
19,4,Windscreen Def
;
20,0,Last 4 Compressor Shutoff COnditions > 20 seconds
;
21,0,Fan Conditions
21,1,Idle Control,0=Off 1=On
21,2,Coolant Fan,Stage 1 0=Off 1=On
21,3,Coolant Fan,Stage 2 0=Off 1=On
21,4,W/scr Washer Sw,0=Off 1=On
;
22,0,Ignition Conditions
22,1,Known Key Alloc,0=Ig. Off 1=Ig. On
22,2,Last Shut Off,Time
22,3,N/A
22,4,N/A
;
; End of File

