;
; VAG-COM Label File
;
; Audi Q7 (4L)
;
; Component: J388/J389 - Rear Door Electronics (#62/72)
;
; P/N: 4L0-910-795-???
;
; includes measuring blocks, coding and selective output test
;
; created on 01/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 02/Jun/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,Door Status,,0 = inactive\n1 = active
; xxxxxxx? = Key Switch open
; xxxxxx?x = Key Switch closed
; xxxxx?xx = Central Locking (CL) Interior Switch locking
; xxxx?xxx = Central Locking (CL) Interior Switch unlocking
; xxx?xxxx = Lock Feedback "locked"
; xx?xxxxx = Lock Feedback "safed" (not USA)
; x?xxxxxx = Door Contact Switch
; ?xxxxxxx = Catch (for Closing Assistance)
001,2,Button Status,,0 = inactive\n1 = active
; 000000x? = Interior Door Handle Button
; 000000?x = External Door Handle Button
001,3,Voltages and,Databus Status,0 = inactive\n1 = active
; 0000xxx? = Terminal 30 (Window Regulator)
; 0000xx?x = Terminal 30 (Central Locking)
; 0000x?xx = Terminal 15
; 0000?xxx = CAN-Comfort in Single-Wire Mode
001,4,Voltage Supply
;
002,0,Window Regulator Buttons (Local)
002,1,WR-Button,(Local),Display Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
;
003,0,Window Regulator
003,1,Window Regulator,Position,Display Range: 0.0...100.0 %
003,2,Window Regulator,Motor Temperature,Display Range: -50.0...+200.0 °C
003,3,Window Regulator,Status,0 = inactive\n1 = active
; xxx? = Window Regulators Enabling
; xx?x = Thermal Protection
; x?xx = Standardized
; ?xxx = Insulated Glass
003,4,Window Regulator,Movement,Display Range: Still/Open/Closed
;
005,1,Vehicle Speed,,Display Range: 0.0...255.0 km/h
005,2,Ambient,Temperature,Display Range: -50.0...+200.0 °C
;
006,4,Miscellaneous,,0 = inactive\n1 = active
; 0000000? = Kessy Lock Button
;
007,1,Closing,Assistance,Display Range: Not Installed
007,2,Opening,Assistance,Display Range: Not Installed
007,3,Child Safety,Lock Button,Display Range: Operated/Not Oper./Not Installed
007,4,Window Regulator,Current Consumpt.
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Rear Door Electronics (J388/J389) Coding
C01,+0000002 = Interior Door Handle Illumination
C02,+0000004 = Insulated Glass installed (PR-4KR/4KV)
C03,+0000008 = Door Warning Lights installed
C04,+0000016 = Right Hand Steering (PR-L0R)
C05,+0000032 = Lighting Package (Interior Lighting - PR-QQ1)
C06,+0000512 = Interior Lock Switch installed
C07,+0002048 = Electrical Child Safety Lock (PR-4H5)
C08,+0004096 = Opening Assistance
C09,+0008192 = Closing Assistance (PR-GZ2)
C10,+0016384 = Keyless-Entry installed (PR-4F2/4K5/4K7)
C11,+0032768 = Safe Function disabled (PR-A8U)
C12,+0065536 = Window Regulator Comfort Function disabled
C13,+0524288 = Pinch Protection disabled
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
T1482,Motors for Central Locking
T2111,Motor for Window Regulator
T2131,Child Safety Lock Motor
T2188,Lighting/Illumination
;
