;
REDIRECT,7L6-907-357-A.LBL,A,C
;
; VCDS Label File
;
; Copyright © 2008-2009 Ross-Tech, LLC
;
; VW Phaeton (3D) / VW Touareg (7L)
;
; Component: J745 - Cornering Lights Headlight Range Control (#55)
;
; P/N: 7L6-907-357-A
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7L6-907-357.LBL
; 7L6-907-357-A.LBL
;
; includes measuring blocks, basic setting, security access, adaptation and coding
;
; created on 14/Feb/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 16/Jun/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15)
001,2,Light Status,(Terminal 56b),Display Range: ON/OFF
001,3,Vehicle Speed
001,4,Steering Angle,Sensor (G85)
;
B001,0,Adjustment Position && Adjustment Learning
B001,1,Status
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,1,Sensor Signal,Front (G78/G289),Range: 0.0...100.0 %
002,2,Sensor Signal,Rear (G76/G77),Range: 0.0...100.0 %
002,3,Actuator Motor,Left Headlight,Range: 0.0...100.0 %
002,4,Actuator Motor,Right Headlight,Range: 0.0...100.0 %
;
003,0,Cornering Light
003,1,Static Cornering,Light Left
003,2,Static Cornering,Light Right
003,3,Dynamic Cornering,Light Left
003,4,Dynamic Cornering,Light Right
;
004,1,Sensor Signal,Front (G78),Range: 0.0...100.0 %
004,2,Sensor Signal,Rear (G76),Range: 0.0...100.0 %
004,3,Movement,Front Suspension,Display Range: -127.0...+128.0 mm
004,4,Movement,Rear Suspension,Display Range: -127.0...+128.0 mm
;
005,0,Voltage Supply
005,2,Sensor,Voltage Supply
005,3,Voltage Light,Module Left
005,4,Voltage Light,Module Right
;
006,1,Reverse Gear,engaged,Range: Reverse: No/Reverse: Yes
006,2,Cornering Light,deactived,Range: Yes/No
;
008,1,Helligkeit,Lichtsensor
008,2,Status,Regensensor
008,3,Status,Lichtsensor
008,4,
;OK , ,
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,2,CAN-Gateway,(J533),Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
125,3,Power Steering,(J500),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
125,4,Engine,Electronics,Specification: Engine 1\Display Range: Engine 1/Engine 0
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Level Control,,Range: Level 0/Level 1
126,2,All Wheel Drive,,Specification: AWD 1\nRange: AWD 0/AWD 1
126,3,Instrument Cluster,(J285),Specification: Instruments 1\nRange: Instruments 1/Instruments 0
;
127,0,CAN-Databus Communication (Light)
127,1,Left Output,Stage (J667),Specification: LeiMo Left 1\nDisplay Range: LeiMo Left 1/LeiMo Left 0
127,2,Right Output,Stage (J668),Specification: LeiMo Right 1\nDisplay Range: LeiMo Right 1/LeiMo Right 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Cornering Lights Headlight Range Control (J745) Coding
C01,0000001 = VW Phaeton (3D3/3D7) Left-Hand-Drive (LHD)
C02,0000002 = VW Touareg (7L6) Steel Suspension / Left-Hand-Drive (LHD)
C03,0000003 = VW Touareg (7L6) Air Suspension / Left-Hand-Drive (LHD)
C04,0000004 = VW Phaeton (3D3/3D7) Right-Hand-Drive (RHD)
C05,0000005 = VW Phaeton (3D3/3D7) North American Region (NAR)
C06,0000006 = VW Touareg (7L6) Steel Suspension / Right-Hand-Drive (RHD)
C07,0000008 = VW Touareg (7L6) Air Suspension / Right-Hand-Drive (RHD)
C08,0000007 = VW Touareg (7L6) Steel Suspension / North American Region (NAR)
C09,0000009 = VW Touareg (7L6) Air Suspension / North American Region (NAR)
C10, 
C11,Note #1: 3D2/3D8 = Pre-Facelift and 3D3/3D7 = Facelift
C12,Note #2: 7LA = Pre-Facelift and 7L6 = Facelift
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Cornering Lights Headlight Range Control (J745) Security Access
S01,15284 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A016,0,Tourist Solution
A016,5,Tourist Solution
A016,6,When driving in countries where driving is performed on the
A016,7,opposite side as in the native country the headlights must
A016,8,be changed over to avoid blinding the oncoming traffic.
A016,9, 
A016,10,0 = Disabled
A016,11,1 = Enabled
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1540,Headlight Range Control: Adjusting to Lowered Position
T1541,Headlight Range Control: Adjusting to Raised Position
T2625,Headlight Range Control: Adjusting to Delivery Position
T2623,Dynamic Cornering Light: Adjusting to Center Position
T2941,Dynamic Cornering Light: Position Left
T2942,Dynamic Cornering Light: Position Right
T2947,Static Cornering Light Left: up/bright
T2948,Static Cornering Light Left: down/dim
T2949,Static Cornering Light Right: up/bright
T2950,Static Cornering Light Right: down/dim
T2952,Control Circuit for Curve Lighting Warning Light
;
