;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A4 (8E)
;
; Component: J104 - Brake Electronics (#03) - Bosch 5.7
;
; P/N: 8E0-614-517-???
;
; includes measuring blocks, coding and login
;
; created on 26/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modificationon on 17/Jul/2012
;
; requires VCDS 11.2.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
B001,0,Steering Angel Sensor (G85) Alignment
B001,1,Steering Angel,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,0,Switches && Buttons
002,1,Brake Test Switch,,Display Range: 0/operated
002,2,Brake Light Switch,,Display Range: 0/operated
002,3,Parking Brake,Button,Display Range: 0/operated
002,4,ESP-Passive,Button,Display Range: 0/operated
;
B002,0,Brake System Bleeding
B002,1,Status, , 
B002,2, , , 
B002,3, , , 
B002,4, , , 
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
B003,0,Activate ESP System/Function Test
B003,1,Status, , 
B003,2, , , 
B003,3, , , 
B003,4, , , 
;
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,Sensor (G85),Display Range: -720.0...+720.0 °\nTolerance (when straight): ±5.0 °
005,2,Rotation Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,(J106),Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,(V39),Display Range: ON/OFF
006,4,Work Shop Code
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 0/Steer. ang. 1
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Engine,,Specification: Engine 1\nDisplay Range: Engine 0/Engine 1
125,4,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 0/Instruments 1
;
;
;---------------------------------------------------
;
; login/coding-ii
;
;---------------------------------------------------
;
;
L00,Brake Electronics (J104/Bosch 5.7) Login
L01,0?xxx: Chassis
L02,9 = Audi A4
L03,0x?xx: Brakes
L04,2 = Brembo 17" (PR-1LJ)
L05,3 = FN3 16" (PR-1LT/1LF)
L06,4 = HP2 16" (PR-1LX)
L07,4 = FNR 16" (PR-1LA/1LG)
L08,5 = FN3 15" (PR-1LB/1LE)
L09,6 = C54 (PR-1LZ)
L10,0xx?x: Engine
L11,5 = 4/6 Cyl. Diesel
L12,7 = 4/5 Cyl. Gasoline
L13,9 = 6/8 Cyl. Gasoline
L14,0xxx?: Transmission
L15,5 = Manual
L16,7 = Automatic (09L)
L17,9 = Multitronic (01J)
L18, 
L19,Note #1: After Login/Coding-II has been carried out you need to recode the Control Module.
L20,Note #2: Special Login/Coding-II 09399 is used for BFB Engine with 1LT Brakes and Multitronic.
L21, 
L22,40168 = Basic Settings Enabling (i.e. mandatory prior to Steering Angle Sensor Alignment)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104/Bosch 5.7) Coding
C01,0?xxx: Chassis
C02,4 = Audi A4
C03,0x?xx: Brakes
C04,1 = C54 (PR-1LZ)
C05,2 = FN3 15" (PR-1LB/1LE)
C06,3 = HP2 16" (PR-1LX)
C07,3 = FNR 16" (PR-1LG)
C08,4 = FN3 16" (PR-1LT/1LF)
C09,5 = Brembo 17" (PR-1LJ)
C10,0xx?x: Engine
C11,5 = 4/6 Cyl. Diesel
C12,7 = 4/5 Cyl. Gasoline
C13,9 = 6/8 Cyl. Gasoline
C14,0xxx?: Transmission
C15,5 = Manual
C16,7 = Automatic (09L)
C17,9 = Multitronic (01J)
C18,Note #1: Coding is accepted after a specific Login has been carried out.
C19,Note #2: Special Coding 04499 is used for BFB Engine with 1LT Brakes and Multitronic.
C20,Note #3: After successful Coding the Steering Angle Sensor Alignment needs to be carried out.
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,Bosch ESP 5.7
;
