;
; VAG-COM Label File
;
; VW Touareg (7L)
;
; Component: J502 - Tire Pressure Monitoring (#65)
;
; P/N: 7L0-907-273-???
;
; includes measuring blocks, coding, adaptation and sec. access
;
; created on 09/Nov/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 14/Aug/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Front Left Wheel Status I
001,1,Position,No Display = Not yet recognized
001,2,Wheel,Temperature,Range: -40.0...+120.0 °C / Not Recogn.
001,3,Wheel Pressure,(actual),Range: 0.0...5.37 bar
001,4,Wheel Pressure,(specified),Range: 0.0...5.37 bar
;
002,0,Front Left Wheel Status II
002,1,Position,No Display = Not yet recognized
002,2,Remaining,Battery Life (Month),Range: 0...99 Month
;
003,0,Front Left Wheel Status III
003,1,Wheel Sensor,Position,No Display = Not yet recognized
003,2,Wheel Sensor,Identification
003,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
003,4,Wheel Sensor,Battery Status
;
004,0,Front Right Wheel Status I
004,1,Position,No Display = Not yet recognized
004,2,Wheel,Temperature,Range: -40.0...+120.0 °C / Not Recogn.
004,3,Wheel Pressure,(actual),Range: 0.0...5.37 bar
004,4,Wheel Pressure,(specified),Range: 0.0...5.37 bar
;
005,0,Front Right Wheel Status II
005,1,Position,No Display = Not yet recognized
005,2,Remaining,Battery Life (Month),Range: 0...99 Month
;
006,0,Front Right Wheel Status II
006,1,Wheel Sensor,Position,No Display = Not yet recognized
006,2,Wheel Sensor,Identification
006,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
006,4,Wheel Sensor,Battery Status
;
007,0,Rear Left Wheel Status I
007,1,Position,No Display = Not yet recognized
007,2,Wheel,Temperature,Range: -40.0...+120.0 °C / Not Recogn.
007,3,Wheel Pressure,(actual),Range: 0.0...5.37 bar
007,4,Wheel Pressure,(specified),Range: 0.0...5.37 bar
;
008,0,Rear Left Wheel Status II
008,1,Position,No Display = Not yet recognized
008,2,Remaining,Battery Life (Month),Range: 0...99 Month
;
009,0,Rear Left Wheel Status III
009,1,Wheel Sensor,Position,No Display = Not yet recognized
009,2,Wheel Sensor,Identification
009,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
009,4,Wheel Sensor,Battery Status
;
010,0,Rear Right Wheel Status I
010,1,Position,No Display = Not yet recognized
010,2,Wheel,Temperature,Range: -40.0...+120.0 °C / Not Recogn.
010,3,Wheel Pressure,(actual),Range: 0.0...5.37 bar
010,4,Wheel Pressure,(specified),Range: 0.0...5.37 bar
;
011,0,Rear Right Wheel Status II
011,1,Position,No Display = Not yet recognized
011,2,Remaining,Battery Life (Month),Range: 0...99 Month
;
012,0,Rear Right Wheel Status III
012,1,Wheel Sensor,Position,No Display = Not yet recognized
012,2,Wheel Sensor,Identification
012,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
012,4,Wheel Sensor,Battery Status
;
013,0,Spare Tire I
013,1,Position,No Display = Not yet recognized
013,2,Wheel,Temperature,Range: -40.0...+120.0 °C / Not Recogn.
013,3,Wheel Pressure,(actual),Range: 0.0...5.37 bar
013,4,Wheel Pressure,(specified),Range: 0.0...5.37 bar
;
014,0,Spare Tire II
014,1,Position,No Display = Not yet recognized
014,2,Remaining,Battery Life (Month),Range: 0...99 Month
;
015,0,Spare Tire III
015,1,Wheel Sensor,Position,No Display = Not yet recognized
015,2,Wheel Sensor,Identification
015,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
015,4,Wheel Sensor,Battery Status
;
016,0,Wheel Sensor Status (from last Received Wheel ID) I
016,1,Wheel Sensor,Identification
016,2,Wheel Sensor,Status,No Display = Not yet recognized
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
016,3,Wheel Sensor,Battery Status
016,4,Wheel Pressure,(actual)
;
017,0,General
017,1,Work Shop Code,(Last Adaptation)
017,2,Voltage,(Terminal 30)
017,3,Vehicle Status,,0 = Vehicle driving (> 5 km/h)\n1 = Vehicle standing
017,4,Vehicle Speed
;
018,0,General
018,1,Ambient,Temperature,Range: -40.0....+120.0 °C
;
019,0,Calibration Status
019,1,Calibration,Status,Specification: 00025 (Ideal)
;
020,0,CAN-Comfort Condition
020,1,CAN-Comfort,Condition,Range: 1-Wire/2-Wire\nSpecification: 2-Wire
;
021,0,Antenna Diagnosis
021,1,Diagnosis,Status,See Adaptation Channel 17
;
080,0,Advanced Control Module Identification I
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Tire Pressure Monitoring (J502) Coding
C01,Software Version "< 0052":
C02,0012339 = Factory
C03,0011339 = Factory (Shortened End of Line Test)
C04,0010339 = Customer Service
C05, 
C06,Software Version "=> 0052":
C07,0210390 = North American Region (NAR)
C08,0110390 = Rest of World (RoW)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Tire Pressure Monitoring
A001,5,Tire Pressure Monitoring
A001,6,0 = Disabled
A001,7,1 = Enabled
A001,8, 
A001,9,The TPMS has to be deactivated e.g. to use winter tires w/o wheel sensors
A001,10,to suppress error messages. The TPMS symbol will be active and can not
A001,11,be deactived unless the system is beeing activated again.
;
A004,0,Tire Pressure Adaptation
A004,5,Tire Pressure Adaptation
A004,6,To force the tire pressure learning process via diagnosis
A004,7,save "1" as new value. As long as the warning message in
A004,8,the dash is active make sure to do a continous 30 minute
A004,9,driving cycle with a speed above 5 km/h. Driving "Stop and Go"
A004,10,will extend the driving cycle. The warning message will
A004,11,go off after the adaptation is successfully finished.
A004,12,This procedure is the same as through the instrument cluster.
;
A017,0,Antenna Diagnosis
A017,5,Antenna Diagnosis
A017,6,0 = ON
A017,7,1 = OFF
A017,8, 
A017,9,See Measuring Block 021.
;
;
;---------------------------------------------------
;
; security access information
;
;---------------------------------------------------
;
;
S00,Tire Pressure Monitoring (J502) Security Access
S01,10896 = General Adaptation "Enabling"
;
