;
; VCDS Label File
;
; Copyright © 2012 Ross-Tech, LLC
;
; Audi A2 (8Z) / Audi A3 (8L) / Audi A4 (8D) / Audi A6 (4B)
;
; Component: Navigation System (#37) - BNS 4.x
;
; T/N: 4B0-919-887-?
;
; includes measuring blocks and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4B-37.LBL
; 8Z-37.LBL
; 4B0-919-887-BNS4.LBL
;
; created on 10/Mar/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 10/Mar/2012
;
; requires VCDS 11.11.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Speed Signal,recognized,Range: 0 = not recognized / 1 = recognized
001,2,Supply Voltage,(Terminal 30),Range: 0.0...20.0 V\nSpecification: 8.0...15.0 V
;
002,0,Input Signals
002,1,Backup-Light,Switch,Range: Reverse OFF/Reverse ON
002,2,Status,Terminal 15,Range: ON/OFF
;
003,0,GPS-Antenna (Active/Remote Supplied)
003,1,GPS-Antenna
003,2,GPS-Antenna,Status,Range: OK/Short Circuit/Open Circuit
;
004,0,External Display
004,1,External Display
004,2,External Display,Status,Range: OK/n.OK
;
005,0,Internal Databus
005,1,Internal,Databus
005,2,Status,Databus,Range: OK/Not OK
;
006,0,Vehicle Speed
006,1,ABS-Sensor,Rear Left
006,2,Calculated,Vehicle Speed,Based on GALA Signal as well as\nWheel Impuls and Circumference.
;
007,0,Production Diagnostics
007,1,System,Status,Specification: 255\n\n+001 = CAN-Communication Navigation System OK\n+002 = Current Draw for GPS-Antenna (10-30 mA) OK\n+004 = Terminal 15 (Ignition ON) recognized\n+008 = Backup-Light Switch recognized\n+016 = CAN-Communication Instrument Cluster OK\n+032 = Signal Wheel Impulse at least once recognized\n+064 = Wheel Impulse Adaptation OK\n+128 = Tire Circumference Adaptation OK
; +001 = CAN-Communication Navigation System OK
; +002 = Current Draw for GPS-Antenna (10-30 mA) OK
; +004 = Terminal 15 (Ignition ON) recognized
; +008 = Backup-Light Switch recognized
; +016 = CAN-Communication Instrument Cluster OK
; +032 = Signal Wheel Impulse at least once recognized
; +064 = Wheel Impulse Adaptation OK
; +128 = Tire Circumference Adaptation OK
;
008,0,Front Speaker
008,1,Front Speaker
008,2,Status,Front Speaker,Range: OK/Short Circuit/Open Circuit
;
010,0,Telephone Mute Status
010,1,Telephone Mute
010,2,Telephone,Mute Status,Range: ON/OFF
;
;
;---------------------------------------------------
;
; Anpassung
;
;---------------------------------------------------
;
;
A001,0,Tire Circumference
A001,5,Tire Circumference
A001,6,The tire circumference is beeing adapted in "mm".
;
A002,0,Wheel Impulse
A002,5,Wheel Impulse
A002,6,The Distance Impulse describes the amount
A002,7,of ABS Pulses per Wheel Revolution.
A002,8, 
A002,9,8 = All Models excl. Audi A3 (8P)
A002,10,43 = Audi A3 (8P)
;
A003,0,Production Diagnostics
A003,5,Production Diagnostics
A003,6,The Result of the Production Diagnostics is
A003,7,displayed in Measuring Value Block 007 Field 1.
A003,8, 
A003,9,0 = Production Diagnostics inactive
A003,10,1 = Production Diagnostics active
;
A004,0,Speaker System
A004,5,Speaker System
A004,6,If a Radio System is installed the Radio Speaker
A004,7,Front Left will be used for Navigation Instructions.
A004,8,Otherwise a separate Speaker will be used/installed.
A004,9, 
A004,10,0 = External Speaker (Radio installed)
A004,11,1 = Internal Speaker
;
A005,0,Country
A005,5,Country
A005,6,0 = Europe (EU)
A005,7,1 = North American Region (NAR)
;
A006,0,Dynamic Route Guidance
A006,5,Dynamic Route Guidance
A006,6,0 = Dynamic Route Guidance NOT active
A006,7,1 = Dynamic Route Guidance via Radio Symphony II
A006,8,2 = Dynamic Route Guidance via Telematics II
A006,9,3 = Dynamic Route Guidance via Radio Symphony II and Telematik II
;
A007,0,Electronic Trip Recorder
A007,5,Electronic Trip Recorder
A007,6,0 = Electronic Trip Recorder NOT installed
A007,7,1 = Electronic Trip Recorder installed
;
A010,0,Communication Type (External Display))
A010,5,Communication Type (External Display))
A010,6,0 = All Models excl. Audi A3 (8P)
A010,7,1 = Audi A3 (8P)
;
A066,0,Speed Signal (GALA) Function
A066,5,Speed Signal (GALA) Function
A066,6,0 = Speed Signal Function active
A066,7,1 = Speed Signal Function inactive
;
