;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Audi A6 (4F)
;
; Component: J533 - Diagnostic Interface for Databus (#19)
;
; P/N: 4F0-910-468-???
;
; includes measuring blocks and long coding
;
; created on 12/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 05/Dec/2010
;
; requires VCDS 10.6.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Line Status
001,1,Wake-Up Line,,Display Range: Passive/Active
001,2,CAN-Comfort,Static,Display Range: [No Value]/CmfCAN Stat
001,3,CAN-Infotainment,Static,Display Range: [No Value]/InfCAN Stat
001,4,CAN-Powertrain,Static,Display Range: [No Value]/PwrCAN Stat
;
002,1,Unlearn Counter
002,4,Ring Break,Diagnostic Wire,0 = Low\n1 = High (~5V)
;
010,0,CAN-Gateway Status
010,1,CAN-Gateway,Status,0 = No Error\n1 = RAM-Error\n2 = ROM-Error\n3 = EEPROM-Error
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,Electronics,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Transmission,Electronics,Specification: Transm. 1\nDisplay Range: Transm. 1/Transm. 0
125,3,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,4,Instrument Cluster,(J285),Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Engine,Electronics II,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
126,2,Airbag System,(J234),Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
126,3,Level Control,(J197),Range: Level 0/Level 1\nSpecification: Level 1
126,4,Headlight Range,(J431),Specification: HdLtRange 1\nDisplay Range: HdLtRange 1/HdLtRange 0
;
127,0,CAN-Databus Powertrain (Communication)
127,1,Parking Brake,Electronics (J540),Specification: Park Brake 1\nDisplay Range: Park Brake 1/Park Brake 0
127,2,Distance,Regulation (J428),Specification: Distance 1\nDisplay Range: Distance 1/Distance 0
127,3,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
;
130,0,CAN-Databus Comfort (Communication)
130,1,CAN-Comfort,Status,Specification: 2-Wire\nDisplay Range: 2-Wire/1-Wire
130,2,Central Electronics,(J519),Specification: E.Load.Crtl 1\nDisplay Range: E.Load.Crtl 1/E.Load.Crtl 0
130,3,Comfort System,(J393),Specification: Central 1\nDisplay Range: Central 1/Central 0
130,4,Door Electronics,Driver (J386),Specification: Dr. Door 1\nDisplay Range: Dr. Door 1/Dr. Door 0
;
131,0,CAN-Databus Comfort (Communication)
131,1,Door Electronics,Passenger (J387),Specification: Pas. Door 1\nDisplay Range: Pas. Door 1/Pas. Door 0
131,2,Door Electronics,Rear Left (J388),Specification: RL Door 1\nDisplay Range: RL Door 1/RL Door 0
131,3,Door Electronics,Rear Right (J389),Specification: RR Door 1\nDisplay Range: RR Door 1/RR Door 0
131,4,Seat Memory,Driver (J521),Specification: Memory 1\nDisplay Range: Memory 1/Memory 0
;
132,0,CAN-Databus Comfort (Communication)
132,1,Parking Aid,Electronics (J446),Specification: Parking 1\nDisplay Range: Parking 1/Parking 0
132,2,Seat Memory,Passenger (J136),Specification: Memory Pax 1\nDisplay Range: Memory Pax 1/Memory Pax 0
132,3,Tire Pressure,Monitoring (J502),Specification: Tire 1\nDisplay Range: Tire 1/Tire 0
132,4,Steering Wheel,Electronics (J527),Specification: St. Wheel 1\nDisplay Range: St. Wheel 1/St. Wheel 0
;
133,0,CAN-Databus Comfort (Communication)
133,1,Engergy,Management,Specification: E-Mgmnt 1\nDisplay Range: E-Mgmnt 1/E-Mgmnt 0
133,2,Heating/Air,Condition (J255),Specification: A/C 1\nDisplay Range: A/C 1/A/C 0
133,3,Access/Start,Authorization,Specification: El.Ign.Lock 1\nDisplay Range: El.Ign.Lock 1/El.Ign.Lock 0
133,4,Driver,Identification
;
134,0,CAN-Databus Comfort (Communication)
134,1,Auxiliary,Heater
134,2,Roof Electronics
134,3,Central (J520),Electronics II,Specification: Electr. ZE2 1\nDisplay Range: Electr. ZE2 1/EElectr. ZE2 0
134,4,Trailer,Electronics (J345),Specification: Trailer 1\nDisplay Range: Trailer 1/Trailer 0
;
140,0,CAN-Databus Infotainment (Communication)
140,1,Analog Radio,,Specification: Radio 1\nDisplay Range: Radio 1/Radio 0
140,2,Navigation,,Specification: Navigation 1\nDisplay Range: Navigation 1/Navigation 0
140,3,Telephone,Electronics,Specification: Telephone 1\nDisplay Range: Telephone 1/Telephone 0
140,4,Voice Control,,Specification: VoiceCmd 1\nDisplay Range: VoiceCmd 1/VoiceCmd 0
;
141,0,CAN-Databus Infotainment (Communication)
141,1,Digital,Soundsystem,Specification: Dig.Soundp. 1\nDisplay Range: Dig.Soundp. 1/Dig.Soundp. 0
141,2,TV-Tuner,(J415),Specification: TV-Tuner 1\nDisplay Range: TV-Tuner 1/TV-Tuner 0
141,3,Telematic,,Specification: Telemat 1\nDisplay Range: Telemat 1/Telemat 0
141,4,Display/Control,Head Front,Specification: Disp/Ctrl/F 1\nDisplay Range: Disp/Ctrl/F 1/Disp/Ctrl/F 0
;
142,0,CAN-Databus Infotainment (Communication)
142,1,Display/Control,Head Rear
142,2,Display/Control,Head Rear Left
142,3,Display/Control,Head Rear Right
142,4,Media Player 1,,Specification: Media P.1 1\nDisplay Range: Media P.1 1/Media P.1 0
;
143,0,CAN-Databus Infotainment (Communication)
143,1,Media Player 2,,Specification: Media P.2 1\nDisplay Range: Media P.2 1/Media P.2 0
143,2,Media Player 3,,Specification: Media P.3 1\nDisplay Range: Media P.2 1/Media P.3 0
143,3,Media Player 4,,Specification: Media P.4 1\nDisplay Range: Media P.3 1/Media P.4 0
;
144,0,CAN-Databus Infotainment (Communication)
144,1,Digital Radio,,Specification: DigitRadio 1\nDisplay Range: DigitRadio 1/DigitRadio 0
;
200,0,Voltage Supply
200,2,Voltage,(Terminal 30)
200,3,Voltage,(Terminal 15)
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,0,[69] Trailer
LC,00,1,[13] Distance Regulation
LC,00,2,[15] Airbag
LC,00,3,[61] Battery Regulation
LC,00,4,[3D] Special Functions
LC,00,5,[03] Brake Electronics
LC,00,6,[53] Parking Brake
LC,00,7,[76] Parking Aid
LC,01,0,[1D] Driver Identification
LC,01,1,[05] Access/Start Authorization
LC,01,2,[25] Immobilizer
LC,01,3,[19] CAN-Gateway (Standard)
LC,01,4,[02] Automatic Transmission
LC,01,5,[09] Central Electronics
LC,01,6,[4F] Central Electronics II
LC,01,7,[46] Central Convenience
LC,02,0,[17] Instrument Cluster
LC,02,1,[08] Heating/Air Conditioning (Front)
LC,02,2,[28] Heating/Air Conditioning (Rear)
LC,02,3,[34] Level Control
LC,02,4,[00] Steering Wheel Sensor (G85)
LC,02,5,[55] Xenon Range
LC,02,6,[01] Engine Electronics I
LC,02,7,[11] Engine Electronics II
LC,03,0,[65] Tire Pressure Monitoring
LC,03,1,[18] Auxiliary Heating
LC,03,2,[16] Steering Wheel Electronics
LC,03,3,[36] Seat Memory (Driver)
LC,03,4,[06] Seat Memory (Passenger)
LC,03,5,[66] Seat Memory (Rear)
LC,03,6,[42] Door Electronics (Driver)
LC,03,7,[52] Door Electronics (Passenger)
LC,04,0,[62] Door Electronics (Rear Left)
LC,04,1,[72] Door Electronics (Rear Right)
LC,04,2,[27] Control Head (Rear)
LC,04,3,[07] Control Head (Front)
LC,04,4,[0E] Mediaplayer Position 1
LC,04,5,[1E] Mediaplayer Position 2
LC,04,6,[2E] Mediaplayer Position 3
LC,04,7,[3E] Mediaplayer Position 4
LC,05,0,[56] Radio (Analog)
LC,05,1,[75] Telematic/Emergency Call
LC,05,2,[57] TV-Tuner
LC,05,3,[0F] Radio (Digital)
LC,05,4,[77] Telephone
LC,05,5,[37] Navigation System
LC,05,6,[67] Voice Control
LC,05,7,[4E] Control Head (Rear Right)
LC,06,0,[5E] Control Head (Rear Left)
LC,06,1,[6D] Trunk Electronics
LC,06,2,[47] Sound System
;
