Maintenance

# Transporting the Scanner

Before transporting the scanner over a long distance or storing it for an extended period, you need to lock the scanner's carriage to prevent damage. Follow the steps below.

| Plug in the scanner and wait until the carriage moves to the home position (position nearest the cover hinges). When the Start button turns on in green, unplug the power cord.

| Disconnect the AC adapter from the DC inlet, and then slide the transportation lock to the left (the locked position).

| Note for Perfection 1660 Photo and 2400 Photo users:

If you are using the optional Film Adapter and it is switched on, the carriage will not move to the home position. Remove the optional Film Adapter first, then perform the steps above.

[Top]

Previous | Next