Technical Specifications

# USB Interface

> Perfection 1260 and 1260 Photo
> Perfection 1660 Photo
> Perfection 2400 Photo

## Perfection 1260 and 1260 Photo

Interface type: | Universal Serial Bus Specification Revision 1.1
Electrical standard: | Full speed mode of Universal Serial Bus Specification Revision 1.1.
Connector type: | One receptacle (Type B)
Configuration: |

Element | Description
Device | Full speed mode (12 Mbit/s) Vendor ID: 04B8h Product ID: 011Dh USB Rev.: 1.1 Class: Vendor-specific
Configuration | Self-powered Remote wake up feature: Not supported Maximum power consumption from VBUS: 2 mA (5 V)
Interface | No alternate setting Class: Vendor-specific
Endpoint | Maximum packet size Bulk in: 64 byte Bulk out: 64 byte
String | Language ID: US, English 1: Manufacturer: "EPSON" 2: Product: "EPSON Scanner"

[Top]

## Perfection 1660 Photo

Interface type: | Universal Serial Bus Specification Revision 2.0
Electrical standard: | Full speed mode and Hi-speed mode of Universal Serial Bus Specification Revision 2.0.
Connector type: | One receptacle (Type B)
Configuration: |

Element | Description
Device | Full speed mode (12 Mbit/s) and Hi-speed mode (480 Mbit/s) Vendor ID: 04B8h Product ID: 011Eh USB Rev.: 2.0 Class: Vendor-specific
Configuration | Self-powered Remote wake up feature: Not supported Maximum power consumption from VBUS: 2 mA (5 V)
Interface | No alternate setting Class: Vendor- specific
Endpoint | Maximum packet size Bulk in: 64 byte (Full speed mode), 512 byte (Hi-speed mode) Bulk out: 64 byte (Full speed mode), 512 byte (Hi-speed mode)
String | Language ID: US, English 1: Manufacturer: "EPSON" 2: Product: "EPSON Scanner"

[Top]

## Perfection 2400 Photo

Interface type: | Universal Serial Bus Specification Revision 2.0
Electrical standard: | Full speed mode and Hi-speed mode of Universal Serial Bus Specification Revision 2.0.
Connector type: | One receptacle (Type B)
Configuration: |

Element | Description
Device | Full speed mode (12 Mbit/s) and Hi-speed mode (480 Mbit/s) Vendor ID: 04B8h Product ID: 011Ch USB Rev.: 2.0 Class: Vendor-specific
Configuration | Self-powered Remote wake up feature: Not supported Maximum power consumption from VBUS: 2 mA (5 V)
Interface | No alternate setting Class: Vendor- specific
Endpoint | Maximum packet size Bulk in: 64 byte (Full speed mode), 512 byte (Hi-speed mode) Bulk out: 64 byte (Full speed mode), 512 byte (Hi-speed mode)
String | Language ID: US, English 1: Manufacturer: "EPSON" 2: Product: "EPSON Scanner"

[Top]

Previous | Next