Technical Specifications

# Film Adapter (Option)

> For the Perfection 1260 and 1260 Photo
> For the Perfection 1660 Photo and 2400 Photo

## For the Perfection 1260 and 1260 Photo

This product conforms to CE marking requirements in accordance with EC Directive 89/336/EEC.

Model: | EU-52
Electrical Specifications:

> Supplied Voltage:

DC 15.2 V

> Rated current:

0.2 A

Environmental Conditions:

> Temperature

Operation: 5 to 35°C (41 to 95°F)
Storage: -25 to 60°C (-13 to 140°F)

> Humidity

Operation: 10 to 80%, without condensation
Storage: 10 to 85%, without condensation

Document:

> Transparencies
> up to

35-mm film strip
35-mm slide

Readable area: | 36 x 36 mm
Dimensions: | Width: 88 mm (3.5 inches) Depth: 145 mm (5.7 inches) Height: 56 mm (2.2 inches)
Weight: | Approx. 170 g (0.4 lb)

[Top]

## For the Perfection 1660 Photo and 2400 Photo

Model: | EU-33
Electrical Specifications:

> Supplied Voltage:

DC 24V

> Rated current:

0.5 A

Environmental Conditions:

> Temperature

Operation: 5 to 35°C (41 to 95°F)
Storage: -25 to 60°C (-13 to 140°F)

> Humidity

Operation: 10 to 80%, without condensation
Storage: 10 to 85%, without condensation

Document:

> Transparencies
> up to

4 x 5 inch film
35-mm film strip
35-mm slide
120/220 size (6 x 9 cm) film strip

Manuscript: | Up to 4 x 5 inches film size
Readable area: | 93 x 118 mm
Dimensions: | Width: 222 mm (8.7 inches) Depth: 305 mm (12.0 inches) Height: 36 mm (1.4 inches)
Weight: | Approx. 700 g (1.5 lb)

[Top]

Previous