Technical Specifications

# Initialization Methods

The scanner can be initialized (returned to a fixed set of conditions) in the following ways:

Hardware initialization | The scanner is plugged in. The USB cable is unplugged from the USB port on the scanner.
Software initialization | Software sends the ESC @ (initialize the scanner) command. The scanner receives a Bus Reset from the USB interface.

[Top]

Previous | Next