Maintenance

# Replacing the Fluorescent Lamp

The luminosity of the fluorescent lamp declines over time. If the lamp breaks or becomes too dim to operate normally, the scanner stops working and the Start button turns red (for Perfection 1260 and 1260 Photo users) or flashes red (for Perfection 1660 Photo and 2400 Photo users). When this happens, the lamp assembly must be replaced. For details, contact your dealer.

| Caution:

| Never open the case of the scanner. If you think repairs or adjustments are necessary, consult your dealer.

[Top]

Previous | Next