Technical Specifications

# Scanning

> Perfection 1260 and 1260 Photo
> Perfection 1660 Photo
> Perfection 2400 Photo

## Perfection 1260 and 1260 Photo

Scanner type | Flatbed, color
Photoelectric device | Color CCD line sensor
Effective pixels | 10200 x 14040 pixels at 1200 dpi, 100%
Document size | 216 x 297 mm (8.5 x 11.7 inches) A4 or US letter size (The reading area can be specified from your software.)
Scanning resolution | 1200 dpi (main scan) 2400 dpi with Micro Step (sub scan)
Output resolution | 50 to 9600 dpi (50 to 4800 dpi in 1 dpi increments, 7200 dpi, and 9600 dpi.)
Image data | 16 bits per pixel per color internal 8 bits per pixel per color external
Line Art settings | Fixed threshold
Gamma correction | 1 type for user-defined
Color correction | 1 type for CRT display 3 types for printer output 1 type for user-defined (Only user-defined Color correction is available in EPSON TWAIN)
Interface | USB (Type B Receptacle Connector)
Light source | White cold cathode fluorescent lamp
Reliability | 10,000 cycles of carriage movements (main unit MCBF)
Dimensions | Width: 278 mm (10.9 inches) Depth: 438 mm (17.2 inches) Height: 67 mm (2.6 inches)
Weight | Approx. 2.5 kg (5.5 lb)

[Top]

## Perfection 1660 Photo

Scanner type | Flatbed, color
Photoelectric device | Color CCD line sensor
Effective pixels | 13600 x 18720 pixels at 1600 dpi, 100%
Document size | 216 x 297 mm (8.5 x 11.7 inches) A4 or US letter size (The reading area can be specified from your software.)
Scanning resolution | 1600 dpi (main scan) 3200 dpi with Micro Step (sub scan)
Output resolution | 50 to 12800 dpi (50 to 6400 dpi in 1 dpi increments, 12,800 dpi performed with zoom function)
Color separation | RGB color filters on CCD
Zoom | 50 to 200% in 1% increments
Image data | 16 bits per pixel per color internal 1 to 16 bits per pixel per color external
Brightness | 7 levels (In EPSON TWAIN, Gamma correction controls Brightness)
Line Art settings | Fixed threshold Text Enhancement Technology (enable/disable selectable)
Halftoning process | AAS (Auto Area Segmentation) Enable/disable selectable 3 halftoning modes (A, B, and C) and 4 dither patterns (A, B, C, and D) for bi-level and quad-level data
(2 downloadable dither patterns)

Gamma correction | 2 types for CRT display 3 types for printer 1 type for user-defined
Color correction | 1 type for CRT display 3 types for printer output 1 type for user-defined (Only user-defined Color correction is available in EPSON TWAIN)
Interface | USB (Type B Receptacle Connector)
Light source | White cold cathode fluorescent lamp
Reliability | 30,000 cycles of carriage movements (main unit MCBF)
Dimensions | Width: 276 mm (10.9 inches) Depth: 450 mm (17.7 inches) Height: 116mm (4.6 inches)
Weight | Approx. 3.1 kg (6.8 lb)

[Top]

## Perfection 2400 Photo

Scanner type | Flatbed, color
Photoelectric device | Color CCD line sensor
Effective pixels | 20,400 x 28,080 pixels at 2400 dpi, 100%
Document size | 216 x 297 mm (8.5 x 11.7 inches) A4 or US letter size (The reading area can be specified from your software.)
Scanning resolution | 2400 dpi (main scan) 4800 dpi with Micro Step (sub scan)
Output resolution | 50 to 12,800 dpi (50 to 6,400 dpi in 1 dpi increments, 12,800 dpi performed with zoom function)
Color separation | RGB color filters on CCD
Zoom | 50 to 200% in 1% increments
Image data | 16 bits per pixel per color internal 1 to 16 bits per pixel per color external
Brightness | 7 levels (In EPSON TWAIN, Gamma correction controls Brightness)
Line Art settings | Fixed threshold Text Enhancement Technology (enable/disable selectable)
Halftoning process | AAS (Auto Area Segmentation) Enable/disable selectable 3 halftoning modes (A, B, and C) and 4 dither patterns (A, B, C, and D) for bi-level and quad-level data
(2 downloadable dither patterns)

Gamma correction | 2 types for CRT display 3 types for printer 1 type for user-defined
Color correction | 1 type for CRT display 3 types for printer output 1 type for user-defined (Only user-defined Color correction is available in EPSON TWAIN)
Interface | USB (Type B Receptacle Connector)
Light source | White cold cathode fluorescent lamp
Reliability | 30,000 cycles of carriage movements (main unit MCBF)
Dimensions | Width: 276 mm (10.9 inches) Depth: 450 mm (17.7 inches) Height: 116 mm (4.6 inches)
Weight | Approx. 3.1 kg (6.8 lb)

[Top]

Previous | Next