Microchip Technology Inc, vv1.24 (0)

Tool Name:
  c:\program files (x86)\microchip\xc16\v1.24\bin\bin\..\bin/elf-ld.exe

Command:
  -p33EP512MU810 \
  -o \
  dist/XC16_dsPIC33EP512MU810/debug/PLCD_P01V49.debug.elf \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/.. \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/PIC24E \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/PIC24E/gld \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/PIC24F \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/PIC24F/gld \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/PIC24H \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/PIC24H/gld \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC30F \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/dsPIC30F/gld \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/dsPIC33E/gld \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33F \
  -Lc:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../support/dsPIC33F/gld \
  build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o \
  build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o \
  build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o \
  build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o \
  build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o \
  build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o \
  build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o \
  build/XC16_dsPIC33EP512MU810/debug/Regul.o \
  build/XC16_dsPIC33EP512MU810/debug/Pesage.o \
  build/XC16_dsPIC33EP512MU810/debug/Process.o \
  build/XC16_dsPIC33EP512MU810/debug/BdC.o \
  build/XC16_dsPIC33EP512MU810/debug/Depeseur.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o \
  build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o \
  build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o \
  build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o \
  build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o \
  build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o \
  build/XC16_dsPIC33EP512MU810/debug/interrupts.o \
  build/XC16_dsPIC33EP512MU810/debug/main.o \
  build/XC16_dsPIC33EP512MU810/debug/system.o \
  build/XC16_dsPIC33EP512MU810/debug/traps.o \
  build/XC16_dsPIC33EP512MU810/debug/user.o \
  build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o \
  build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o \
  build/XC16_dsPIC33EP512MU810/debug/AD7190.o \
  build/XC16_dsPIC33EP512MU810/debug/ADComm.o \
  build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o \
  build/XC16_dsPIC33EP512MU810/debug/MemFlash.o \
  build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o \
  build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o \
  build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o \
  build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.00 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.01 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.02 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.03 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.04 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.05 \
  -TC:\Users\David_2\AppData\Local\Temp\tmp000004ac.06 \
  --local-stack \
  --defsym=__MPLAB_BUILD=1 \
  --defsym=__MPLAB_DEBUG=1 \
  --defsym=__DEBUG=1 \
  --defsym=__MPLAB_DEBUGGER_PK3=1 \
  -Tp33EP512MU810.gld.07 \
  --stack=16 \
  --check-sections \
  --data-init \
  --pack-data \
  --handles \
  --isr \
  --no-gc-sections \
  --fill-upper=0 \
  --stackguard=16 \
  --no-force-link \
  --smart-io \
  -Map=dist/XC16_dsPIC33EP512MU810/debug/PLCD_P01V49.debug.map \
  --report-mem \
  -start-group \
  --library=pic30-elf \
  --library=m-elf \
  --library=c-elf \
  -end-group \

Archive member included because of file (symbol)

c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI1.o)
                              build/XC16_dsPIC33EP512MU810/debug/ADComm.o (_CloseSPI1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI3.o)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o (_CloseSPI3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI1.o)
                              build/XC16_dsPIC33EP512MU810/debug/ADComm.o (_DataRdySPI1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI3.o)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o (_DataRdySPI3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI1.o)
                              build/XC16_dsPIC33EP512MU810/debug/ADComm.o (_OpenSPI1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI3.o)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o (_OpenSPI3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI1.o)
                              build/XC16_dsPIC33EP512MU810/debug/ADComm.o (_ReadSPI1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI3.o)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o (_ReadSPI3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI1.o)
                              build/XC16_dsPIC33EP512MU810/debug/ADComm.o (_WriteSPI1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI3.o)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o (_WriteSPI3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/main.o (_BusyUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (_BusyUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (_BusyUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_CloseUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_CloseUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_CloseUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_CloseUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_ConfigIntUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_ConfigIntUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_ConfigIntUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_ConfigIntUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_DataRdyUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_DataRdyUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_DataRdyUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_DataRdyUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_OpenUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_OpenUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_OpenUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o (_OpenUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/main.o (_putsUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (_putsUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/main.o (_putsUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/main.o (_putsUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART1.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_ReadUART1)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART2.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_ReadUART2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART3.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_ReadUART3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART4.o)
                              build/XC16_dsPIC33EP512MU810/debug/interrupts.o (_ReadUART4)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(crt0_extendedep.o)
                              (__resetPRI)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(data_init_extendedep.o)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(crt0_extendedep.o) (__data_init_extended)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (___subsf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsf3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (___divsf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsi3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Pesage.o (___divsi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(feqltle.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Pesage.o (___eqsf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fgtge.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o (___gtsf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixsfsi.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (_(float, int, long long, short, float, short, int))
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunssfsi.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (___fixunssfsi)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatsisf.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Pesage.o (___floatsisf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsisf.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (___floatunsisf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fpack.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo) (__fpack)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixsfsi.epeo) (__funpack)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack2.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo) (__funpack2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(futil.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo) (__fPropagateNaN)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsf3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Regul.o (___mulsf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(udivsi3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o (___udivsi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umodsi3.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o (___umodsi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fcompare.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(feqltle.epeo) (__fcompare)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatdisf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatsisf.epeo) (___floatdisf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundisf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsisf.epeo) (___floatundisf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o (_atof)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atoi.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/user.o (_atoi)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atol.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o (_atol)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(errno.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo) (_errno)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(ltoa.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o (_ltoa)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcmp.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o (_memcmp)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcpy.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o (_memcpy)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memset.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o (_memset)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o (_srand)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (_sprintf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcmp.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o (_strcmp)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcpy.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/user.o (_strcpy)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strlen.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o (_strlen)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strncpy.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o (_strncpy)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/user.o (_strtok)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(putchar.epeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o (_putchar)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(putchar.epeo) (__iob)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdnopuxX.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (__sprintf_cdnopuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdnopuxX.EPeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdnopuxX.EPeo) (__vfprintf_cdnopuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_cdnopuxX.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o (__printf_cdnopuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdfFnopsuxX.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/Process.o (__sprintf_cdfFnopsuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdfFnopsuxX.EPeo) (__vfprintf_cdfFnopsuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdnopsuxX.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/user.o (__sprintf_cdnopsuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdnopsuxX.EPeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdnopsuxX.EPeo) (__vfprintf_cdnopsuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_cdnopsuxX.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o (__printf_cdnopsuxX)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_s.EPeo)
                              build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o (__printf_0)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(isspace.epeso)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo) (_isspace)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf.epeo) (_vfprintf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(fputc.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(putchar.epeo) (_fputc)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(powers.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (__powers_)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcspn.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo) (_strcspn)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strspn.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo) (_strspn)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strchr.epelo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcspn.epeo) (_strchr)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_s.EPeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_s.EPeo) (__vfprintf_s)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(flsbuf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(fputc.epeo) (__flsbuf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(writeep.eo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(fputc.epeo) (_write)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(adddf3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___adddf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(deqltle.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___ltdf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dgtge.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___gedf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divdf3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___divdf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dne.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___nedf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpack.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(adddf3.epeo) (__dpack)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack2.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(adddf3.epeo) (__dunpack2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(extendsfdf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___extendsfdf2)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfdi.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___fixunsdfdi)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfsi.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo) (___fixunsdfsi)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundidf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___floatundidf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsidf.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo) (___floatunsidf)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(frexp.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (_frexpl)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldf3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___muldf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(subdf3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo) (___subdf3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsi3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo) (___mulsi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdnopuxX.EPeo) (___udivdi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldi3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdnopuxX.EPeo) (___muldi3)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dcompare.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(deqltle.epeo) (__dcompare)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpropagateNaN.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack2.epeo) (__dPropagateNaN)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dtype.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dcompare.epeo) (__dtype)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack2.epeo) (__dunpack)
c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umuldi3.epeo)
                              c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldi3.epeo) (___umuldi3)


Program Memory  [Origin = 0x200, Length = 0x555fe]

section                    address   length (PC units)   length (bytes) (dec)
-------                    -------   -----------------   --------------------
.text                        0x200              0x3ea4          0x5df6  (24054)
.const                      0x40a4              0x16a6          0x21f9  (8697)
.text                       0x574a              0x63f0          0x95e8  (38376)
MPFSData                    0xbb3a              0x51ea          0x7adf  (31455)
.text                      0x10d24             0x13c7c         0x1daba  (121530)
.dinit                     0x249a0               0x4fa           0x777  (1911)
.text                      0x24e9a              0x4932          0x6dcb  (28107)
MPFSHelpers                0x297cc                 0xe            0x15  (21)

                     Total program memory used (bytes):        0x3e0c7  (254151) 48%


Auxflash Memory  [Origin = 0x7fc000, Length = 0x3ff8]

section                    address   length (PC units)   length (bytes) (dec)
-------                    -------   -----------------   --------------------

                     Total auxflash memory used (bytes):              0  (0) <1%


Data Memory  [Origin = 0x1000, Length = 0xd000]

section                    address      alignment gaps    total length  (dec)
-------                    -------      --------------    -------------------
reserve_data_0x1000         0x1000                0x1c            0x1c  (28)
reserve_data_0x101c         0x101c                 0x2             0x2  (2)
reserve_data_0x101e         0x101e                 0x2             0x2  (2)
reserve_data_0x1020         0x1020                 0x2             0x2  (2)
reserve_data_0x1022         0x1022                 0x2             0x2  (2)
reserve_data_0x1024         0x1024                 0x4             0x4  (4)
reserve_data_0x1028         0x1028                0x28            0x28  (40)
.bss                        0x1050                   0          0x208e  (8334)
.data._powers_              0x30de                   0            0xb0  (176)
.data._npowers_             0x318e                   0            0xb0  (176)
.bss                        0x323e                   0            0xac  (172)
.data.dpowers               0x32ea                   0           0x140  (320)
.bss                        0x342a                   0            0xfc  (252)
.bss                        0x3526                   0            0x94  (148)
.data                       0x35ba                   0            0x2a  (42)
.bss                        0x35e4                   0            0x18  (24)
.bss                        0x35fc                   0             0x4  (4)
_04CAD60056823d9e           0x3600                   0            0x60  (96)
.bss                        0x3660                   0            0xe6  (230)
.bss                        0x3746                   0            0x8c  (140)
.data                       0x37d2                   0            0x70  (112)
.bss                        0x3842                   0            0x6c  (108)
.data                       0x38ae                   0            0x66  (102)
.bss                        0x3914                   0            0x9a  (154)
.data                       0x39ae                   0            0x2a  (42)
.bss                        0x39d8                   0            0x24  (36)
.data._iob                  0x39fc                   0            0x24  (36)
.bss                        0x3a20                   0            0x68  (104)
.data                       0x3a88                   0            0x74  (116)
.bss                        0x3afc                   0            0x90  (144)
.data                       0x3b8c                   0            0x10  (16)
.bss                        0x3b9c                   0            0x28  (40)
.data                       0x3bc4                   0             0x6  (6)
.bss                        0x3bca                   0             0xc  (12)
_04E28D2056823d9b           0x3bd6                   0             0x6  (6)
.bss                        0x3bdc                   0             0x6  (6)
.bss                        0x3be2                   0             0x4  (4)
.data                       0x3be6                   0             0x8  (8)
.bss                        0x3bee                   0             0xc  (12)
.data                       0x3bfa                   0             0x4  (4)
.bss                        0x3bfe                   0             0x8  (8)
.bss.randx                  0x3c06                   0             0x4  (4)
.bss                        0x3c0a                   0             0x2  (2)
.data                       0x3c0c                   0             0x8  (8)
.pbss                       0x3c14                   0             0x2  (2)
.data                       0x3c16                   0             0x4  (4)
.pbss                       0x3c1a                   0             0x2  (2)
.data                       0x3c1c                   0             0x2  (2)
.pbss                       0x3c1e                   0             0x2  (2)
.bss                        0x3c20                   0             0x4  (4)
.bss.errno                  0x3c24                   0             0x2  (2)
.bss.randf                  0x3c26                   0             0x2  (2)
.bss.sp.1310                0x3c28                   0             0x2  (2)
.data._Files                0x3c2a                   0             0x2  (2)
.bss._outdone               0x3c2c                   0             0x2  (2)
.bss._sibuf                 0x3c2e                   0             0x2  (2)
.bss._sobuf                 0x3c30                   0             0x2  (2)
_04789A2056823da3           0xd800                   0           0x210  (528)
_047D678056823d8b           0xdb00                   0             0xe  (14)
_0478984056823da3           0xdc00                   0           0x210  (528)
_047D69C056823d8b           0xdf00                   0            0x80  (128)

                        Total data memory used (bytes):         0x30e0  (12512) 23%


Dynamic Memory Usage

region                     address                      maximum length  (dec)
------                     -------                      ---------------------
heap                             0                                   0  (0)
stack                       0x3c32                              0x43ce  (17358)

                        Maximum dynamic memory (bytes):         0x43ce  (17358)


External Symbols in Data Memory (by address):

                    0x1050                  _PAR
                    0x1452                  _EXP
                    0x18d8                  _sorTOR
                    0x18e2                  _entTOR
                    0x18ec                  _Cav_USR1
                    0x18ee                  _Cav_CLR
                    0x18f0                  _T100
                    0x192c                  _T10
                    0x1940                  _AD7190_PoidsPret
                    0x1942                  _Compteur
                    0x1944                  _NbTopTotal
                    0x1948                  _CompteurTot
                    0x194c                  _entreeTorVitesseMem
                    0x1956                  _U1Baudvalue
                    0x1958                  _U2Baudvalue
                    0x195a                  _U3Baudvalue
                    0x195c                  _U4Baudvalue
                    0x195e                  _U1MODEvalue
                    0x1960                  _U1STAvalue
                    0x1962                  _U2MODEvalue
                    0x1964                  _U2STAvalue
                    0x1966                  _U3MODEvalue
                    0x1968                  _U3STAvalue
                    0x196a                  _U4MODEvalue
                    0x196c                  _U4STAvalue
                    0x196e                  _TrameU1
                    0x1b70                  _TrameU2
                    0x1d72                  _TrameU3
                    0x1f74                  _TrameU4
                    0x2606                  _link_bPool
                    0x2a72                  _MODBUS_COMMAND
                    0x2a7e                  _WriteByteReverse
                    0x2a80                  _MODBUS_RX
                    0x2c80                  _MODBUS_TX
                    0x2e80                  _COIL
                    0x2e82                  _COIL_REG
                    0x2fcc                  _USB_In_Buffer
                    0x300c                  _USB_Mess_head
                    0x300e                  _USB_Mess
                    0x30da                  _USB_list_count
                    0x30de                  __powers_
                    0x318e                  __npowers_
                    0x323e                  _cdc_data_tx
                    0x327e                  _cdc_data_rx
                    0x32be                  _line_coding
                    0x32c6                  _cdc_notice
                    0x32d0                  _cdc_rx_len
                    0x32d1                  _cdc_trf_state
                    0x32d2                  _pCDCSrc
                    0x32d4                  _pCDCDst
                    0x32d6                  _cdc_tx_len
                    0x32d7                  _cdc_mem_type
                    0x32d8                  _CDCDataOutHandle
                    0x32da                  _CDCDataInHandle
                    0x32dc                  _control_signal_bitmap
                    0x32de                  _BaudRateGen
                    0x32e2                  _dummy_encapsulated_cmd_response
                    0x342a                  _UDPSocketInfo
                    0x351a                  _activeUDPSocket
                    0x351c                  _UDPTxCount
                    0x351e                  _UDPRxCount
                    0x3600                  _BDT
                    0x3660                  _AD_asDefaultMap
                    0x3662                  _AD_asADIEntryList
                    0x3746                  _curHTTP
                    0x37c8                  _httpStubs
                    0x37d0                  _curHTTPID
                    0x38ae                  _ReadByteReverse
                    0x38af                  _InputByteReverse
                    0x38b0                  _HOLDING_REG
                    0x38e2                  _INPUT_REG
                    0x3914                  _fResetABCC
                    0x3916                  _ABCCPowerState
                    0x3918                  _address
                    0x391c                  _AppConfig
                    0x3964                  _USBDeviceState
                    0x3966                  _USBActiveConfiguration
                    0x3967                  _USBAlternateInterface
                    0x396a                  _pBDTEntryEP0OutCurrent
                    0x396c                  _pBDTEntryEP0OutNext
                    0x396e                  _pBDTEntryOut
                    0x3974                  _pBDTEntryIn
                    0x397a                  _shortPacketStatus
                    0x397b                  _controlTransferState
                    0x397c                  _inPipes
                    0x3982                  _outPipes
                    0x398a                  _pDst
                    0x398c                  _RemoteWakeup
                    0x398d                  _USBBusIsSuspended
                    0x398e                  _USTATcopy
                    0x398f                  _endpoint_number
                    0x3990                  _BothEP0OutUOWNsSet
                    0x3991                  _ep_data_in
                    0x3994                  _ep_data_out
                    0x3997                  _USBStatusStageTimeoutCounter
                    0x3998                  _USBDeferStatusStagePacket
                    0x3999                  _USBStatusStageEnabledFlag1
                    0x399a                  _USBStatusStageEnabledFlag2
                    0x399b                  _USBDeferINDataStagePackets
                    0x399c                  _USBDeferOUTDataStagePackets
                    0x399d                  _SetupPkt
                    0x39a5                  _CtrlTrfData
                    0x39fc                  __iob
                    0x3afc                  _ABCC_RunDriver
                    0x3afe                  _ABCC_ISR
                    0x3b00                  _pnABCC_DrvInit
                    0x3b02                  _pnABCC_DrvISR
                    0x3b04                  _pnABCC_DrvRunDriverTx
                    0x3b06                  _pnABCC_DrvRunDriverRx
                    0x3b08                  _pnABCC_DrvWriteMessage
                    0x3b0a                  _pnABCC_DrvWriteProcessData
                    0x3b0c                  _pnABCC_DrvISReadyForWrPd
                    0x3b0e                  _pnABCC_DrvISReadyForWriteMessage
                    0x3b10                  _pnABCC_DrvISReadyForCmd
                    0x3b12                  _pnABCC_DrvSetNbrOfCmds
                    0x3b14                  _pnABCC_DrvSetAppStatus
                    0x3b16                  _pnABCC_DrvSetPdSize
                    0x3b18                  _pnABCC_DrvSetMsgReceiverBuffer
                    0x3b1a                  _pnABCC_DrvSetIntMask
                    0x3b1c                  _pnABCC_DrvGetWrPdBuffer
                    0x3b1e                  _pnABCC_DrvGetModCap
                    0x3b20                  _pnABCC_DrvGetLedStatus
                    0x3b22                  _pnABCC_DrvGetIntStatus
                    0x3b24                  _pnABCC_DrvGetAnybusState
                    0x3b26                  _pnABCC_DrvReadProcessData
                    0x3b28                  _pnABCC_DrvReadMessage
                    0x3b2a                  _pnABCC_DrvIsSupervised
                    0x3b2c                  _pnABCC_DrvGetAnbStatus
                    0x3b3a                  _ADI_DebitInstan
                    0x3b3e                  _ADI_PoidsInstan
                    0x3b42                  _ADI_PoidsMetre
                    0x3b46                  _ADI_Vitesse
                    0x3b4a                  _ADI_TotalPartiel
                    0x3b4e                  _ADI_TotalGlobal
                    0x3b52                  _ADI_Tare
                    0x3b56                  _ADI_EtatBascule
                    0x3b5a                  _ADI_CmdsBascule
                    0x3b5e                  _ADI_DigitalInput
                    0x3b5f                  _ADI_DigitalOutput
                    0x3b9e                  _remoteNode
                    0x3baa                  _receivedECANmsg
                    0x3bac                  _transmitNextECANmsg
                    0x3bae                  _sentPacketECANMSG
                    0x3bb0                  _rxECANIndex
                    0x3bb2                  _txECANBufferIndex
                    0x3bb4                  _SPI3CON1Value
                    0x3bb6                  _SPI3CON2Value
                    0x3bb8                  _SPI3STATValue
                    0x3bc4                  _app_aacLanguages
                    0x3bc6                  _app_sInstance
                    0x3bca                  _us_bSwitch1
                    0x3bcb                  _us_bSwitch2
                    0x3bcc                  _us_fSwitch1Set
                    0x3bcd                  _us_fSwitch2Set
                    0x3bdc                  _SPICON1Value
                    0x3bde                  _SPICON2Value
                    0x3be0                  _SPISTATValue
                    0x3bfa                  _ABCC_StateMachineEnabled
                    0x3bfc                  ___C30_UART
                    0x3c02                  _Nb_Octets_Log
                    0x3c04                  _Address_Log_L
                    0x3c05                  _Address_Log_B
                    0x3c0a                  _ErrorReporter
                    0x3c0c                  _dpv_sInstance
                    0x3c0e                  _rxECANBufferIndex
                    0x3c10                  _Demarrage1er
                    0x3c20                  _DmaBufferSwitch
                    0x3c24                  _errno
                    0x3c2a                  __Files
                    0x3c2c                  __outdone
                    0x3c2e                  __sibuf
                    0x3c30                  __sobuf
                    0xd800                  _BufferB
                    0xdb00                  _ecanTxMsgBuffer
                    0xdc00                  _BufferA
                    0xdf00                  _ecanRxMsgBuffer

External Symbols in Data Memory (by name):

                    0x3916                  _ABCCPowerState
                    0x3afe                  _ABCC_ISR
                    0x3afc                  _ABCC_RunDriver
                    0x3bfa                  _ABCC_StateMachineEnabled
                    0x1940                  _AD7190_PoidsPret
                    0x3b5a                  _ADI_CmdsBascule
                    0x3b3a                  _ADI_DebitInstan
                    0x3b5e                  _ADI_DigitalInput
                    0x3b5f                  _ADI_DigitalOutput
                    0x3b56                  _ADI_EtatBascule
                    0x3b3e                  _ADI_PoidsInstan
                    0x3b42                  _ADI_PoidsMetre
                    0x3b52                  _ADI_Tare
                    0x3b4e                  _ADI_TotalGlobal
                    0x3b4a                  _ADI_TotalPartiel
                    0x3b46                  _ADI_Vitesse
                    0x3662                  _AD_asADIEntryList
                    0x3660                  _AD_asDefaultMap
                    0x3c05                  _Address_Log_B
                    0x3c04                  _Address_Log_L
                    0x391c                  _AppConfig
                    0x3600                  _BDT
                    0x32de                  _BaudRateGen
                    0x3990                  _BothEP0OutUOWNsSet
                    0xdc00                  _BufferA
                    0xd800                  _BufferB
                    0x32da                  _CDCDataInHandle
                    0x32d8                  _CDCDataOutHandle
                    0x2e80                  _COIL
                    0x2e82                  _COIL_REG
                    0x18ee                  _Cav_CLR
                    0x18ec                  _Cav_USR1
                    0x1942                  _Compteur
                    0x1948                  _CompteurTot
                    0x39a5                  _CtrlTrfData
                    0x3c10                  _Demarrage1er
                    0x3c20                  _DmaBufferSwitch
                    0x1452                  _EXP
                    0x3c0a                  _ErrorReporter
                    0x38b0                  _HOLDING_REG
                    0x38e2                  _INPUT_REG
                    0x38af                  _InputByteReverse
                    0x2a72                  _MODBUS_COMMAND
                    0x2a80                  _MODBUS_RX
                    0x2c80                  _MODBUS_TX
                    0x1944                  _NbTopTotal
                    0x3c02                  _Nb_Octets_Log
                    0x1050                  _PAR
                    0x38ae                  _ReadByteReverse
                    0x398c                  _RemoteWakeup
                    0x3bb4                  _SPI3CON1Value
                    0x3bb6                  _SPI3CON2Value
                    0x3bb8                  _SPI3STATValue
                    0x3bdc                  _SPICON1Value
                    0x3bde                  _SPICON2Value
                    0x3be0                  _SPISTATValue
                    0x399d                  _SetupPkt
                    0x192c                  _T10
                    0x18f0                  _T100
                    0x196e                  _TrameU1
                    0x1b70                  _TrameU2
                    0x1d72                  _TrameU3
                    0x1f74                  _TrameU4
                    0x1956                  _U1Baudvalue
                    0x195e                  _U1MODEvalue
                    0x1960                  _U1STAvalue
                    0x1958                  _U2Baudvalue
                    0x1962                  _U2MODEvalue
                    0x1964                  _U2STAvalue
                    0x195a                  _U3Baudvalue
                    0x1966                  _U3MODEvalue
                    0x1968                  _U3STAvalue
                    0x195c                  _U4Baudvalue
                    0x196a                  _U4MODEvalue
                    0x196c                  _U4STAvalue
                    0x351e                  _UDPRxCount
                    0x342a                  _UDPSocketInfo
                    0x351c                  _UDPTxCount
                    0x3966                  _USBActiveConfiguration
                    0x3967                  _USBAlternateInterface
                    0x398d                  _USBBusIsSuspended
                    0x399b                  _USBDeferINDataStagePackets
                    0x399c                  _USBDeferOUTDataStagePackets
                    0x3998                  _USBDeferStatusStagePacket
                    0x3964                  _USBDeviceState
                    0x3999                  _USBStatusStageEnabledFlag1
                    0x399a                  _USBStatusStageEnabledFlag2
                    0x3997                  _USBStatusStageTimeoutCounter
                    0x2fcc                  _USB_In_Buffer
                    0x300e                  _USB_Mess
                    0x300c                  _USB_Mess_head
                    0x30da                  _USB_list_count
                    0x398e                  _USTATcopy
                    0x2a7e                  _WriteByteReverse
                    0x3c2a                  __Files
                    0x3bfc                  ___C30_UART
                    0x39fc                  __iob
                    0x318e                  __npowers_
                    0x3c2c                  __outdone
                    0x30de                  __powers_
                    0x3c2e                  __sibuf
                    0x3c30                  __sobuf
                    0x351a                  _activeUDPSocket
                    0x3918                  _address
                    0x3bc4                  _app_aacLanguages
                    0x3bc6                  _app_sInstance
                    0x327e                  _cdc_data_rx
                    0x323e                  _cdc_data_tx
                    0x32d7                  _cdc_mem_type
                    0x32c6                  _cdc_notice
                    0x32d0                  _cdc_rx_len
                    0x32d1                  _cdc_trf_state
                    0x32d6                  _cdc_tx_len
                    0x397b                  _controlTransferState
                    0x32dc                  _control_signal_bitmap
                    0x3746                  _curHTTP
                    0x37d0                  _curHTTPID
                    0x3c0c                  _dpv_sInstance
                    0x32e2                  _dummy_encapsulated_cmd_response
                    0xdf00                  _ecanRxMsgBuffer
                    0xdb00                  _ecanTxMsgBuffer
                    0x398f                  _endpoint_number
                    0x18e2                  _entTOR
                    0x194c                  _entreeTorVitesseMem
                    0x3991                  _ep_data_in
                    0x3994                  _ep_data_out
                    0x3c24                  _errno
                    0x3914                  _fResetABCC
                    0x37c8                  _httpStubs
                    0x397c                  _inPipes
                    0x32be                  _line_coding
                    0x2606                  _link_bPool
                    0x3982                  _outPipes
                    0x396a                  _pBDTEntryEP0OutCurrent
                    0x396c                  _pBDTEntryEP0OutNext
                    0x3974                  _pBDTEntryIn
                    0x396e                  _pBDTEntryOut
                    0x32d4                  _pCDCDst
                    0x32d2                  _pCDCSrc
                    0x398a                  _pDst
                    0x3b2c                  _pnABCC_DrvGetAnbStatus
                    0x3b24                  _pnABCC_DrvGetAnybusState
                    0x3b22                  _pnABCC_DrvGetIntStatus
                    0x3b20                  _pnABCC_DrvGetLedStatus
                    0x3b1e                  _pnABCC_DrvGetModCap
                    0x3b1c                  _pnABCC_DrvGetWrPdBuffer
                    0x3b02                  _pnABCC_DrvISR
                    0x3b10                  _pnABCC_DrvISReadyForCmd
                    0x3b0c                  _pnABCC_DrvISReadyForWrPd
                    0x3b0e                  _pnABCC_DrvISReadyForWriteMessage
                    0x3b00                  _pnABCC_DrvInit
                    0x3b2a                  _pnABCC_DrvIsSupervised
                    0x3b28                  _pnABCC_DrvReadMessage
                    0x3b26                  _pnABCC_DrvReadProcessData
                    0x3b06                  _pnABCC_DrvRunDriverRx
                    0x3b04                  _pnABCC_DrvRunDriverTx
                    0x3b14                  _pnABCC_DrvSetAppStatus
                    0x3b1a                  _pnABCC_DrvSetIntMask
                    0x3b18                  _pnABCC_DrvSetMsgReceiverBuffer
                    0x3b12                  _pnABCC_DrvSetNbrOfCmds
                    0x3b16                  _pnABCC_DrvSetPdSize
                    0x3b08                  _pnABCC_DrvWriteMessage
                    0x3b0a                  _pnABCC_DrvWriteProcessData
                    0x3baa                  _receivedECANmsg
                    0x3b9e                  _remoteNode
                    0x3c0e                  _rxECANBufferIndex
                    0x3bb0                  _rxECANIndex
                    0x3bae                  _sentPacketECANMSG
                    0x397a                  _shortPacketStatus
                    0x18d8                  _sorTOR
                    0x3bac                  _transmitNextECANmsg
                    0x3bb2                  _txECANBufferIndex
                    0x3bca                  _us_bSwitch1
                    0x3bcb                  _us_bSwitch2
                    0x3bcc                  _us_fSwitch1Set
                    0x3bcd                  _us_fSwitch2Set

External Symbols in Program Memory (by address):

                  0x000200                  __resetPRI
                  0x00022c                  __psv_init
                  0x000238                  __data_init
                  0x000238                  __data_init_extended
                  0x000356                  __U1RXInterrupt
                  0x0003e0                  __U2RXInterrupt
                  0x00046a                  __U3RXInterrupt
                  0x0004f4                  __U4RXInterrupt
                  0x00057e                  __DMA0Interrupt
                  0x000622                  __INT1Interrupt
                  0x00065c                  __INT2Interrupt
                  0x000678                  __INT3Interrupt
                  0x0006be                  __INT4Interrupt
                  0x0006ec                  __USB1Interrupt
                  0x000714                  __C1Interrupt
                  0x000758                  __OscillatorFail
                  0x00075e                  __AddressError
                  0x000764                  __StackError
                  0x00076a                  __MathError
                  0x000770                  __DMACError
                  0x000776                  __DefaultInterrupt
                  0x00077a                  __HardTrapError
                  0x00077e                  __SoftTrapError
                  0x000782                  _isspace
                  0x0007f2                  _CloseSPI1
                  0x0007fe                  _CloseSPI3
                  0x00080a                  _DataRdySPI1
                  0x000814                  _DataRdySPI3
                  0x00081e                  _OpenSPI1
                  0x00082a                  _OpenSPI3
                  0x000836                  _ReadSPI1
                  0x000856                  _ReadSPI3
                  0x000876                  _WriteSPI1
                  0x000888                  _WriteSPI3
                  0x00089a                  _BusyUART2
                  0x0008a8                  _BusyUART3
                  0x0008b6                  _BusyUART4
                  0x0008c4                  _CloseUART1
                  0x0008d4                  _CloseUART2
                  0x0008e4                  _CloseUART3
                  0x0008f4                  _CloseUART4
                  0x000904                  _ConfigIntUART1
                  0x000950                  _ConfigIntUART2
                  0x00099c                  _ConfigIntUART3
                  0x0009e8                  _ConfigIntUART4
                  0x000a30                  _DataRdyUART1
                  0x000a3a                  _DataRdyUART2
                  0x000a44                  _DataRdyUART3
                  0x000a4e                  _DataRdyUART4
                  0x000a58                  _OpenUART1
                  0x000a64                  _OpenUART2
                  0x000a70                  _OpenUART3
                  0x000a7c                  _OpenUART4
                  0x000a88                  _putsUART1
                  0x000ab4                  _putsUART2
                  0x000ae0                  _putsUART3
                  0x000b0c                  _putsUART4
                  0x000b38                  _ReadUART1
                  0x000b4e                  _ReadUART2
                  0x000b64                  _ReadUART3
                  0x000b7a                  _ReadUART4
                  0x000b90                  ___subsf3
                  0x000b92                  ___addsf3
                  0x000c4c                  ___divsf3
                  0x000cd0                  ___divsi3
                  0x000cee                  ___eqsf2
                  0x000cee                  ___lesf2
                  0x000cee                  ___ltsf2
                  0x000cf2                  ___gesf2
                  0x000cf2                  ___gtsf2
                  0x000cf6                  ___fixsfsi
                  0x000d38                  ___fixunssfsi
                  0x000d6e                  ___floatsisf
                  0x000d74                  ___floatunsisf
                  0x000d78                  __fpack
                  0x000dc4                  __funpack
                  0x000dee                  __funpack2
                  0x000dfe                  __fPropagateNaN
                  0x000e10                  __fbopExit
                  0x000e18                  __fbopReturnNaN
                  0x000e1e                  ___mulsf3
                  0x000e86                  ___udivsi3
                  0x000ea6                  ___umodsi3
                  0x000eac                  __fcompare
                  0x000ee2                  ___floatdisf
                  0x000f02                  ___floatundisf
                  0x000f60                  _strtof
                  0x001146                  _strtod
                  0x00114e                  _atof
                  0x001158                  _atoi
                  0x00119a                  _atol
                  0x0011f4                  _ultoa
                  0x001244                  _ltoa
                  0x001268                  _memcmp
                  0x001296                  _memcpy
                  0x0012a8                  _memset
                  0x0012ba                  _srand
                  0x0012cc                  _rand
                  0x0012f8                  _sprintf
                  0x001322                  _strcmp
                  0x001334                  _strcpy
                  0x001344                  _strlen
                  0x001356                  _strncpy
                  0x00137c                  _strtok
                  0x0013be                  _putchar
                  0x0013c8                  __sprintf_cdnopsuxX
                  0x0013c8                  __sprintf_cdfFnopsuxX
                  0x0013c8                  __sprintf_cdnopuxX
                  0x001554                  __vfprintf_cdnopsuxX
                  0x001554                  __vfprintf_0
                  0x001554                  __vfprintf_s
                  0x001554                  __vfprintf_cdnopuxX
                  0x001554                  __vfprintf_cdfFnopsuxX
                  0x0021a2                  __printf_0
                  0x0021a2                  __printf_s
                  0x0021a2                  __printf_cdnopuxX
                  0x0021a2                  __printf_cdnopsuxX
                  0x002312                  _vfprintf
                  0x003744                  _strcspn
                  0x00376e                  _strspn
                  0x003798                  _strchr
                  0x00383a                  ___adddf3
                  0x003934                  ___ltdf2
                  0x003934                  ___ledf2
                  0x003934                  ___eqdf2
                  0x00393e                  ___gtdf2
                  0x00393e                  ___gedf2
                  0x003948                  ___divdf3
                  0x0039fc                  ___nedf2
                  0x003a06                  __dpack
                  0x003a5e                  __dunpack2
                  0x003a80                  __dreturnNaN
                  0x003a86                  __dunpack2exit
                  0x003a90                  ___extendsfdf2
                  0x003ace                  ___fixunsdfdi
                  0x003b30                  ___fixunsdfsi
                  0x003b7c                  ___floatundidf
                  0x003bd2                  ___floatunsidf
                  0x003bd6                  _frexp
                  0x003bd6                  _frexpl
                  0x003c10                  ___muldf3
                  0x003cfa                  ___subdf3
                  0x003cfe                  ___mulp32peds3
                  0x003cfe                  ___mulsi3
                  0x003cfe                  ___mulp32eds3
                  0x003d78                  ___udivmoddi3
                  0x003e48                  ___udivdi3
                  0x003e5a                  ___umoddi3
                  0x003e66                  ___divdi3
                  0x003eca                  ___moddi3
                  0x003f2a                  ___muldi3
                  0x003f80                  __dcompare
                  0x003fd2                  __dPropagateNaN
                  0x003fee                  __dtype
                  0x004012                  __dunpack
                  0x004060                  ___umuldi3
                  0x00480e                  _DELIMITER
                  0x004812                  _DELIMITER_NULL
                  0x0051e5                  _HTML_UP_ARROW
                  0x0051e8                  _HTML_DOWN_ARROW
                  0x005506                  _device_dsc
                  0x005518                  _configDescriptor1
                  0x00555c                  _sd000
                  0x005560                  _sd001
                  0x005578                  _sd002
                  0x005590                  _USB_CD_Ptr
                  0x005592                  _USB_SD_Ptr
                  0x005598                  _abBitReverseTable16
                  0x0055a8                  _crc_table32
                  0x00566e                  _TCPSocketInitializer
                  0x0056a6                  _app_sObject
                  0x0056f4                  _dpv1_sObject
                  0x005746                  _MPFS_Start
                  0x00574a                  _ModbusUartServer
                  0x0057f2                  _ProcessMessageRecu
                  0x00589a                  _LectureMots
                  0x0084ca                  _LectureModbus
                  0x008580                  _envoieLongPF
                  0x0085e0                  _envoieLongPf
                  0x00860c                  _envoieReelPF
                  0x0086b8                  _envoieReelPf
                  0x00876a                  _EcritureMots
                  0x00aa38                  _AffectationIO
                  0x00aa76                  _ModifParamMetro
                  0x00b6b0                  _LectureLong
                  0x00b792                  _LectureReel
                  0x00b8bc                  _ValidationCodeMetrologie
                  0x00b9d8                  _ModbusErreur
                  0x00ba06                  _Random
                  0x00ba36                  _ModifieVitesseComm
                  0x00bb3e                  BEGIN_MPFS
                  0x010d24                  _EcrFRAM_Param
                  0x010d6c                  _EcrFRAM
                  0x010db4                  _LecFRAM_Param
                  0x010e18                  _LecFRAM
                  0x010e60                  _InitParams
                  0x01131c                  _gestion_profibus
                  0x011548                  _process_plcd
                  0x0119a0                  _gestion_defauts_BI
                  0x011c38                  _gestion_cycle_BI
                  0x011f42                  _ImpressionTotalisateur
                  0x0122f0                  _ValEntTOR
                  0x012328                  _gestion_vitesse
                  0x0125ba                  _EnvoieSerie1
                  0x0125fe                  _EnvoieSerie
                  0x01270e                  _gestion_totalisateurs
                  0x012b26                  _verif_totaux
                  0x012d9c                  _etatSortieTOR
                  0x012dd2                  _forcageSortiesTOR
                  0x012f20                  _sortiesTOR
                  0x012f70                  _gestion_poids
                  0x013104                  _gestion_debit
                  0x013224                  _envoyer_reel
                  0x013302                  _moyenne_glissante_debit
                  0x013326                  _moyenne_glissante_poids
                  0x013588                  _conversion_poids
                  0x01360e                  _lecture_entrees_TOR
                  0x0136ea                  _EcritSortieAna
                  0x013c02                  _TCPInit
                  0x013cd2                  _TCPOpen
                  0x013e2c                  _TCPWasReset
                  0x013e5a                  _TCPIsConnected
                  0x013e7e                  _TCPDisconnect
                  0x013f1e                  _TCPClose
                  0x013f3e                  _TCPGetRemoteInfo
                  0x013f68                  _TCPFlush
                  0x013f8e                  _TCPIsPutReady
                  0x013fdc                  _TCPPut
                  0x014082                  _TCPPutArray
                  0x014168                  _TCPPutString
                  0x01418c                  _TCPGetTxFIFOFull
                  0x0141b8                  _TCPDiscard
                  0x0141d8                  _TCPIsGetReady
                  0x014210                  _TCPGet
                  0x01428a                  _TCPGetArray
                  0x014356                  _TCPGetRxFIFOFree
                  0x014380                  _TCPPeekArray
                  0x01442a                  _TCPPeek
                  0x014442                  _TCPFindArrayEx
                  0x0146b2                  _TCPFindEx
                  0x0146d6                  _TCPTick
                  0x014bc6                  _TCPProcess
                  0x015dd4                  _TCPAdjustFIFOSize
                  0x015fd6                  _AD_Init
                  0x01616c                  _AD_GetAdiIndex
                  0x0161a2                  _AD_GetAdiInstEntry
                  0x0161c8                  _AD_ProcObjectRequest
                  0x017168                  _AD_GetAdiValue
                  0x017308                  _AD_SetAdiValue
                  0x017882                  _AD_UpdatePdReadData
                  0x0178d4                  _AD_UpdatePdWriteData
                  0x017936                  _AD_NewWrPd
                  0x017940                  _AD_AdiMappingReq
                  0x017d86                  _AD_RemapDone
                  0x017dae                  _HTTPPrint
                  0x017ffc                  _HTTPPrint_
                  0x01801a                  _HTTPInit
                  0x0180a8                  _HTTPServer
                  0x0193d6                  _HTTPURLDecode
                  0x0194aa                  _HTTPGetArg
                  0x019500                  _HTTPReadPostName
                  0x01952c                  _HTTPReadPostValue
                  0x019748                  _HTTPIncFile
                  0x01982e                  _USBDeviceInit
                  0x019942                  _USBDeviceTasks
                  0x019ade                  _USBEnableEndpoint
                  0x019b18                  _USBTransferOnePacket
                  0x019c52                  _USBStallEndpoint
                  0x019de0                  _USBCancelIO
                  0x019f72                  _USBDeviceDetach
                  0x019f84                  _USBDeviceAttach
                  0x019fc6                  _USBCtrlEPAllowStatusStage
                  0x01a0fe                  _USBCtrlEPAllowDataStage
                  0x01b0fc                  _GestionCyclePesage
                  0x01c366                  _MACInit
                  0x01c496                  _MACIsLinked
                  0x01c4ac                  _MACIsTxReady
                  0x01c4c4                  _MACDiscardRx
                  0x01c500                  _MACGetFreeRxSize
                  0x01c58a                  _MACGetHeader
                  0x01c65c                  _MACPutHeader
                  0x01c6b2                  _MACFlush
                  0x01c7f4                  _MACSetReadPtrInRx
                  0x01c826                  _MACSetWritePtr
                  0x01c85c                  _MACSetReadPtr
                  0x01c892                  _MACCalcRxChecksum
                  0x01c8f8                  _CalcIPBufferChecksum
                  0x01c9ae                  _MACMemCopyAsync
                  0x01cbb4                  _MACIsMemCopyDone
                  0x01cbcc                  _MACGet
                  0x01cbfe                  _MACGetArray
                  0x01ccdc                  _MACPut
                  0x01cd14                  _MACPutArray
                  0x01cece                  _ReadPHYReg
                  0x01d016                  _WritePHYReg
                  0x01d06e                  _MACPowerDown
                  0x01d0a2                  _MACPowerUp
                  0x01d0c4                  _SetCLKOUT
                  0x01d0da                  _GetCLKOUT
                  0x01d0f8                  _InitApp
                  0x01d114                  _putsUSB
                  0x01d178                  _USB_enqMsg
                  0x01d1c4                  _DeviceCDCInitialize
                  0x01d1e8                  _DeviceCDCTasks
                  0x01d286                  _ProccessCmd
                  0x01d9f6                  _CRC_Init
                  0x01da06                  _CRC_ChecksumWord
                  0x01da6c                  _ResetCounterMillis
                  0x01da76                  _GetCounterMillis
                  0x01da8c                  _UpdateB40ADI
                  0x01dcac                  _BerkeleySocketInit
                  0x01dcd8                  _socket
                  0x01dd72                  _bind
                  0x01de12                  _listen
                  0x01df2e                  _accept
                  0x01e074                  _connect
                  0x01e1f4                  _send
                  0x01e214                  _sendto
                  0x01e3d8                  _recv
                  0x01e470                  _recvfrom
                  0x01e5d0                  _gethostname
                  0x01e632                  _closesocket
                  0x01e80a                  _HTTPNeedsAuth
                  0x01e83e                  _HTTPCheckAuth
                  0x01e870                  _HTTPExecuteGet
                  0x01e8f4                  _HTTPExecutePost
                  0x01ec66                  _HTTPPrint_builddate
                  0x01ecb4                  _HTTPPrint_version
                  0x01ecd4                  _HTTPPrint_btn
                  0x01ed2a                  _HTTPPrint_led
                  0x01ed7e                  _HTTPPrint_ledSelected
                  0x01ede2                  _HTTPPrint_pot
                  0x01ee10                  _HTTPPrint_lcdtext
                  0x01ee4a                  _HTTPPrint_hellomsg
                  0x01ee96                  _HTTPPrint_cookiename
                  0x01eee4                  _HTTPPrint_uploadeImage
                  0x01eeea                  _HTTPPrint_uploadedmd5
                  0x01ef3c                  _HTTPPrintIP
                  0x01efa2                  _HTTPPrint_config_hostname
                  0x01efc0                  _HTTPPrint_config_dhcpchecked
                  0x01efea                  _HTTPPrint_config_ip
                  0x01f018                  _HTTPPrint_config_gw
                  0x01f046                  _HTTPPrint_config_subnet
                  0x01f074                  _HTTPPrint_config_dns1
                  0x01f0a2                  _HTTPPrint_config_dns2
                  0x01f0d0                  _HTTPPrint_config_mac
                  0x01f188                  _HTTPPrint_read_comm
                  0x01f190                  _HTTPPrint_write_comm
                  0x01f198                  _HTTPPrint_reboot
                  0x01f1a0                  _HTTPPrint_rebootaddr
                  0x01f1be                  _HTTPPrint_ddns_user
                  0x01f1c4                  _HTTPPrint_ddns_pass
                  0x01f1ca                  _HTTPPrint_ddns_host
                  0x01f1d0                  _HTTPPrint_ddns_service
                  0x01f1d8                  _HTTPPrint_ddns_status
                  0x01f1f8                  _HTTPPrint_ddns_status_msg
                  0x01f246                  _HTTPPrint_smtps_en
                  0x01f266                  _HTTPPrint_snmp_en
                  0x01f286                  _HTTPPrint_status_ok
                  0x01f2cc                  _HTTPPrint_status_fail
                  0x01f312                  _MPFSInit
                  0x01f33e                  _MPFSOpen
                  0x01f494                  _MPFSOpenID
                  0x01f51e                  _MPFSClose
                  0x01f544                  _MPFSGet
                  0x01f6d4                  _MPFSGetArray
                  0x01f8fe                  _MPFSGetLong
                  0x01f920                  _MPFSSeek
                  0x01fb32                  _MPFSGetTimestamp
                  0x01fb78                  _MPFSGetMicrotime
                  0x01fbbe                  _MPFSGetFlags
                  0x01fc02                  _MPFSGetSize
                  0x01fc48                  _MPFSGetBytesRem
                  0x01fc86                  _MPFSGetStartAddr
                  0x01fcce                  _MPFSGetEndAddr
                  0x01fd20                  _MPFSGetFilename
                  0x01fd84                  _MPFSGetPosition
                  0x01fdaa                  _MPFSGetID
                  0x01fe04                  _main
                  0x01ff34                  _ABCCMainStateMachine
                  0x01ffda                  _DisplayIPValue
                  0x020010                  _GestionReponseModbus
                  0x02017c                  _ProcessIO
                  0x0203c0                  _InitTCPIPAppConfig
                  0x02049c                  _InitializeBoard
                  0x02066e                  _SaveAppConfig
                  0x0206a6                  _ADInit
                  0x0206f8                  _LEDUpdateUSBStatus
                  0x020766                  _USER_USB_CALLBACK_EVENT_HANDLER
                  0x0207ca                  _LFSRSeedRand
                  0x02080c                  _LFSRRand
                  0x02087c                  _GenerateRandomDWORD
                  0x020986                  _StringToIPAddress
                  0x020b00                  _Base64Decode
                  0x020c68                  _uitoa
                  0x020ce8                  _hexatob
                  0x020d52                  _btohexa_high
                  0x020d74                  _btohexa_low
                  0x020d92                  _stricmppgm2ram
                  0x020e2a                  _swaps
                  0x020e46                  _swapl
                  0x020ea6                  _CalcIPChecksum
                  0x020f28                  _strupr
                  0x020f68                  _FormatNetBIOSName
                  0x020fb2                  _strnchr
                  0x021000                  _strncpy_m
                  0x02107e                  _DNSBeginUsage
                  0x02109e                  _DNSEndUsage
                  0x0210d6                  _DNSResolve
                  0x021116                  _DNSIsResolved
                  0x021914                  _UDPInit
                  0x021934                  _UDPOpenEx
                  0x021a4e                  _UDPTask
                  0x021c90                  _UDPIsOpened
                  0x021cb2                  _UDPClose
                  0x021cf4                  _UDPSetTxBuffer
                  0x021d0a                  _UDPSetRxBuffer
                  0x021d20                  _UDPIsPutReady
                  0x021d56                  _UDPPut
                  0x021d86                  _UDPPutArray
                  0x021dc2                  _UDPPutString
                  0x021de0                  _UDPFlush
                  0x021eda                  _UDPIsGetReady
                  0x021f10                  _UDPGet
                  0x021f44                  _UDPGetArray
                  0x021f90                  _UDPDiscard
                  0x021fb6                  _UDPProcess
                  0x02218e                  _UARTs_Init
                  0x022284                  _BaudrateIsValid
                  0x0222f4                  _UART1_SetBaudrate
                  0x02234a                  _UART2_SetBaudrate
                  0x0223a0                  _UART3_SetBaudrate
                  0x0223f6                  _UART4_SetBaudrate
                  0x02244c                  _UART1_SetStopBit
                  0x02248a                  _UART2_SetStopBit
                  0x0224c8                  _UART1_SetParityNBits
                  0x022520                  _UART2_SetParityNBits
                  0x022578                  _ReceiveUART1
                  0x0225ee                  _ReceiveUART2
                  0x02272c                  _ReceiveUART3
                  0x02285e                  _ReceiveUART4
                  0x022990                  _SendStrUART3
                  0x0229bc                  _SendStrUART4
                  0x0229f4                  _ABCC_SetupInit
                  0x022a22                  _ABCC_SetupCommands
                  0x022d52                  _ABCC_SetupResponses
                  0x0230dc                  _ABCC_UserInitComplete
                  0x023114                  _ABCC_NetworkType
                  0x02311e                  _ABCC_ModuleType
                  0x023128                  _ABCC_NetFormatType
                  0x023132                  _ABCC_ParameterSupport
                  0x02316a                  _ABCC_DrvSpiRunDriverTx
                  0x0232a6                  _ABCC_DrvSpiRunDriverRx
                  0x023438                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_spi_drv_DataReceived
                  0x02347e                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_drv_WdTimeoutHandler
                  0x02348c                  _ABCC_DrvSpiInit
                  0x023534                  _ABCC_DrvSpiWriteMessage
                  0x0235b0                  _ABCC_DrvSpiWriteProcessData
                  0x0235e6                  _ABCC_DrvSpiIsReadyForWriteMessage
                  0x02360c                  _ABCC_DrvSpiIsReadyForCmd
                  0x02362c                  _ABCC_DrvSpiSetNbrOfCmds
                  0x023638                  _ABCC_DrvSpiSetAppStatus
                  0x023648                  _ABCC_DrvSpiSetPdSize
                  0x0236a4                  _ABCC_DrvSpiSetMsgReceiverBuffer
                  0x0236ec                  _ABCC_DrvSpiGetIntStatus
                  0x023710                  _ABCC_DrvSpiGetAnybusState
                  0x02371e                  _ABCC_DrvSpiReadProcessData
                  0x023736                  _ABCC_DrvSpiReadMessage
                  0x023758                  _ABCC_DrvSpiSetIntMask
                  0x023768                  _ABCC_DrvSpiGetWrPdBuffer
                  0x023778                  _ABCC_DrvSpiGetModCap
                  0x02379c                  _ABCC_DrvSpiGetLedStatus
                  0x0237a6                  _ABCC_DrvSpiIsReadyForWrPd
                  0x0237ba                  _ABCC_DrvSpiIsSupervised
                  0x0237d0                  _ABCC_DrvSpiGetAnbStatus
                  0x0237de                  _AD7190_SetRegisterValue
                  0x023830                  _AD7190_GetRegisterValue
                  0x0238a2                  _AD7190_Init
                  0x0238d6                  _AD7190_Reset
                  0x023902                  _AD7190_SetPower
                  0x023992                  _AD7190_WaitRdyGoLow
                  0x0239c6                  _AD7190_ChannelSelect
                  0x023a26                  _AD7190_Calibrate
                  0x023ab4                  _AD7190_RangeSetup
                  0x023b3a                  _AD7190_SingleConversion
                  0x023b7a                  _AD7190_ContinuousReadAvg
                  0x023be2                  _AD7190_TemperatureRead
                  0x023c44                  _AD7190_StartContinuousRead
                  0x023cac                  _AD7190_StopContinuousRead
                  0x023cce                  _AD7190_PrintRegisters
                  0x023e08                  _ABCC_SetReadyForCommunication
                  0x023e12                  _ABCC_SetMainStateError
                  0x023e1c                  _ABCC_GetMainState
                  0x023e26                  _ABCC_CheckAnbStatus
                  0x023e46                  _ABCC_CheckSendMessage
                  0x023e50                  _ABCC_StartDriver
                  0x023fe8                  _ABCC_isReadyForCommunication
                  0x024070                  _ABCC_NewWrPdEvent
                  0x02409e                  _ABCC_RdPdEvent
                  0x0240c2                  _ABCC_RdMsgEvent
                  0x02414a                  _ABCC_SendCmdMsg
                  0x02419a                  _ABCC_GetCmdQueueSize
                  0x0241a8                  _ABCC_SendRespMsg
                  0x0241ba                  _ABCC_MsgAlloc
                  0x0241c8                  _ABCC_MsgFree
                  0x0241da                  _ABCC_SetPdSize
                  0x024202                  _ABCC_HWReset
                  0x02421e                  _ABCC_ShutdownDriver
                  0x024240                  _ABCC_ModuleDetect
                  0x02424e                  _ABCC_ModCap
                  0x02425c                  _ABCC_LedStatus
                  0x02426a                  _ABCC_AnbState
                  0x024278                  _ABCC_IsSupervised
                  0x024286                  _ABCC_HWReleaseReset
                  0x024290                  _ABCC_SetAppStatus
                  0x02429e                  _ABCC_ReadModuleId
                  0x0242ac                  _ABCC_RunTimerSystem
                  0x0242ba                  _ABCC_GetNewSourceId
                  0x0242ea                  _ABCC_GetOpmode
                  0x0242f8                  _ABCC_GetAttribute
                  0x024350                  _ABCC_SetByteAttribute
                  0x0243b2                  _ABCC_VerifyMessage
                  0x0243c6                  _SetErrorReporter
                  0x0243d2                  _ABCC_GetDataTypeSize
                  0x02450e                  _ABCC_LinkInit
                  0x024598                  _ABCC_LinkReadMessage
                  0x024618                  _ABCC_LinkCheckSendMessage
                  0x0246a2                  _ABCC_LinkRunDriverRx
                  0x0246c0                  _ABCC_LinkGetNumCmdQueueEntries
                  0x0246d4                  _ABCC_LinkWriteMessage
                  0x0247f2                  _ABCC_LinkWrMsgWithNotification
                  0x024836                  _ABCC_LinkAlloc
                  0x02484c                  _ABCC_LinkFree
                  0x0248aa                  _ABCC_LinkMapMsgHandler
                  0x0248fe                  _ABCC_LinkGetMsgHandler
                  0x02495c                  _ABCC_LinkIsSrcIdUsed
                  0x024e9a                  _Flash_N_Clock
                  0x024eb8                  _Active_Flash
                  0x024ec0                  _Desactive_Flash
                  0x024ece                  _Flash_Ready
                  0x024ef0                  _Wait_Flash_Ready
                  0x024f00                  _Write_Flash
                  0x024f32                  _Charge_Pointeurs
                  0x024f4a                  _Lecture_Byte_In_Flash
                  0x024f66                  _Direct_Byte_Write_In_Page
                  0x024f7e                  _Transfert_Page_To_Buffer
                  0x024f96                  _Read_Flash
                  0x024fd2                  _Incremente_Adresse_FlashDB32
                  0x0250a0                  _Incremente_Adresse_FlashDB64
                  0x02516e                  _MakeAddrDB32
                  0x0251ca                  _MakeAddrDB64
                  0x02522c                  _Ecriture_Memoire_Flash_Ligne_Str
                  0x0252bc                  _Lecture_Memoire_Flash_Ligne_Str
                  0x025344                  _USBCheckCDCRequest
                  0x02548e                  _CDCInitEP
                  0x0254de                  _USBCDCEventHandler
                  0x025524                  _getsUSBUSART
                  0x0255b8                  _putUSBUSART
                  0x0255e4                  _putsUSBUSART
                  0x02563a                  _putrsUSBUSART
                  0x025690                  _CDCTxService
                  0x025792                  _APP_IsResetRequestAllowed
                  0x0257a8                  _APP_ProcResetRequest
                  0x0257d4                  _APP_ProcessCmdMsg
                  0x0257fe                  _app_InstanceCommand
                  0x025a08                  _app_ObjectCommand
                  0x025bd2                  _NBNSTask
                  0x025f80                  _ARPSendPkt
                  0x026054                  _ARPInit
                  0x026086                  _ARPProcess
                  0x02615e                  _ARPResolve
                  0x026228                  _ARPIsResolved
                  0x0262f0                  _SwapARPPacket
                  0x026328                  _FRAMInit
                  0x026340                  _FRAMBeginRead
                  0x026358                  _FRAMRead
                  0x02639c                  _FRAMReadArray
                  0x026478                  _FRAMBeginWrite
                  0x026490                  _FRAMWrite
                  0x0264d2                  _FRAMWriteArray
                  0x026500                  _FRAMEndWrite
                  0x02660e                  _FRAMIsBusy
                  0x026680                  _Dep_AttenteDCY
                  0x0266fe                  _Dep_Chargement
                  0x0267d6                  _Dep_AttenteFermVanne
                  0x0268c4                  _Dep_Suspension
                  0x026968                  _gestion_cycle_Depeseur
                  0x0269d0                  _XEEInit
                  0x0269ee                  _XEEBeginRead
                  0x026a06                  _XEERead
                  0x026a4a                  _XEEEndRead
                  0x026a54                  _XEEReadArray
                  0x026b12                  _XEEBeginWrite
                  0x026b2a                  _XEEWrite
                  0x026b6c                  _XEEWriteArray
                  0x026b9a                  _XEEEndWrite
                  0x026c94                  _XEEIsBusy
                  0x026d06                  _TestModbus
                  0x026d6a                  _BerkeleyTCPServer
                  0x027006                  _ECANFilterSID
                  0x027036                  _ECANFilterEID
                  0x027048                  _ECAN1DMAConfig
                  0x027090                  _ECAN1ClockConfig
                  0x0270a0                  _ECAN1InterruptConfig
                  0x0270ca                  _ECAN1TxRxBuffersConfig
                  0x0270d4                  _ECAN1RxFiltersConfig
                  0x027140                  _ECAN1SendPacket
                  0x027176                  _ECAN1SetOPMode
                  0x027192                  _ECANCreateSIDPacket
                  0x0271e6                  _ECANCreateEIDPacket
                  0x0272f2                  _DPV1_ProcessCmdMsg
                  0x02731c                  _dpv1_InstanceCommand
                  0x027478                  _dpv1_ObjectCommand
                  0x0275d6                  _ICMPProcess
                  0x0276c2                  _ICMPSendPing
                  0x0276e6                  _ICMPSendPingToHost
                  0x027710                  _ICMPGetReply
                  0x02786a                  _ICMPBeginUsage
                  0x02788a                  _ICMPEndUsage
                  0x027898                  _RegulationDoseur
                  0x0279a8                  _RegulationPID
                  0x027b18                  _BerkeleyUDPClient
                  0x027d40                  _BerkeleySNTPGetUTCSeconds
                  0x027d92                  _CRC_Crc32
                  0x027fe4                  _US_Init
                  0x027fee                  _US_RunUserInitStateMachine
                  0x0280e4                  build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o:_US_ProcessRespMsg
                  0x0281fc                  _US_SetSwitch1
                  0x02820e                  _US_SetSwitch2
                  0x028220                  _ABCC_TimerInit
                  0x028242                  _ABCC_TimerCreate
                  0x0282b4                  _ABCC_TimerStart
                  0x028332                  _ABCC_TimerStop
                  0x028374                  _ABCC_TimerTick
                  0x028414                  _BdC_VerifContacts
                  0x02841a                  _BdC_AttenteDCY
                  0x028480                  _BdC_InitChargement
                  0x0285aa                  _BdC_Chargement
                  0x0285cc                  _gestion_cycle_BdC
                  0x0285ec                  _IPGetHeader
                  0x0286b6                  _IPPutHeader
                  0x028768                  _IPSetRxBuffer
                  0x0287b6                  _AnnounceIP
                  0x028860                  _DiscoveryTask
                  0x028978                  _StackInit
                  0x0289b0                  _StackTask
                  0x028b24                  _StackApplications
                  0x028b3a                  _ABCC_CbfUserInitReq
                  0x028b48                  _ABCC_CbfAdiMappingReq
                  0x028b5a                  _ABCC_CbfRemapDone
                  0x028b64                  _ABCC_CbfUpdateWriteProcessData
                  0x028b76                  _ABCC_CbfNewReadPd
                  0x028b84                  _ABCC_CbfDriverError
                  0x028ba6                  _ABCC_CbfReceiveMsg
                  0x028c16                  _ABCC_CbfWdTimeout
                  0x028c2c                  _ABCC_CbfWdTimeoutRecovered
                  0x028c42                  _ABCC_CbfEvent
                  0x028c7c                  _ABCC_CbfAnbStatusChanged
                  0x028ca4                  _MODBUSTCPServer
                  0x028d42                  _ProcessReceivedMessage
                  0x028dd6                  _ModbusError
                  0x028e04                  _TickInit
                  0x028e96                  _TickGet
                  0x028ec8                  _TickGetDiv256
                  0x028efa                  _TickGetDiv64K
                  0x028f2c                  _TickConvertToMilliseconds
                  0x028f46                  __T1Interrupt
                  0x028f5e                  _BerkeleyTCPClient
                  0x02908c                  _ABCC_SYS_Init
                  0x0290b6                  _ABCC_SYS_Close
                  0x0290c0                  _ABCC_SYS_SetOpmode
                  0x0290c8                  _ABCC_SYS_GetOpmode
                  0x0290d2                  _ABCC_SYS_HWReset
                  0x0290da                  _ABCC_SYS_HWReleaseReset
                  0x0290e2                  _ABCC_SYS_ReadModuleId
                  0x0290ec                  _ABCC_SYS_ModuleDetect
                  0x029104                  _ABCC_SYS_AbccInterruptEnable
                  0x029110                  _ABCC_SYS_AbccInterruptDisable
                  0x029118                  _ABCC_SYS_EnterCriticalImpl
                  0x02911e                  _ABCC_SYS_ExitCriticalImpl
                  0x029124                  _ABCC_SYS_UseCriticalImpl
                  0x02912a                  _ABCC_SYS_SpiRegDataReceived
                  0x029136                  _ABCC_SYS_SpiSendReceive
                  0x0291a4                  _RebootTask
                  0x0292bc                  _InitAdc1
                  0x02931c                  _InitTmr3
                  0x029330                  _InitDma0
                  0x029368                  _ProcessADCSamples
                  0x0293d2                  _ADSPI_Init
                  0x0293f8                  _SPI_Read
                  0x02946a                  _SPI_Write
                  0x0294d2                  _ABCC_MemCreatePool
                  0x02951e                  _ABCC_MemAlloc
                  0x02955a                  _ABCC_MemFree
                  0x02959a                  _ABCC_SpiRunDriver
                  0x0295f6                  _ABCC_SpiISR
                  0x029620                  _ConfigureOscillator
                  0x02969e                  _DelayMs
                  0x0296da                  _Delay10us
                  0x029716                  _USBSleepOnSuspend
                  0x02976c                  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o:_abcc_RemapRespMsgSent
                  0x029782                  _ABCC_SendRemapRespMsg
                  0x0297ae                  _AD_GetNumAdi
                  0x0297b8                  _ADI_GetDefaultMap
                  0x0297c2                  _ADI_GetADIEntryList
                  0x0297cc                  _ReadProgramMemory

External Symbols in Program Memory (by name):

                  0x00bb3e                  BEGIN_MPFS
                  0x01ff34                  _ABCCMainStateMachine
                  0x02426a                  _ABCC_AnbState
                  0x028b48                  _ABCC_CbfAdiMappingReq
                  0x028c7c                  _ABCC_CbfAnbStatusChanged
                  0x028b84                  _ABCC_CbfDriverError
                  0x028c42                  _ABCC_CbfEvent
                  0x028b76                  _ABCC_CbfNewReadPd
                  0x028ba6                  _ABCC_CbfReceiveMsg
                  0x028b5a                  _ABCC_CbfRemapDone
                  0x028b64                  _ABCC_CbfUpdateWriteProcessData
                  0x028b3a                  _ABCC_CbfUserInitReq
                  0x028c16                  _ABCC_CbfWdTimeout
                  0x028c2c                  _ABCC_CbfWdTimeoutRecovered
                  0x023e26                  _ABCC_CheckAnbStatus
                  0x023e46                  _ABCC_CheckSendMessage
                  0x0237d0                  _ABCC_DrvSpiGetAnbStatus
                  0x023710                  _ABCC_DrvSpiGetAnybusState
                  0x0236ec                  _ABCC_DrvSpiGetIntStatus
                  0x02379c                  _ABCC_DrvSpiGetLedStatus
                  0x023778                  _ABCC_DrvSpiGetModCap
                  0x023768                  _ABCC_DrvSpiGetWrPdBuffer
                  0x02348c                  _ABCC_DrvSpiInit
                  0x02360c                  _ABCC_DrvSpiIsReadyForCmd
                  0x0237a6                  _ABCC_DrvSpiIsReadyForWrPd
                  0x0235e6                  _ABCC_DrvSpiIsReadyForWriteMessage
                  0x0237ba                  _ABCC_DrvSpiIsSupervised
                  0x023736                  _ABCC_DrvSpiReadMessage
                  0x02371e                  _ABCC_DrvSpiReadProcessData
                  0x0232a6                  _ABCC_DrvSpiRunDriverRx
                  0x02316a                  _ABCC_DrvSpiRunDriverTx
                  0x023638                  _ABCC_DrvSpiSetAppStatus
                  0x023758                  _ABCC_DrvSpiSetIntMask
                  0x0236a4                  _ABCC_DrvSpiSetMsgReceiverBuffer
                  0x02362c                  _ABCC_DrvSpiSetNbrOfCmds
                  0x023648                  _ABCC_DrvSpiSetPdSize
                  0x023534                  _ABCC_DrvSpiWriteMessage
                  0x0235b0                  _ABCC_DrvSpiWriteProcessData
                  0x0242f8                  _ABCC_GetAttribute
                  0x02419a                  _ABCC_GetCmdQueueSize
                  0x0243d2                  _ABCC_GetDataTypeSize
                  0x023e1c                  _ABCC_GetMainState
                  0x0242ba                  _ABCC_GetNewSourceId
                  0x0242ea                  _ABCC_GetOpmode
                  0x024286                  _ABCC_HWReleaseReset
                  0x024202                  _ABCC_HWReset
                  0x024278                  _ABCC_IsSupervised
                  0x02425c                  _ABCC_LedStatus
                  0x024836                  _ABCC_LinkAlloc
                  0x024618                  _ABCC_LinkCheckSendMessage
                  0x02484c                  _ABCC_LinkFree
                  0x0248fe                  _ABCC_LinkGetMsgHandler
                  0x0246c0                  _ABCC_LinkGetNumCmdQueueEntries
                  0x02450e                  _ABCC_LinkInit
                  0x02495c                  _ABCC_LinkIsSrcIdUsed
                  0x0248aa                  _ABCC_LinkMapMsgHandler
                  0x024598                  _ABCC_LinkReadMessage
                  0x0246a2                  _ABCC_LinkRunDriverRx
                  0x0247f2                  _ABCC_LinkWrMsgWithNotification
                  0x0246d4                  _ABCC_LinkWriteMessage
                  0x02951e                  _ABCC_MemAlloc
                  0x0294d2                  _ABCC_MemCreatePool
                  0x02955a                  _ABCC_MemFree
                  0x02424e                  _ABCC_ModCap
                  0x024240                  _ABCC_ModuleDetect
                  0x02311e                  _ABCC_ModuleType
                  0x0241ba                  _ABCC_MsgAlloc
                  0x0241c8                  _ABCC_MsgFree
                  0x023128                  _ABCC_NetFormatType
                  0x023114                  _ABCC_NetworkType
                  0x024070                  _ABCC_NewWrPdEvent
                  0x023132                  _ABCC_ParameterSupport
                  0x0240c2                  _ABCC_RdMsgEvent
                  0x02409e                  _ABCC_RdPdEvent
                  0x02429e                  _ABCC_ReadModuleId
                  0x0242ac                  _ABCC_RunTimerSystem
                  0x029110                  _ABCC_SYS_AbccInterruptDisable
                  0x029104                  _ABCC_SYS_AbccInterruptEnable
                  0x0290b6                  _ABCC_SYS_Close
                  0x029118                  _ABCC_SYS_EnterCriticalImpl
                  0x02911e                  _ABCC_SYS_ExitCriticalImpl
                  0x0290c8                  _ABCC_SYS_GetOpmode
                  0x0290da                  _ABCC_SYS_HWReleaseReset
                  0x0290d2                  _ABCC_SYS_HWReset
                  0x02908c                  _ABCC_SYS_Init
                  0x0290ec                  _ABCC_SYS_ModuleDetect
                  0x0290e2                  _ABCC_SYS_ReadModuleId
                  0x0290c0                  _ABCC_SYS_SetOpmode
                  0x02912a                  _ABCC_SYS_SpiRegDataReceived
                  0x029136                  _ABCC_SYS_SpiSendReceive
                  0x029124                  _ABCC_SYS_UseCriticalImpl
                  0x02414a                  _ABCC_SendCmdMsg
                  0x029782                  _ABCC_SendRemapRespMsg
                  0x0241a8                  _ABCC_SendRespMsg
                  0x024290                  _ABCC_SetAppStatus
                  0x024350                  _ABCC_SetByteAttribute
                  0x023e12                  _ABCC_SetMainStateError
                  0x0241da                  _ABCC_SetPdSize
                  0x023e08                  _ABCC_SetReadyForCommunication
                  0x022a22                  _ABCC_SetupCommands
                  0x0229f4                  _ABCC_SetupInit
                  0x022d52                  _ABCC_SetupResponses
                  0x02421e                  _ABCC_ShutdownDriver
                  0x0295f6                  _ABCC_SpiISR
                  0x02959a                  _ABCC_SpiRunDriver
                  0x023e50                  _ABCC_StartDriver
                  0x028242                  _ABCC_TimerCreate
                  0x028220                  _ABCC_TimerInit
                  0x0282b4                  _ABCC_TimerStart
                  0x028332                  _ABCC_TimerStop
                  0x028374                  _ABCC_TimerTick
                  0x0230dc                  _ABCC_UserInitComplete
                  0x0243b2                  _ABCC_VerifyMessage
                  0x023fe8                  _ABCC_isReadyForCommunication
                  0x023a26                  _AD7190_Calibrate
                  0x0239c6                  _AD7190_ChannelSelect
                  0x023b7a                  _AD7190_ContinuousReadAvg
                  0x023830                  _AD7190_GetRegisterValue
                  0x0238a2                  _AD7190_Init
                  0x023cce                  _AD7190_PrintRegisters
                  0x023ab4                  _AD7190_RangeSetup
                  0x0238d6                  _AD7190_Reset
                  0x023902                  _AD7190_SetPower
                  0x0237de                  _AD7190_SetRegisterValue
                  0x023b3a                  _AD7190_SingleConversion
                  0x023c44                  _AD7190_StartContinuousRead
                  0x023cac                  _AD7190_StopContinuousRead
                  0x023be2                  _AD7190_TemperatureRead
                  0x023992                  _AD7190_WaitRdyGoLow
                  0x0297c2                  _ADI_GetADIEntryList
                  0x0297b8                  _ADI_GetDefaultMap
                  0x0206a6                  _ADInit
                  0x0293d2                  _ADSPI_Init
                  0x017940                  _AD_AdiMappingReq
                  0x01616c                  _AD_GetAdiIndex
                  0x0161a2                  _AD_GetAdiInstEntry
                  0x017168                  _AD_GetAdiValue
                  0x0297ae                  _AD_GetNumAdi
                  0x015fd6                  _AD_Init
                  0x017936                  _AD_NewWrPd
                  0x0161c8                  _AD_ProcObjectRequest
                  0x017d86                  _AD_RemapDone
                  0x017308                  _AD_SetAdiValue
                  0x017882                  _AD_UpdatePdReadData
                  0x0178d4                  _AD_UpdatePdWriteData
                  0x025792                  _APP_IsResetRequestAllowed
                  0x0257a8                  _APP_ProcResetRequest
                  0x0257d4                  _APP_ProcessCmdMsg
                  0x026054                  _ARPInit
                  0x026228                  _ARPIsResolved
                  0x026086                  _ARPProcess
                  0x02615e                  _ARPResolve
                  0x025f80                  _ARPSendPkt
                  0x024eb8                  _Active_Flash
                  0x00aa38                  _AffectationIO
                  0x0287b6                  _AnnounceIP
                  0x020b00                  _Base64Decode
                  0x022284                  _BaudrateIsValid
                  0x02841a                  _BdC_AttenteDCY
                  0x0285aa                  _BdC_Chargement
                  0x028480                  _BdC_InitChargement
                  0x028414                  _BdC_VerifContacts
                  0x027d40                  _BerkeleySNTPGetUTCSeconds
                  0x01dcac                  _BerkeleySocketInit
                  0x028f5e                  _BerkeleyTCPClient
                  0x026d6a                  _BerkeleyTCPServer
                  0x027b18                  _BerkeleyUDPClient
                  0x00089a                  _BusyUART2
                  0x0008a8                  _BusyUART3
                  0x0008b6                  _BusyUART4
                  0x02548e                  _CDCInitEP
                  0x025690                  _CDCTxService
                  0x01da06                  _CRC_ChecksumWord
                  0x027d92                  _CRC_Crc32
                  0x01d9f6                  _CRC_Init
                  0x01c8f8                  _CalcIPBufferChecksum
                  0x020ea6                  _CalcIPChecksum
                  0x024f32                  _Charge_Pointeurs
                  0x0007f2                  _CloseSPI1
                  0x0007fe                  _CloseSPI3
                  0x0008c4                  _CloseUART1
                  0x0008d4                  _CloseUART2
                  0x0008e4                  _CloseUART3
                  0x0008f4                  _CloseUART4
                  0x000904                  _ConfigIntUART1
                  0x000950                  _ConfigIntUART2
                  0x00099c                  _ConfigIntUART3
                  0x0009e8                  _ConfigIntUART4
                  0x029620                  _ConfigureOscillator
                  0x00480e                  _DELIMITER
                  0x004812                  _DELIMITER_NULL
                  0x02107e                  _DNSBeginUsage
                  0x02109e                  _DNSEndUsage
                  0x021116                  _DNSIsResolved
                  0x0210d6                  _DNSResolve
                  0x0272f2                  _DPV1_ProcessCmdMsg
                  0x00080a                  _DataRdySPI1
                  0x000814                  _DataRdySPI3
                  0x000a30                  _DataRdyUART1
                  0x000a3a                  _DataRdyUART2
                  0x000a44                  _DataRdyUART3
                  0x000a4e                  _DataRdyUART4
                  0x0296da                  _Delay10us
                  0x02969e                  _DelayMs
                  0x026680                  _Dep_AttenteDCY
                  0x0267d6                  _Dep_AttenteFermVanne
                  0x0266fe                  _Dep_Chargement
                  0x0268c4                  _Dep_Suspension
                  0x024ec0                  _Desactive_Flash
                  0x01d1c4                  _DeviceCDCInitialize
                  0x01d1e8                  _DeviceCDCTasks
                  0x024f66                  _Direct_Byte_Write_In_Page
                  0x028860                  _DiscoveryTask
                  0x01ffda                  _DisplayIPValue
                  0x027090                  _ECAN1ClockConfig
                  0x027048                  _ECAN1DMAConfig
                  0x0270a0                  _ECAN1InterruptConfig
                  0x0270d4                  _ECAN1RxFiltersConfig
                  0x027140                  _ECAN1SendPacket
                  0x027176                  _ECAN1SetOPMode
                  0x0270ca                  _ECAN1TxRxBuffersConfig
                  0x0271e6                  _ECANCreateEIDPacket
                  0x027192                  _ECANCreateSIDPacket
                  0x027036                  _ECANFilterEID
                  0x027006                  _ECANFilterSID
                  0x010d6c                  _EcrFRAM
                  0x010d24                  _EcrFRAM_Param
                  0x0136ea                  _EcritSortieAna
                  0x00876a                  _EcritureMots
                  0x02522c                  _Ecriture_Memoire_Flash_Ligne_Str
                  0x0125fe                  _EnvoieSerie
                  0x0125ba                  _EnvoieSerie1
                  0x026340                  _FRAMBeginRead
                  0x026478                  _FRAMBeginWrite
                  0x026500                  _FRAMEndWrite
                  0x026328                  _FRAMInit
                  0x02660e                  _FRAMIsBusy
                  0x026358                  _FRAMRead
                  0x02639c                  _FRAMReadArray
                  0x026490                  _FRAMWrite
                  0x0264d2                  _FRAMWriteArray
                  0x024e9a                  _Flash_N_Clock
                  0x024ece                  _Flash_Ready
                  0x020f68                  _FormatNetBIOSName
                  0x02087c                  _GenerateRandomDWORD
                  0x01b0fc                  _GestionCyclePesage
                  0x020010                  _GestionReponseModbus
                  0x01d0da                  _GetCLKOUT
                  0x01da76                  _GetCounterMillis
                  0x0051e8                  _HTML_DOWN_ARROW
                  0x0051e5                  _HTML_UP_ARROW
                  0x01e83e                  _HTTPCheckAuth
                  0x01e870                  _HTTPExecuteGet
                  0x01e8f4                  _HTTPExecutePost
                  0x0194aa                  _HTTPGetArg
                  0x019748                  _HTTPIncFile
                  0x01801a                  _HTTPInit
                  0x01e80a                  _HTTPNeedsAuth
                  0x017dae                  _HTTPPrint
                  0x01ef3c                  _HTTPPrintIP
                  0x017ffc                  _HTTPPrint_
                  0x01ecd4                  _HTTPPrint_btn
                  0x01ec66                  _HTTPPrint_builddate
                  0x01efc0                  _HTTPPrint_config_dhcpchecked
                  0x01f074                  _HTTPPrint_config_dns1
                  0x01f0a2                  _HTTPPrint_config_dns2
                  0x01f018                  _HTTPPrint_config_gw
                  0x01efa2                  _HTTPPrint_config_hostname
                  0x01efea                  _HTTPPrint_config_ip
                  0x01f0d0                  _HTTPPrint_config_mac
                  0x01f046                  _HTTPPrint_config_subnet
                  0x01ee96                  _HTTPPrint_cookiename
                  0x01f1ca                  _HTTPPrint_ddns_host
                  0x01f1c4                  _HTTPPrint_ddns_pass
                  0x01f1d0                  _HTTPPrint_ddns_service
                  0x01f1d8                  _HTTPPrint_ddns_status
                  0x01f1f8                  _HTTPPrint_ddns_status_msg
                  0x01f1be                  _HTTPPrint_ddns_user
                  0x01ee4a                  _HTTPPrint_hellomsg
                  0x01ee10                  _HTTPPrint_lcdtext
                  0x01ed2a                  _HTTPPrint_led
                  0x01ed7e                  _HTTPPrint_ledSelected
                  0x01ede2                  _HTTPPrint_pot
                  0x01f188                  _HTTPPrint_read_comm
                  0x01f198                  _HTTPPrint_reboot
                  0x01f1a0                  _HTTPPrint_rebootaddr
                  0x01f246                  _HTTPPrint_smtps_en
                  0x01f266                  _HTTPPrint_snmp_en
                  0x01f2cc                  _HTTPPrint_status_fail
                  0x01f286                  _HTTPPrint_status_ok
                  0x01eee4                  _HTTPPrint_uploadeImage
                  0x01eeea                  _HTTPPrint_uploadedmd5
                  0x01ecb4                  _HTTPPrint_version
                  0x01f190                  _HTTPPrint_write_comm
                  0x019500                  _HTTPReadPostName
                  0x01952c                  _HTTPReadPostValue
                  0x0180a8                  _HTTPServer
                  0x0193d6                  _HTTPURLDecode
                  0x02786a                  _ICMPBeginUsage
                  0x02788a                  _ICMPEndUsage
                  0x027710                  _ICMPGetReply
                  0x0275d6                  _ICMPProcess
                  0x0276c2                  _ICMPSendPing
                  0x0276e6                  _ICMPSendPingToHost
                  0x0285ec                  _IPGetHeader
                  0x0286b6                  _IPPutHeader
                  0x028768                  _IPSetRxBuffer
                  0x011f42                  _ImpressionTotalisateur
                  0x024fd2                  _Incremente_Adresse_FlashDB32
                  0x0250a0                  _Incremente_Adresse_FlashDB64
                  0x0292bc                  _InitAdc1
                  0x01d0f8                  _InitApp
                  0x029330                  _InitDma0
                  0x010e60                  _InitParams
                  0x0203c0                  _InitTCPIPAppConfig
                  0x02931c                  _InitTmr3
                  0x02049c                  _InitializeBoard
                  0x0206f8                  _LEDUpdateUSBStatus
                  0x02080c                  _LFSRRand
                  0x0207ca                  _LFSRSeedRand
                  0x010e18                  _LecFRAM
                  0x010db4                  _LecFRAM_Param
                  0x00b6b0                  _LectureLong
                  0x0084ca                  _LectureModbus
                  0x00589a                  _LectureMots
                  0x00b792                  _LectureReel
                  0x024f4a                  _Lecture_Byte_In_Flash
                  0x0252bc                  _Lecture_Memoire_Flash_Ligne_Str
                  0x01c892                  _MACCalcRxChecksum
                  0x01c4c4                  _MACDiscardRx
                  0x01c6b2                  _MACFlush
                  0x01cbcc                  _MACGet
                  0x01cbfe                  _MACGetArray
                  0x01c500                  _MACGetFreeRxSize
                  0x01c58a                  _MACGetHeader
                  0x01c366                  _MACInit
                  0x01c496                  _MACIsLinked
                  0x01cbb4                  _MACIsMemCopyDone
                  0x01c4ac                  _MACIsTxReady
                  0x01c9ae                  _MACMemCopyAsync
                  0x01d06e                  _MACPowerDown
                  0x01d0a2                  _MACPowerUp
                  0x01ccdc                  _MACPut
                  0x01cd14                  _MACPutArray
                  0x01c65c                  _MACPutHeader
                  0x01c85c                  _MACSetReadPtr
                  0x01c7f4                  _MACSetReadPtrInRx
                  0x01c826                  _MACSetWritePtr
                  0x028ca4                  _MODBUSTCPServer
                  0x01f51e                  _MPFSClose
                  0x01f544                  _MPFSGet
                  0x01f6d4                  _MPFSGetArray
                  0x01fc48                  _MPFSGetBytesRem
                  0x01fcce                  _MPFSGetEndAddr
                  0x01fd20                  _MPFSGetFilename
                  0x01fbbe                  _MPFSGetFlags
                  0x01fdaa                  _MPFSGetID
                  0x01f8fe                  _MPFSGetLong
                  0x01fb78                  _MPFSGetMicrotime
                  0x01fd84                  _MPFSGetPosition
                  0x01fc02                  _MPFSGetSize
                  0x01fc86                  _MPFSGetStartAddr
                  0x01fb32                  _MPFSGetTimestamp
                  0x01f312                  _MPFSInit
                  0x01f33e                  _MPFSOpen
                  0x01f494                  _MPFSOpenID
                  0x01f920                  _MPFSSeek
                  0x005746                  _MPFS_Start
                  0x02516e                  _MakeAddrDB32
                  0x0251ca                  _MakeAddrDB64
                  0x00b9d8                  _ModbusErreur
                  0x028dd6                  _ModbusError
                  0x00574a                  _ModbusUartServer
                  0x00aa76                  _ModifParamMetro
                  0x00ba36                  _ModifieVitesseComm
                  0x025bd2                  _NBNSTask
                  0x00081e                  _OpenSPI1
                  0x00082a                  _OpenSPI3
                  0x000a58                  _OpenUART1
                  0x000a64                  _OpenUART2
                  0x000a70                  _OpenUART3
                  0x000a7c                  _OpenUART4
                  0x01d286                  _ProccessCmd
                  0x029368                  _ProcessADCSamples
                  0x02017c                  _ProcessIO
                  0x0057f2                  _ProcessMessageRecu
                  0x028d42                  _ProcessReceivedMessage
                  0x00ba06                  _Random
                  0x01cece                  _ReadPHYReg
                  0x0297cc                  _ReadProgramMemory
                  0x000836                  _ReadSPI1
                  0x000856                  _ReadSPI3
                  0x000b38                  _ReadUART1
                  0x000b4e                  _ReadUART2
                  0x000b64                  _ReadUART3
                  0x000b7a                  _ReadUART4
                  0x024f96                  _Read_Flash
                  0x0291a4                  _RebootTask
                  0x022578                  _ReceiveUART1
                  0x0225ee                  _ReceiveUART2
                  0x02272c                  _ReceiveUART3
                  0x02285e                  _ReceiveUART4
                  0x027898                  _RegulationDoseur
                  0x0279a8                  _RegulationPID
                  0x01da6c                  _ResetCounterMillis
                  0x0293f8                  _SPI_Read
                  0x02946a                  _SPI_Write
                  0x02066e                  _SaveAppConfig
                  0x022990                  _SendStrUART3
                  0x0229bc                  _SendStrUART4
                  0x01d0c4                  _SetCLKOUT
                  0x0243c6                  _SetErrorReporter
                  0x028b24                  _StackApplications
                  0x028978                  _StackInit
                  0x0289b0                  _StackTask
                  0x020986                  _StringToIPAddress
                  0x0262f0                  _SwapARPPacket
                  0x015dd4                  _TCPAdjustFIFOSize
                  0x013f1e                  _TCPClose
                  0x0141b8                  _TCPDiscard
                  0x013e7e                  _TCPDisconnect
                  0x014442                  _TCPFindArrayEx
                  0x0146b2                  _TCPFindEx
                  0x013f68                  _TCPFlush
                  0x014210                  _TCPGet
                  0x01428a                  _TCPGetArray
                  0x013f3e                  _TCPGetRemoteInfo
                  0x014356                  _TCPGetRxFIFOFree
                  0x01418c                  _TCPGetTxFIFOFull
                  0x013c02                  _TCPInit
                  0x013e5a                  _TCPIsConnected
                  0x0141d8                  _TCPIsGetReady
                  0x013f8e                  _TCPIsPutReady
                  0x013cd2                  _TCPOpen
                  0x01442a                  _TCPPeek
                  0x014380                  _TCPPeekArray
                  0x014bc6                  _TCPProcess
                  0x013fdc                  _TCPPut
                  0x014082                  _TCPPutArray
                  0x014168                  _TCPPutString
                  0x00566e                  _TCPSocketInitializer
                  0x0146d6                  _TCPTick
                  0x013e2c                  _TCPWasReset
                  0x026d06                  _TestModbus
                  0x028f2c                  _TickConvertToMilliseconds
                  0x028e96                  _TickGet
                  0x028ec8                  _TickGetDiv256
                  0x028efa                  _TickGetDiv64K
                  0x028e04                  _TickInit
                  0x024f7e                  _Transfert_Page_To_Buffer
                  0x0222f4                  _UART1_SetBaudrate
                  0x0224c8                  _UART1_SetParityNBits
                  0x02244c                  _UART1_SetStopBit
                  0x02234a                  _UART2_SetBaudrate
                  0x022520                  _UART2_SetParityNBits
                  0x02248a                  _UART2_SetStopBit
                  0x0223a0                  _UART3_SetBaudrate
                  0x0223f6                  _UART4_SetBaudrate
                  0x02218e                  _UARTs_Init
                  0x021cb2                  _UDPClose
                  0x021f90                  _UDPDiscard
                  0x021de0                  _UDPFlush
                  0x021f10                  _UDPGet
                  0x021f44                  _UDPGetArray
                  0x021914                  _UDPInit
                  0x021eda                  _UDPIsGetReady
                  0x021c90                  _UDPIsOpened
                  0x021d20                  _UDPIsPutReady
                  0x021934                  _UDPOpenEx
                  0x021fb6                  _UDPProcess
                  0x021d56                  _UDPPut
                  0x021d86                  _UDPPutArray
                  0x021dc2                  _UDPPutString
                  0x021d0a                  _UDPSetRxBuffer
                  0x021cf4                  _UDPSetTxBuffer
                  0x021a4e                  _UDPTask
                  0x0254de                  _USBCDCEventHandler
                  0x019de0                  _USBCancelIO
                  0x025344                  _USBCheckCDCRequest
                  0x01a0fe                  _USBCtrlEPAllowDataStage
                  0x019fc6                  _USBCtrlEPAllowStatusStage
                  0x019f84                  _USBDeviceAttach
                  0x019f72                  _USBDeviceDetach
                  0x01982e                  _USBDeviceInit
                  0x019942                  _USBDeviceTasks
                  0x019ade                  _USBEnableEndpoint
                  0x029716                  _USBSleepOnSuspend
                  0x019c52                  _USBStallEndpoint
                  0x019b18                  _USBTransferOnePacket
                  0x005590                  _USB_CD_Ptr
                  0x005592                  _USB_SD_Ptr
                  0x01d178                  _USB_enqMsg
                  0x020766                  _USER_USB_CALLBACK_EVENT_HANDLER
                  0x027fe4                  _US_Init
                  0x027fee                  _US_RunUserInitStateMachine
                  0x0281fc                  _US_SetSwitch1
                  0x02820e                  _US_SetSwitch2
                  0x01da8c                  _UpdateB40ADI
                  0x0122f0                  _ValEntTOR
                  0x00b8bc                  _ValidationCodeMetrologie
                  0x024ef0                  _Wait_Flash_Ready
                  0x01d016                  _WritePHYReg
                  0x000876                  _WriteSPI1
                  0x000888                  _WriteSPI3
                  0x024f00                  _Write_Flash
                  0x0269ee                  _XEEBeginRead
                  0x026b12                  _XEEBeginWrite
                  0x026a4a                  _XEEEndRead
                  0x026b9a                  _XEEEndWrite
                  0x0269d0                  _XEEInit
                  0x026c94                  _XEEIsBusy
                  0x026a06                  _XEERead
                  0x026a54                  _XEEReadArray
                  0x026b2a                  _XEEWrite
                  0x026b6c                  _XEEWriteArray
                  0x00075e                  __AddressError
                  0x000714                  __C1Interrupt
                  0x00057e                  __DMA0Interrupt
                  0x000770                  __DMACError
                  0x000776                  __DefaultInterrupt
                  0x00077a                  __HardTrapError
                  0x000622                  __INT1Interrupt
                  0x00065c                  __INT2Interrupt
                  0x000678                  __INT3Interrupt
                  0x0006be                  __INT4Interrupt
                  0x00076a                  __MathError
                  0x000758                  __OscillatorFail
                  0x00077e                  __SoftTrapError
                  0x000764                  __StackError
                  0x028f46                  __T1Interrupt
                  0x000356                  __U1RXInterrupt
                  0x0003e0                  __U2RXInterrupt
                  0x00046a                  __U3RXInterrupt
                  0x0004f4                  __U4RXInterrupt
                  0x0006ec                  __USB1Interrupt
                  0x00383a                  ___adddf3
                  0x000b92                  ___addsf3
                  0x003948                  ___divdf3
                  0x003e66                  ___divdi3
                  0x000c4c                  ___divsf3
                  0x000cd0                  ___divsi3
                  0x003934                  ___eqdf2
                  0x000cee                  ___eqsf2
                  0x003a90                  ___extendsfdf2
                  0x000cf6                  ___fixsfsi
                  0x003ace                  ___fixunsdfdi
                  0x003b30                  ___fixunsdfsi
                  0x000d38                  ___fixunssfsi
                  0x000ee2                  ___floatdisf
                  0x000d6e                  ___floatsisf
                  0x003b7c                  ___floatundidf
                  0x000f02                  ___floatundisf
                  0x003bd2                  ___floatunsidf
                  0x000d74                  ___floatunsisf
                  0x00393e                  ___gedf2
                  0x000cf2                  ___gesf2
                  0x00393e                  ___gtdf2
                  0x000cf2                  ___gtsf2
                  0x003934                  ___ledf2
                  0x000cee                  ___lesf2
                  0x003934                  ___ltdf2
                  0x000cee                  ___ltsf2
                  0x003eca                  ___moddi3
                  0x003c10                  ___muldf3
                  0x003f2a                  ___muldi3
                  0x003cfe                  ___mulp32eds3
                  0x003cfe                  ___mulp32peds3
                  0x000e1e                  ___mulsf3
                  0x003cfe                  ___mulsi3
                  0x0039fc                  ___nedf2
                  0x003cfa                  ___subdf3
                  0x000b90                  ___subsf3
                  0x003e48                  ___udivdi3
                  0x003d78                  ___udivmoddi3
                  0x000e86                  ___udivsi3
                  0x003e5a                  ___umoddi3
                  0x000ea6                  ___umodsi3
                  0x004060                  ___umuldi3
                  0x003fd2                  __dPropagateNaN
                  0x000238                  __data_init
                  0x000238                  __data_init_extended
                  0x003f80                  __dcompare
                  0x003a06                  __dpack
                  0x003a80                  __dreturnNaN
                  0x003fee                  __dtype
                  0x004012                  __dunpack
                  0x003a5e                  __dunpack2
                  0x003a86                  __dunpack2exit
                  0x000dfe                  __fPropagateNaN
                  0x000e10                  __fbopExit
                  0x000e18                  __fbopReturnNaN
                  0x000eac                  __fcompare
                  0x000d78                  __fpack
                  0x000dc4                  __funpack
                  0x000dee                  __funpack2
                  0x0021a2                  __printf_0
                  0x0021a2                  __printf_cdnopsuxX
                  0x0021a2                  __printf_cdnopuxX
                  0x0021a2                  __printf_s
                  0x00022c                  __psv_init
                  0x000200                  __resetPRI
                  0x0013c8                  __sprintf_cdfFnopsuxX
                  0x0013c8                  __sprintf_cdnopsuxX
                  0x0013c8                  __sprintf_cdnopuxX
                  0x001554                  __vfprintf_0
                  0x001554                  __vfprintf_cdfFnopsuxX
                  0x001554                  __vfprintf_cdnopsuxX
                  0x001554                  __vfprintf_cdnopuxX
                  0x001554                  __vfprintf_s
                  0x005598                  _abBitReverseTable16
                  0x01df2e                  _accept
                  0x0257fe                  _app_InstanceCommand
                  0x025a08                  _app_ObjectCommand
                  0x0056a6                  _app_sObject
                  0x00114e                  _atof
                  0x001158                  _atoi
                  0x00119a                  _atol
                  0x01dd72                  _bind
                  0x020d52                  _btohexa_high
                  0x020d74                  _btohexa_low
                  0x01e632                  _closesocket
                  0x005518                  _configDescriptor1
                  0x01e074                  _connect
                  0x013588                  _conversion_poids
                  0x0055a8                  _crc_table32
                  0x005506                  _device_dsc
                  0x02731c                  _dpv1_InstanceCommand
                  0x027478                  _dpv1_ObjectCommand
                  0x0056f4                  _dpv1_sObject
                  0x008580                  _envoieLongPF
                  0x0085e0                  _envoieLongPf
                  0x00860c                  _envoieReelPF
                  0x0086b8                  _envoieReelPf
                  0x013224                  _envoyer_reel
                  0x012d9c                  _etatSortieTOR
                  0x012dd2                  _forcageSortiesTOR
                  0x003bd6                  _frexp
                  0x003bd6                  _frexpl
                  0x011c38                  _gestion_cycle_BI
                  0x0285cc                  _gestion_cycle_BdC
                  0x026968                  _gestion_cycle_Depeseur
                  0x013104                  _gestion_debit
                  0x0119a0                  _gestion_defauts_BI
                  0x012f70                  _gestion_poids
                  0x01131c                  _gestion_profibus
                  0x01270e                  _gestion_totalisateurs
                  0x012328                  _gestion_vitesse
                  0x01e5d0                  _gethostname
                  0x025524                  _getsUSBUSART
                  0x020ce8                  _hexatob
                  0x000782                  _isspace
                  0x01360e                  _lecture_entrees_TOR
                  0x01de12                  _listen
                  0x001244                  _ltoa
                  0x01fe04                  _main
                  0x001268                  _memcmp
                  0x001296                  _memcpy
                  0x0012a8                  _memset
                  0x013302                  _moyenne_glissante_debit
                  0x013326                  _moyenne_glissante_poids
                  0x011548                  _process_plcd
                  0x0255b8                  _putUSBUSART
                  0x0013be                  _putchar
                  0x02563a                  _putrsUSBUSART
                  0x000a88                  _putsUART1
                  0x000ab4                  _putsUART2
                  0x000ae0                  _putsUART3
                  0x000b0c                  _putsUART4
                  0x01d114                  _putsUSB
                  0x0255e4                  _putsUSBUSART
                  0x0012cc                  _rand
                  0x01e3d8                  _recv
                  0x01e470                  _recvfrom
                  0x00555c                  _sd000
                  0x005560                  _sd001
                  0x005578                  _sd002
                  0x01e1f4                  _send
                  0x01e214                  _sendto
                  0x01dcd8                  _socket
                  0x012f20                  _sortiesTOR
                  0x0012f8                  _sprintf
                  0x0012ba                  _srand
                  0x003798                  _strchr
                  0x001322                  _strcmp
                  0x001334                  _strcpy
                  0x003744                  _strcspn
                  0x020d92                  _stricmppgm2ram
                  0x001344                  _strlen
                  0x020fb2                  _strnchr
                  0x001356                  _strncpy
                  0x021000                  _strncpy_m
                  0x00376e                  _strspn
                  0x001146                  _strtod
                  0x000f60                  _strtof
                  0x00137c                  _strtok
                  0x020f28                  _strupr
                  0x020e46                  _swapl
                  0x020e2a                  _swaps
                  0x020c68                  _uitoa
                  0x0011f4                  _ultoa
                  0x012b26                  _verif_totaux
                  0x002312                  _vfprintf
                  0x02976c                  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o:_abcc_RemapRespMsgSent
                  0x02347e                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_drv_WdTimeoutHandler
                  0x023438                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_spi_drv_DataReceived
                  0x0280e4                  build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o:_US_ProcessRespMsg

Memory Configuration

Name             Origin             Length             Attributes
data             0x001000           0x00d000           a !xr
reset            0x000000           0x000004  
ivt              0x000004           0x0001fc  
program          0x000200           0x0555fe           xr
auxflash         0x7fc000           0x003ff8           xr
FGS              0xf80004           0x000002  
FOSCSEL          0xf80006           0x000002  
FOSC             0xf80008           0x000002  
FWDT             0xf8000a           0x000002  
FPOR             0xf8000c           0x000002  
FICD             0xf8000e           0x000002  
FAS              0xf80010           0x000002  
FUID0            0xf80012           0x000002  
*default*        0x000000           0xffffffff  

Linker script and memory map

LOAD build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
LOAD build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
LOAD build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
LOAD build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
LOAD build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
LOAD build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
LOAD build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
LOAD build/XC16_dsPIC33EP512MU810/debug/Regul.o
LOAD build/XC16_dsPIC33EP512MU810/debug/Pesage.o
LOAD build/XC16_dsPIC33EP512MU810/debug/Process.o
LOAD build/XC16_dsPIC33EP512MU810/debug/BdC.o
LOAD build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
LOAD build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
LOAD build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
LOAD build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
LOAD build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
LOAD build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
LOAD build/XC16_dsPIC33EP512MU810/debug/interrupts.o
LOAD build/XC16_dsPIC33EP512MU810/debug/main.o
LOAD build/XC16_dsPIC33EP512MU810/debug/system.o
LOAD build/XC16_dsPIC33EP512MU810/debug/traps.o
LOAD build/XC16_dsPIC33EP512MU810/debug/user.o
LOAD build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
LOAD build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
LOAD build/XC16_dsPIC33EP512MU810/debug/AD7190.o
LOAD build/XC16_dsPIC33EP512MU810/debug/ADComm.o
LOAD build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
LOAD build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
LOAD build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
LOAD build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
LOAD build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
LOAD build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

reserve_data_0x1000
                    0x1000         0x1c
                    0x101c                  . = 0x1c
 *fill*             0x1000         0x1c00

reserve_data_0x101c
                    0x101c          0x2
                    0x101e                  . = 0x2
 *fill*             0x101c          0x200

reserve_data_0x101e
                    0x101e          0x2
                    0x1020                  . = 0x2
 *fill*             0x101e          0x200

reserve_data_0x1020
                    0x1020          0x2
                    0x1022                  . = 0x2
 *fill*             0x1020          0x200

reserve_data_0x1022
                    0x1022          0x2
                    0x1024                  . = 0x2
 *fill*             0x1022          0x200

reserve_data_0x1024
                    0x1024          0x4
                    0x1028                  . = 0x4
 *fill*             0x1024          0x400

reserve_data_0x1028
                    0x1028         0x28
                    0x1050                  . = 0x28
 *fill*             0x1028         0x2800
                    0x0001                  __MPLAB_BUILD = 0x1
                    0x0001                  __MPLAB_DEBUG = 0x1
                    0x0001                  __DEBUG = 0x1
                    0x0001                  __MPLAB_DEBUGGER_PK3 = 0x1
LOAD c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a
                    0xf80004                  __FGS = 0xf80004
                    0xf80006                  __FOSCSEL = 0xf80006
                    0xf80008                  __FOSC = 0xf80008
                    0xf8000a                  __FWDT = 0xf8000a
                    0xf8000c                  __FPOR = 0xf8000c
                    0xf8000e                  __FICD = 0xf8000e
                    0xf80010                  __FAS = 0xf80010
                    0xf80012                  __FUID0 = 0xf80012
                    0x0004                  __IVT_BASE = 0x4
                    0x1000                  __DATA_BASE = 0x1000
                    0xd000                  __DATA_LENGTH = 0xd000
                    0x9000                  __YDATA_BASE = 0x9000
                    0xd000                  __DMA_BASE = 0xd000
                    0xdfff                  __DMA_END = 0xdfff
                    0x7fc000                  __CODE_BASE = 0x7fc000
                    0x3ffa                  __CODE_LENGTH = 0x3ffa

.reset            0x000000          0x4
                  0x000000          0x2 SHORT 0x200 ABSOLUTE (__reset)
                  0x000001          0x2 SHORT 0x4
                  0x000002          0x2 SHORT 0x0 ((ABSOLUTE (__reset) >> 0x10) & 0x7f)
                  0x000003          0x2 SHORT 0x0

.text             0x000200       0x3ea4
 *(.init)
 .init            0x000200         0x38 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(crt0_extendedep.o)
                  0x000200                  __resetPRI
                  0x000200                  __reset
                  0x00022c                  __psv_init
 .init            0x000238         0x9a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(data_init_extendedep.o)
                  0x000238                  __data_init
                  0x000238                  __data_init_extended
 *(.user_init)
 *(.handle)
 .handle          0x0002d2         0x84 jump_table
 *(.isr*)
 .isr.text        0x000356        0x402 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
                  0x000356                  __U1RXInterrupt
                  0x0003e0                  __U2RXInterrupt
                  0x00046a                  __U3RXInterrupt
                  0x0004f4                  __U4RXInterrupt
                  0x00057e                  __DMA0Interrupt
                  0x000622                  __INT1Interrupt
                  0x00065c                  __INT2Interrupt
                  0x000678                  __INT3Interrupt
                  0x0006be                  __INT4Interrupt
                  0x0006ec                  __USB1Interrupt
                  0x000714                  __C1Interrupt
 .isr.text        0x000758         0x2a build/XC16_dsPIC33EP512MU810/debug/traps.o
                  0x000758                  __OscillatorFail
                  0x00075e                  __AddressError
                  0x000764                  __StackError
                  0x00076a                  __MathError
                  0x000770                  __DMACError
                  0x000776                  __DefaultInterrupt
                  0x00077a                  __HardTrapError
                  0x00077e                  __SoftTrapError
 *(.libc)
 .libc            0x000782         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(isspace.epeso)
                  0x000782                  _isspace
 .libc            0x000792         0x60 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(writeep.eo)
                  0x000792                  _write
 *(.libm)
 *(.libdsp)
 *(.lib*)
 .libperi         0x0007f2          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI1.o)
                  0x0007f2                  _CloseSPI1
 .libperi         0x0007fe          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI3.o)
                  0x0007fe                  _CloseSPI3
 .libperi         0x00080a          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI1.o)
                  0x00080a                  _DataRdySPI1
 .libperi         0x000814          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI3.o)
                  0x000814                  _DataRdySPI3
 .libperi         0x00081e          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI1.o)
                  0x00081e                  _OpenSPI1
 .libperi         0x00082a          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI3.o)
                  0x00082a                  _OpenSPI3
 .libperi         0x000836         0x20 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI1.o)
                  0x000836                  _ReadSPI1
 .libperi         0x000856         0x20 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI3.o)
                  0x000856                  _ReadSPI3
 .libperi         0x000876         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI1.o)
                  0x000876                  _WriteSPI1
 .libperi         0x000888         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI3.o)
                  0x000888                  _WriteSPI3
 .libperi         0x00089a          0xe c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART2.o)
                  0x00089a                  _BusyUART2
 .libperi         0x0008a8          0xe c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART3.o)
                  0x0008a8                  _BusyUART3
 .libperi         0x0008b6          0xe c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART4.o)
                  0x0008b6                  _BusyUART4
 .libperi         0x0008c4         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART1.o)
                  0x0008c4                  _CloseUART1
 .libperi         0x0008d4         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART2.o)
                  0x0008d4                  _CloseUART2
 .libperi         0x0008e4         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART3.o)
                  0x0008e4                  _CloseUART3
 .libperi         0x0008f4         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART4.o)
                  0x0008f4                  _CloseUART4
 .libperi         0x000904         0x4c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART1.o)
                  0x000904                  _ConfigIntUART1
 .libperi         0x000950         0x4c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART2.o)
                  0x000950                  _ConfigIntUART2
 .libperi         0x00099c         0x4c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART3.o)
                  0x00099c                  _ConfigIntUART3
 .libperi         0x0009e8         0x48 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART4.o)
                  0x0009e8                  _ConfigIntUART4
 .libperi         0x000a30          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART1.o)
                  0x000a30                  _DataRdyUART1
 .libperi         0x000a3a          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART2.o)
                  0x000a3a                  _DataRdyUART2
 .libperi         0x000a44          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART3.o)
                  0x000a44                  _DataRdyUART3
 .libperi         0x000a4e          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART4.o)
                  0x000a4e                  _DataRdyUART4
 .libperi         0x000a58          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART1.o)
                  0x000a58                  _OpenUART1
 .libperi         0x000a64          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART2.o)
                  0x000a64                  _OpenUART2
 .libperi         0x000a70          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART3.o)
                  0x000a70                  _OpenUART3
 .libperi         0x000a7c          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART4.o)
                  0x000a7c                  _OpenUART4
 .libperi         0x000a88         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART1.o)
                  0x000a88                  _putsUART1
 .libperi         0x000ab4         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART2.o)
                  0x000ab4                  _putsUART2
 .libperi         0x000ae0         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART3.o)
                  0x000ae0                  _putsUART3
 .libperi         0x000b0c         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART4.o)
                  0x000b0c                  _putsUART4
 .libperi         0x000b38         0x16 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART1.o)
                  0x000b38                  _ReadUART1
 .libperi         0x000b4e         0x16 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART2.o)
                  0x000b4e                  _ReadUART2
 .libperi         0x000b64         0x16 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART3.o)
                  0x000b64                  _ReadUART3
 .libperi         0x000b7a         0x16 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART4.o)
                  0x000b7a                  _ReadUART4
 .libm.subsf3     0x000b90         0xbc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo)
                  0x000b90                  ___subsf3
                  0x000b92                  ___addsf3
 .libm.divfs3     0x000c4c         0x84 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsf3.epeo)
                  0x000c4c                  ___divsf3
 .libm.divsi3     0x000cd0         0x1e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsi3.epeo)
                  0x000cd0                  ___divsi3
 .libm.eqsf2      0x000cee          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(feqltle.epeo)
                  0x000cee                  ___eqsf2
                  0x000cee                  ___ltsf2
                  0x000cee                  ___lesf2
 .libm.gtsf2      0x000cf2          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fgtge.epeo)
                  0x000cf2                  ___gesf2
                  0x000cf2                  ___gtsf2
 .libm.fixsfsi    0x000cf6         0x42 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixsfsi.epeo)
                  0x000cf6                  _(float, int, long long, short, float, short, int)
 .libm.fixunssfsi
                  0x000d38         0x36 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunssfsi.epeo)
                  0x000d38                  ___fixunssfsi
 .libm.floatsisf
                  0x000d6e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatsisf.epeo)
                  0x000d6e                  ___floatsisf
 .libm.floatunsisf
                  0x000d74          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsisf.epeo)
                  0x000d74                  ___floatunsisf
 .libm.fpack      0x000d78         0x4c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fpack.epeo)
                  0x000d78                  __fpack
 .libm.funpack    0x000dc4         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack.epeo)
                  0x000dc4                  __funpack
 .libm.funpack2
                  0x000dee         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack2.epeo)
                  0x000dee                  __funpack2
 .libm.fPropagateNaN
                  0x000dfe         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(futil.epeo)
                  0x000dfe                  __fPropagateNaN
 .libm.fbobExit
                  0x000e10          0x8 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(futil.epeo)
                  0x000e10                  __fbopExit
 .libm.fbopReturnNaN
                  0x000e18          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(futil.epeo)
                  0x000e18                  __fbopReturnNaN
 .libm.mulsf3     0x000e1e         0x68 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsf3.epeo)
                  0x000e1e                  ___mulsf3
 .libm.udivsi3    0x000e86         0x20 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(udivsi3.epeo)
                  0x000e86                  ___udivsi3
 .libm.umodsi3    0x000ea6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umodsi3.epeo)
                  0x000ea6                  ___umodsi3
 .libm.fcompare
                  0x000eac         0x36 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fcompare.epeo)
                  0x000eac                  __fcompare
 .libm.floatdisf
                  0x000ee2         0x20 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatdisf.epeo)
                  0x000ee2                  ___floatdisf
 .libm.floatundisf
                  0x000f02         0x5e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundisf.epeo)
                  0x000f02                  ___floatundisf
 .libc.strtof     0x000f60        0x1e6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo)
                  0x000f60                  _strtof
 .libc.strtod     0x001146          0x8 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo)
                  0x001146                  _strtod
 .libc.atof       0x00114e          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo)
                  0x00114e                  _atof
 .libc.atoi       0x001158         0x42 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atoi.epeo)
                  0x001158                  _atoi
 .libc.atol       0x00119a         0x5a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atol.epeo)
                  0x00119a                  _atol
 .libc.ultoa      0x0011f4         0x50 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(ltoa.epeo)
                  0x0011f4                  _ultoa
 .libc.ltoa       0x001244         0x24 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(ltoa.epeo)
                  0x001244                  _ltoa
 .libc.memcmp     0x001268         0x2e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcmp.epeo)
                  0x001268                  _memcmp
 .libc.memcpy     0x001296         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcpy.epeo)
                  0x001296                  _memcpy
 .libc.memset     0x0012a8         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memset.epeo)
                  0x0012a8                  _memset
 .libc.srand      0x0012ba         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)
                  0x0012ba                  _srand
 .libc.rand       0x0012cc         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)
                  0x0012cc                  _rand
 .libc.sprintf    0x0012f8         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf.epeo)
                  0x0012f8                  _sprintf
 .libc.strcmp     0x001322         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcmp.epeo)
                  0x001322                  _strcmp
 .libc.strcpy     0x001334         0x10 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcpy.epeo)
                  0x001334                  _strcpy
 .libc.strlen     0x001344         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strlen.epeo)
                  0x001344                  _strlen
 .libc.strncpy    0x001356         0x26 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strncpy.epeo)
                  0x001356                  _strncpy
 .libc.strtok     0x00137c         0x42 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo)
                  0x00137c                  _strtok
 .libc.putchar    0x0013be          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(putchar.epeo)
                  0x0013be                  _putchar
 .libc._sprintf_cdfFnopsuxX
                  0x0013c8         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdfFnopsuxX.EPeo)
                  0x0013c8                  __sprintf_cdfFnopsuxX
                  0x0013c8                  __sprintf_cdnopuxX
                  0x0013c8                  __sprintf_cdnopsuxX
 .libc.fround     0x0013f2         0xaa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
 .libc.scale      0x00149c         0xb8 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
 .libc._vfprintf_cdfFnopsuxX
                  0x001554        0xc4e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
                  0x001554                  __vfprintf_cdfFnopsuxX
                  0x001554                  __vfprintf_cdnopuxX
                  0x001554                  __vfprintf_cdnopsuxX
                  0x001554                  __vfprintf_0
                  0x001554                  __vfprintf_s
 .libc._printf_cdnopsuxX
                  0x0021a2          0xe c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_cdnopsuxX.EPeo)
                  0x0021a2                  __printf_0
                  0x0021a2                  __printf_s
                  0x0021a2                  __printf_cdnopuxX
                  0x0021a2                  __printf_cdnopsuxX
 .libc.fround     0x0021b0         0xaa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)
 .libc.scale      0x00225a         0xb8 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)
 .libc.vfprintf
                  0x002312       0x13a6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)
                  0x002312                  _vfprintf
 .libc.fputc      0x0036b8         0x8c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(fputc.epeo)
                  0x0036b8                  _fputc
 .libc.strcspn    0x003744         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcspn.epeo)
                  0x003744                  _strcspn
 .libc.strspn     0x00376e         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strspn.epeo)
                  0x00376e                  _strspn
 .libc.strchr     0x003798         0x1a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strchr.epelo)
                  0x003798                  _strchr
 .libc._flsbuf    0x0037b2         0x80 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(flsbuf.epeo)
                  0x0037b2                  __flsbuf
 .libc.dowrite    0x003832          0x8 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(writeep.eo)
 .libm.adddf3     0x00383a         0xfa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(adddf3.epeo)
                  0x00383a                  ___adddf3
 .libm.eqdf2      0x003934          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(deqltle.epeo)
                  0x003934                  ___eqdf2
                  0x003934                  ___ltdf2
                  0x003934                  ___ledf2
 .libm.gtdf2      0x00393e          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dgtge.epeo)
                  0x00393e                  ___gtdf2
                  0x00393e                  ___gedf2
 .libm.divdf3     0x003948         0xb4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divdf3.epeo)
                  0x003948                  ___divdf3
 .libm.nedf2      0x0039fc          0xa c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dne.epeo)
                  0x0039fc                  ___nedf2
 .libm.dpack      0x003a06         0x58 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpack.epeo)
                  0x003a06                  __dpack
 .libm.dunpack2
                  0x003a5e         0x32 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack2.epeo)
                  0x003a5e                  __dunpack2
                  0x003a80                  __dreturnNaN
                  0x003a86                  __dunpack2exit
 .libm.extendsfdf2
                  0x003a90         0x3e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(extendsfdf.epeo)
                  0x003a90                  ___extendsfdf2
 .libm.fixunsdfdi
                  0x003ace         0x62 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfdi.epeo)
                  0x003ace                  ___fixunsdfdi
 .libm.fixunsdfsi
                  0x003b30         0x4c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfsi.epeo)
                  0x003b30                  ___fixunsdfsi
 .libm.floatundidf
                  0x003b7c         0x56 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundidf.epeo)
                  0x003b7c                  ___floatundidf
 .libm.floatunsidf
                  0x003bd2          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsidf.epeo)
                  0x003bd2                  ___floatunsidf
 .libm.frexp      0x003bd6         0x3a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(frexp.epeo)
                  0x003bd6                  _frexp
                  0x003bd6                  _frexpl
 .libm.muldf3     0x003c10         0xea c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldf3.epeo)
                  0x003c10                  ___muldf3
 .libm.subdf3     0x003cfa          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(subdf3.epeo)
                  0x003cfa                  ___subdf3
 .libm.mulsi3     0x003cfe          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsi3.epeo)
                  0x003cfe                  ___mulp32peds3
                  0x003cfe                  ___mulsi3
                  0x003cfe                  ___mulp32eds3
 .libm.__PplusBdi
                  0x003d0a         0x2c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
 .libm.__PminusBdi
                  0x003d36         0x42 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
 .libm.__udivmoddi3
                  0x003d78         0xd0 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                  0x003d78                  ___udivmoddi3
 .libm.__udivdi3
                  0x003e48         0x12 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                  0x003e48                  ___udivdi3
 .libm.__umoddi3
                  0x003e5a          0xc c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                  0x003e5a                  ___umoddi3
 .libm.__divdi3
                  0x003e66         0x64 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                  0x003e66                  ___divdi3
 .libm.__moddi3
                  0x003eca         0x60 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
                  0x003eca                  ___moddi3
 .libm.__muldi3
                  0x003f2a         0x56 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldi3.epeo)
                  0x003f2a                  ___muldi3
 .libm.dcompare
                  0x003f80         0x52 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dcompare.epeo)
                  0x003f80                  __dcompare
 .libm.dPropagateNaN
                  0x003fd2         0x1c c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpropagateNaN.epeo)
                  0x003fd2                  __dPropagateNaN
 .libm.dtype      0x003fee         0x24 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dtype.epeo)
                  0x003fee                  __dtype
 .libm.dunpack    0x004012         0x4e c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack.epeo)
                  0x004012                  __dunpack
 .libm.umuldi3    0x004060         0x44 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umuldi3.epeo)
                  0x004060                  ___umuldi3

usercode
 *(usercode)

__FGS
 *(__FGS.sec*)

__FOSCSEL
 *(__FOSCSEL.sec*)

__FOSC
 *(__FOSC.sec*)

__FWDT
 *(__FWDT.sec*)

__FPOR
 *(__FPOR.sec*)

__FICD
 *(__FICD.sec*)

__FAS
 *(__FAS.sec*)

__FUID0
 *(__FUID0.sec*)

.comment
 *(.comment)

.debug_info       0x000000      0x4d342
 *(.debug_info)
 .debug_info      0x000000        0x14a build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
 .debug_info      0x00014a        0x146 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
 .debug_info      0x000290        0x266 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_info      0x0004f6        0x626 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_info      0x000b1c       0x134c build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_info      0x001e68       0x1122 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_info      0x002f8a        0x4de build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_info      0x003468       0x1693 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_info      0x004afb        0xfa5 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_info      0x005aa0        0x2ed build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_info      0x005d8d        0x3f1 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_info      0x00617e       0x1195 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_info      0x007313        0xe3f build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_info      0x008152        0x756 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_info      0x0088a8       0x1638 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_info      0x009ee0        0x91a build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_info      0x00a7fa        0x920 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_info      0x00b11a        0xb68 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_info      0x00bc82        0x487 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_info      0x00c109       0x2154 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_info      0x00e25d        0xae8 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_info      0x00ed45       0x1388 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_info      0x0100cd        0xb7f build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_info      0x010c4c        0x5e7 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_info      0x011233       0x1fa9 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_info      0x0131dc       0x2532 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_info      0x01570e       0x4c81 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_info      0x01a38f       0x2523 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_info      0x01c8b2       0x25d9 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_info      0x01ee8b        0xb33 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_info      0x01f9be        0x13b build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
 .debug_info      0x01faf9        0xb63 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_info      0x02065c        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
 .debug_info      0x020796       0x1466 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_info      0x021bfc        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
 .debug_info      0x021d36        0x1ce build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_info      0x021f04        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
 .debug_info      0x02203c        0x139 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
 .debug_info      0x022175        0xd85 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_info      0x022efa        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
 .debug_info      0x023032        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
 .debug_info      0x02316c       0x2d29 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_info      0x025e95        0x13e build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
 .debug_info      0x025fd3        0x137 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
 .debug_info      0x02610a        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
 .debug_info      0x026244       0x1068 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_info      0x0272ac       0x1305 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_info      0x0285b1        0xac9 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_info      0x02907a        0xb16 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_info      0x029b90        0x13f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
 .debug_info      0x029ccf        0xe2f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_info      0x02aafe        0xc6a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_info      0x02b768        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
 .debug_info      0x02b8a2        0xa51 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_info      0x02c2f3        0x137 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
 .debug_info      0x02c42a        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
 .debug_info      0x02c562        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
 .debug_info      0x02c69a        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
 .debug_info      0x02c7d4        0x13d build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
 .debug_info      0x02c911        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
 .debug_info      0x02ca49       0x1072 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_info      0x02dabb        0x13c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
 .debug_info      0x02dbf7        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
 .debug_info      0x02dd31        0x137 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
 .debug_info      0x02de68        0x9e1 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_info      0x02e849       0x21dc build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_info      0x030a25        0x146 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
 .debug_info      0x030b6b        0x13a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
 .debug_info      0x030ca5        0x139 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
 .debug_info      0x030dde        0xb0e build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_info      0x0318ec        0x138 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
 .debug_info      0x031a24        0x142 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
 .debug_info      0x031b66       0x11e4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_info      0x032d4a        0x146 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
 .debug_info      0x032e90        0x142 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
 .debug_info      0x032fd2        0x145 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
 .debug_info      0x033117        0x148 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
 .debug_info      0x03325f       0x2a14 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_info      0x035c73       0x1620 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_info      0x037293        0x5d4 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_info      0x037867         0x9d build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
 .debug_info      0x037904       0x21b7 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_info      0x039abb       0x661f build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_info      0x0400da        0x895 build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_info      0x04096f        0x37a build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_info      0x040ce9       0x1a11 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_info      0x0426fa         0x6e build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
 .debug_info      0x042768       0x1be7 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_info      0x04434f        0xb87 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_info      0x044ed6        0x50c build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_info      0x0453e2       0x1be5 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_info      0x046fc7        0xb81 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_info      0x047b48       0x115b build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_info      0x048ca3        0xf7a build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_info      0x049c1d        0x7b9 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_info      0x04a3d6       0x2f6c build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o
 *(.gnu.linkonce.wi.*)

.debug_abbrev     0x000000       0x67ae
 *(.debug_abbrev)
 .debug_abbrev    0x000000         0x1f build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
 .debug_abbrev    0x00001f         0x1f build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
 .debug_abbrev    0x00003e         0xa7 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_abbrev    0x0000e5         0xce build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_abbrev    0x0001b3        0x214 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_abbrev    0x0003c7        0x1ac build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_abbrev    0x000573         0x7b build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_abbrev    0x0005ee        0x260 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_abbrev    0x00084e        0x250 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_abbrev    0x000a9e         0xc0 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_abbrev    0x000b5e         0xe8 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_abbrev    0x000c46        0x208 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_abbrev    0x000e4e        0x151 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_abbrev    0x000f9f        0x143 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_abbrev    0x0010e2        0x290 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_abbrev    0x001372        0x153 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_abbrev    0x0014c5        0x15e build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_abbrev    0x001623        0x14c build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_abbrev    0x00176f        0x13e build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_abbrev    0x0018ad        0x1b1 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_abbrev    0x001a5e        0x145 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_abbrev    0x001ba3        0x151 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_abbrev    0x001cf4        0x154 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_abbrev    0x001e48        0x15e build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_abbrev    0x001fa6         0xcf build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_abbrev    0x002075         0xe6 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_abbrev    0x00215b        0x353 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_abbrev    0x0024ae         0xdf build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_abbrev    0x00258d         0xf7 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_abbrev    0x002684        0x159 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_abbrev    0x0027dd         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
 .debug_abbrev    0x0027fc        0x1cb build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_abbrev    0x0029c7         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
 .debug_abbrev    0x0029e6        0x236 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_abbrev    0x002c1c         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
 .debug_abbrev    0x002c3b         0x68 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_abbrev    0x002ca3         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
 .debug_abbrev    0x002cc2         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
 .debug_abbrev    0x002ce1        0x1db build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_abbrev    0x002ebc         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
 .debug_abbrev    0x002edb         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
 .debug_abbrev    0x002efa        0x2b5 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_abbrev    0x0031af         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
 .debug_abbrev    0x0031ce         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
 .debug_abbrev    0x0031ed         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
 .debug_abbrev    0x00320c        0x1aa build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_abbrev    0x0033b6        0x225 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_abbrev    0x0035db        0x19f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_abbrev    0x00377a        0x198 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_abbrev    0x003912         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
 .debug_abbrev    0x003931        0x1eb build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_abbrev    0x003b1c        0x1aa build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_abbrev    0x003cc6         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
 .debug_abbrev    0x003ce5        0x134 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_abbrev    0x003e19         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
 .debug_abbrev    0x003e38         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
 .debug_abbrev    0x003e57         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
 .debug_abbrev    0x003e76         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
 .debug_abbrev    0x003e95         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
 .debug_abbrev    0x003eb4         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
 .debug_abbrev    0x003ed3        0x214 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_abbrev    0x0040e7         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
 .debug_abbrev    0x004106         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
 .debug_abbrev    0x004125         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
 .debug_abbrev    0x004144        0x158 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_abbrev    0x00429c        0x246 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_abbrev    0x0044e2         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
 .debug_abbrev    0x004501         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
 .debug_abbrev    0x004520         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
 .debug_abbrev    0x00453f        0x15f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_abbrev    0x00469e         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
 .debug_abbrev    0x0046bd         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
 .debug_abbrev    0x0046dc        0x258 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_abbrev    0x004934         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
 .debug_abbrev    0x004953         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
 .debug_abbrev    0x004972         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
 .debug_abbrev    0x004991         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
 .debug_abbrev    0x0049b0        0x2bc build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_abbrev    0x004c6c        0x25f build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_abbrev    0x004ecb         0xa1 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_abbrev    0x004f6c         0x1f build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
 .debug_abbrev    0x004f8b        0x1a4 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_abbrev    0x00512f        0x2d4 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_abbrev    0x005403         0xb8 build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_abbrev    0x0054bb         0x7d build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_abbrev    0x005538        0x2aa build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_abbrev    0x0057e2         0x10 build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
 .debug_abbrev    0x0057f2        0x257 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_abbrev    0x005a49        0x196 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_abbrev    0x005bdf        0x118 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_abbrev    0x005cf7        0x21e build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_abbrev    0x005f15        0x1ec build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_abbrev    0x006101        0x150 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_abbrev    0x006251        0x214 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_abbrev    0x006465        0x102 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_abbrev    0x006567        0x247 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.debug_line       0x000000      0x1b742
 *(.debug_line)
 .debug_line      0x000000         0x24 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
 .debug_line      0x000024         0x24 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
 .debug_line      0x000048        0x13f build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_line      0x000187        0x190 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_line      0x000317        0x980 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_line      0x000c97        0x283 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_line      0x000f1a         0x79 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_line      0x000f93        0x9d2 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_line      0x001965        0x709 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_line      0x00206e        0x169 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_line      0x0021d7         0xde build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_line      0x0022b5        0x695 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_line      0x00294a        0x369 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_line      0x002cb3        0x277 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_line      0x002f2a        0xfde build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_line      0x003f08        0x30c build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_line      0x004214        0x228 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_line      0x00443c         0xe6 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_line      0x004522        0x357 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_line      0x004879        0x45e build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_line      0x004cd7        0x249 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_line      0x004f20        0x362 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_line      0x005282        0x2dc build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_line      0x00555e        0x217 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_line      0x005775        0x188 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_line      0x0058fd        0xc2f build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_line      0x00652c       0x2097 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_line      0x0085c3        0x1c4 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_line      0x008787        0x391 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_line      0x008b18        0x25b build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_line      0x008d73         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
 .debug_line      0x008d97        0x3e5 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_line      0x00917c         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
 .debug_line      0x0091a0        0xb3a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_line      0x009cda         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
 .debug_line      0x009cfe        0x106 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_line      0x009e04         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
 .debug_line      0x009e28         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
 .debug_line      0x009e4c        0x7f7 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_line      0x00a643         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
 .debug_line      0x00a667         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
 .debug_line      0x00a68b       0x1285 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_line      0x00b910         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
 .debug_line      0x00b934         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
 .debug_line      0x00b958         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
 .debug_line      0x00b97c        0xade build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_line      0x00c45a       0x14bf build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_line      0x00d919        0x427 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_line      0x00dd40        0x249 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_line      0x00df89         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
 .debug_line      0x00dfad        0x94b build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_line      0x00e8f8        0x3cd build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_line      0x00ecc5         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
 .debug_line      0x00ece9        0x185 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_line      0x00ee6e         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
 .debug_line      0x00ee92         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
 .debug_line      0x00eeb6         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
 .debug_line      0x00eeda         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
 .debug_line      0x00eefe         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
 .debug_line      0x00ef22         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
 .debug_line      0x00ef46        0x5ab build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_line      0x00f4f1         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
 .debug_line      0x00f515         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
 .debug_line      0x00f539         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
 .debug_line      0x00f55d        0x24d build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_line      0x00f7aa       0x2726 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_line      0x011ed0         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
 .debug_line      0x011ef4         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
 .debug_line      0x011f18         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
 .debug_line      0x011f3c        0x326 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_line      0x012262         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
 .debug_line      0x012286         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
 .debug_line      0x0122aa        0x936 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_line      0x012be0         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
 .debug_line      0x012c04         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
 .debug_line      0x012c28         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
 .debug_line      0x012c4c         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
 .debug_line      0x012c70       0x131a build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_line      0x013f8a        0x5f8 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_line      0x014582        0x144 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_line      0x0146c6         0x24 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
 .debug_line      0x0146ea        0x4f3 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_line      0x014bdd        0xdf0 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_line      0x0159cd        0x11a build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_line      0x015ae7        0x187 build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_line      0x015c6e        0x917 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_line      0x016585         0x50 build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
 .debug_line      0x0165d5        0xb08 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_line      0x0170dd        0x6a3 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_line      0x017780        0x1ce build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_line      0x01794e        0x957 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_line      0x0182a5        0x708 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_line      0x0189ad        0x29b build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_line      0x018c48        0x531 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_line      0x019179         0xbc build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_line      0x019235       0x250d build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.debug_frame      0x000000       0x4300
 *(.debug_frame)
 .debug_frame     0x000000         0x24 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_frame     0x000024         0x50 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_frame     0x000074        0x2e4 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_frame     0x000358        0x138 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_frame     0x000490        0x380 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_frame     0x000810        0x1c8 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_frame     0x0009d8         0x44 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_frame     0x000a1c         0x34 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_frame     0x000a50        0x30c build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_frame     0x000d5c        0x104 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_frame     0x000e60         0x80 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_frame     0x000ee0         0xd4 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_frame     0x000fb4         0x64 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_frame     0x001018         0x44 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_frame     0x00105c         0x44 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_frame     0x0010a0        0x15c build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_frame     0x0011fc         0xc4 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_frame     0x0012c0         0x24 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_frame     0x0012e4         0x34 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_frame     0x001318         0x34 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_frame     0x00134c         0x44 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_frame     0x001390         0x34 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_frame     0x0013c4         0x24 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_frame     0x0013e8        0x5a0 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_frame     0x001988         0x64 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_frame     0x0019ec         0x64 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_frame     0x001a50         0x34 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_frame     0x001a84         0x84 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_frame     0x001b08         0xe4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_frame     0x001bec         0x34 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_frame     0x001c20         0x74 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_frame     0x001c94        0x214 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_frame     0x001ea8        0x124 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_frame     0x001fcc        0x124 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_frame     0x0020f0         0x74 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_frame     0x002164         0x54 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_frame     0x0021b8        0x154 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_frame     0x00230c         0x44 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_frame     0x002350         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_frame     0x002374         0xc4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_frame     0x002438         0x44 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_frame     0x00247c        0x234 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_frame     0x0026b0         0x84 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_frame     0x002734        0x134 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_frame     0x002868        0x1b4 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_frame     0x002a1c         0x94 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_frame     0x002ab0         0x24 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_frame     0x002ad4         0xc4 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_frame     0x002b98         0xc4 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_frame     0x002c5c         0x24 build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_frame     0x002c80         0x94 build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_frame     0x002d14        0x268 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_frame     0x002f7c        0x284 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_frame     0x003200        0x21c build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_frame     0x00341c         0x44 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_frame     0x003460        0x114 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_frame     0x003574        0x124 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_frame     0x003698         0x54 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_frame     0x0036ec         0xb4 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_frame     0x0037a0        0xb60 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.debug_str        0x000000       0x25ab
 *(.debug_str)
 .debug_str       0x000000         0x20 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_str       0x000020         0x67 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_str       0x000087         0xb8 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_str       0x00013f        0x16d build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_str       0x0002ac         0x25 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_str       0x0002d1        0x2ce build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_str       0x00059f        0x154 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_str       0x0006f3          0xd build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_str       0x000700         0x1e build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_str       0x00071e        0x1ce build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_str       0x0008ec         0x71 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_str       0x00095d         0x61 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_str       0x0009be        0x225 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_str       0x000be3         0x97 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_str       0x000c7a         0x68 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_str       0x000ce2        0x1c8 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_str       0x000eaa         0x54 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_str       0x000efe        0x16d build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_str       0x00106b          0xa build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_str       0x001075         0x14 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_str       0x001089         0x23 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_str       0x0010ac         0x50 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_str       0x0010fc         0x50 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_str       0x00114c        0x2ae build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_str       0x0013fa         0x50 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_str       0x00144a         0x5a build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_str       0x0014a4         0x2c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_str       0x0014d0         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_str       0x0014e8         0x5a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_str       0x001542          0xa build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_str       0x00154c         0xbf build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_str       0x00160b          0x9 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_str       0x001614         0x2c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_str       0x001640         0x13 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_str       0x001653         0x11 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_str       0x001664         0x23 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_str       0x001687         0x1e build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_str       0x0016a5         0x64 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_str       0x001709         0x15 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_str       0x00171e         0xcb build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_str       0x0017e9         0x25 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_str       0x00180e         0x7f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_str       0x00188d        0x290 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_str       0x001b1d         0xde build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_str       0x001bfb         0x1e build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_str       0x001c19        0x10b build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_str       0x001d24        0x2e1 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_str       0x002005         0x3e build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_str       0x002043          0xc build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_str       0x00204f         0xf6 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_str       0x002145         0x61 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_str       0x0021a6         0x7b build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_str       0x002221         0x58 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_str       0x002279         0xdf build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_str       0x002358         0x65 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_str       0x0023bd         0x9b build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_str       0x002458         0x5a build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_str       0x0024b2         0x2a build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_str       0x0024dc         0xcf build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.debug_loc
 *(.debug_loc)

.debug_macinfo
 *(.debug_macinfo)

.debug_pubnames
                  0x000000       0x3c91
 *(.debug_pubnames)
 .debug_pubnames
                  0x000000         0x48 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_pubnames
                  0x000048         0x38 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_pubnames
                  0x000080        0x286 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_pubnames
                  0x000306        0x126 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_pubnames
                  0x00042c         0x24 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_pubnames
                  0x000450        0x598 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_pubnames
                  0x0009e8        0x157 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_pubnames
                  0x000b3f         0x4c build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_pubnames
                  0x000b8b         0x2c build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_pubnames
                  0x000bb7         0xc8 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_pubnames
                  0x000c7f        0x1d9 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_pubnames
                  0x000e58         0x74 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_pubnames
                  0x000ecc        0x117 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_pubnames
                  0x000fe3         0xc4 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_pubnames
                  0x0010a7         0x7c build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_pubnames
                  0x001123        0x125 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_pubnames
                  0x001248         0xa7 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_pubnames
                  0x0012ef        0x1a8 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_pubnames
                  0x001497         0x28 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_pubnames
                  0x0014bf         0x37 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_pubnames
                  0x0014f6         0x46 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_pubnames
                  0x00153c         0xf2 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_pubnames
                  0x00162e         0x39 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_pubnames
                  0x001667         0x29 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_pubnames
                  0x001690        0x2d6 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_pubnames
                  0x001966         0x7b build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_pubnames
                  0x0019e1         0x7f build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_pubnames
                  0x001a60         0x33 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_pubnames
                  0x001a93         0x6f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_pubnames
                  0x001b02         0xa9 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_pubnames
                  0x001bab         0x2c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_pubnames
                  0x001bd7         0x55 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_pubnames
                  0x001c2c        0x1b8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_pubnames
                  0x001de4        0x11b build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_pubnames
                  0x001eff         0xcf build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_pubnames
                  0x001fce         0x7f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_pubnames
                  0x00204d         0x44 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_pubnames
                  0x002091        0x140 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_pubnames
                  0x0021d1         0x1f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_pubnames
                  0x0021f0         0x21 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_pubnames
                  0x002211         0xaa build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_pubnames
                  0x0022bb         0x53 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_pubnames
                  0x00230e        0x1ba build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_pubnames
                  0x0024c8         0x7e build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_pubnames
                  0x002546        0x155 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_pubnames
                  0x00269b        0x33a build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_pubnames
                  0x0029d5        0x1b2 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_pubnames
                  0x002b87         0x28 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_pubnames
                  0x002baf         0xe1 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_pubnames
                  0x002c90        0x159 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_pubnames
                  0x002de9         0x2a build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_pubnames
                  0x002e13         0xa2 build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_pubnames
                  0x002eb5        0x138 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_pubnames
                  0x002fed        0x3bd build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_pubnames
                  0x0033aa        0x186 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_pubnames
                  0x003530         0x6f build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_pubnames
                  0x00359f        0x23b build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_pubnames
                  0x0037da        0x1da build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_pubnames
                  0x0039b4         0x7b build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_pubnames
                  0x003a2f         0xa4 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_pubnames
                  0x003ad3         0x73 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_pubnames
                  0x003b46        0x14b build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.debug_ranges
 *(.debug_ranges)

.debug_aranges    0x000000        0x5c0
 *(.debug_aranges)
 .debug_aranges
                  0x000000         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_aranges
                  0x000018         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_aranges
                  0x000030         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_aranges
                  0x000048         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_aranges
                  0x000060         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_aranges
                  0x000078         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_aranges
                  0x000090         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_aranges
                  0x0000a8         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_aranges
                  0x0000c0         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_aranges
                  0x0000d8         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_aranges
                  0x0000f0         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_aranges
                  0x000108         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_aranges
                  0x000120         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_aranges
                  0x000138         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_aranges
                  0x000150         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_aranges
                  0x000168         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_aranges
                  0x000180         0x18 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_aranges
                  0x000198         0x18 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_aranges
                  0x0001b0         0x18 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_aranges
                  0x0001c8         0x18 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_aranges
                  0x0001e0         0x18 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_aranges
                  0x0001f8         0x18 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_aranges
                  0x000210         0x18 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_aranges
                  0x000228         0x18 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_aranges
                  0x000240         0x18 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_aranges
                  0x000258         0x18 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_aranges
                  0x000270         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_aranges
                  0x000288         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_aranges
                  0x0002a0         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_aranges
                  0x0002b8         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_aranges
                  0x0002d0         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_aranges
                  0x0002e8         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_aranges
                  0x000300         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_aranges
                  0x000318         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_aranges
                  0x000330         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_aranges
                  0x000348         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_aranges
                  0x000360         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_aranges
                  0x000378         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_aranges
                  0x000390         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_aranges
                  0x0003a8         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_aranges
                  0x0003c0         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_aranges
                  0x0003d8         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_aranges
                  0x0003f0         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_aranges
                  0x000408         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_aranges
                  0x000420         0x18 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_aranges
                  0x000438         0x18 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_aranges
                  0x000450         0x18 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_aranges
                  0x000468         0x18 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_aranges
                  0x000480         0x18 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_aranges
                  0x000498         0x18 build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_aranges
                  0x0004b0         0x18 build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_aranges
                  0x0004c8         0x18 build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_aranges
                  0x0004e0         0x20 build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
 .debug_aranges
                  0x000500         0x18 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_aranges
                  0x000518         0x18 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_aranges
                  0x000530         0x18 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_aranges
                  0x000548         0x18 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_aranges
                  0x000560         0x18 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_aranges
                  0x000578         0x18 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_aranges
                  0x000590         0x18 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_aranges
                  0x0005a8         0x18 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.ivt              0x000004        0x130
                  0x000004          0x4 LONG 0x758 DEFINED (__OscillatorFail)?ABSOLUTE (__OscillatorFail):ABSOLUTE (__DefaultInterrupt)
                  0x000006          0x4 LONG 0x75e DEFINED (__AddressError)?ABSOLUTE (__AddressError):ABSOLUTE (__DefaultInterrupt)
                  0x000008          0x4 LONG 0x77a DEFINED (__HardTrapError)?ABSOLUTE (__HardTrapError):ABSOLUTE (__DefaultInterrupt)
                  0x00000a          0x4 LONG 0x764 DEFINED (__StackError)?ABSOLUTE (__StackError):ABSOLUTE (__DefaultInterrupt)
                  0x00000c          0x4 LONG 0x76a DEFINED (__MathError)?ABSOLUTE (__MathError):ABSOLUTE (__DefaultInterrupt)
                  0x00000e          0x4 LONG 0x770 DEFINED (__DMACError)?ABSOLUTE (__DMACError):ABSOLUTE (__DefaultInterrupt)
                  0x000010          0x4 LONG 0x77e DEFINED (__SoftTrapError)?ABSOLUTE (__SoftTrapError):ABSOLUTE (__DefaultInterrupt)
                  0x000012          0x4 LONG 0x776 DEFINED (__ReservedTrap7)?ABSOLUTE (__ReservedTrap7):ABSOLUTE (__DefaultInterrupt)
                  0x000014          0x4 LONG 0x776 DEFINED (__INT0Interrupt)?ABSOLUTE (__INT0Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000016          0x4 LONG 0x776 DEFINED (__IC1Interrupt)?ABSOLUTE (__IC1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000018          0x4 LONG 0x776 DEFINED (__OC1Interrupt)?ABSOLUTE (__OC1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00001a          0x4 LONG 0x28f46 DEFINED (__T1Interrupt)?ABSOLUTE (__T1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00001c          0x4 LONG 0x57e DEFINED (__DMA0Interrupt)?ABSOLUTE (__DMA0Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00001e          0x4 LONG 0x776 DEFINED (__IC2Interrupt)?ABSOLUTE (__IC2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000020          0x4 LONG 0x776 DEFINED (__OC2Interrupt)?ABSOLUTE (__OC2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000022          0x4 LONG 0x776 DEFINED (__T2Interrupt)?ABSOLUTE (__T2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000024          0x4 LONG 0x776 DEFINED (__T3Interrupt)?ABSOLUTE (__T3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000026          0x4 LONG 0x776 DEFINED (__SPI1ErrInterrupt)?ABSOLUTE (__SPI1ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000028          0x4 LONG 0x776 DEFINED (__SPI1Interrupt)?ABSOLUTE (__SPI1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00002a          0x4 LONG 0x356 DEFINED (__U1RXInterrupt)?ABSOLUTE (__U1RXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00002c          0x4 LONG 0x776 DEFINED (__U1TXInterrupt)?ABSOLUTE (__U1TXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00002e          0x4 LONG 0x776 DEFINED (__AD1Interrupt)?ABSOLUTE (__AD1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000030          0x4 LONG 0x776 DEFINED (__DMA1Interrupt)?ABSOLUTE (__DMA1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000032          0x4 LONG 0x776 DEFINED (__NVMInterrupt)?ABSOLUTE (__NVMInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000034          0x4 LONG 0x776 DEFINED (__SI2C1Interrupt)?ABSOLUTE (__SI2C1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000036          0x4 LONG 0x776 DEFINED (__MI2C1Interrupt)?ABSOLUTE (__MI2C1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000038          0x4 LONG 0x776 DEFINED (__CM1Interrupt)?ABSOLUTE (__CM1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00003a          0x4 LONG 0x776 DEFINED (__CNInterrupt)?ABSOLUTE (__CNInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00003c          0x4 LONG 0x622 DEFINED (__INT1Interrupt)?ABSOLUTE (__INT1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00003e          0x4 LONG 0x776 DEFINED (__AD2Interrupt)?ABSOLUTE (__AD2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000040          0x4 LONG 0x776 DEFINED (__IC7Interrupt)?ABSOLUTE (__IC7Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000042          0x4 LONG 0x776 DEFINED (__IC8Interrupt)?ABSOLUTE (__IC8Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000044          0x4 LONG 0x776 DEFINED (__DMA2Interrupt)?ABSOLUTE (__DMA2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000046          0x4 LONG 0x776 DEFINED (__OC3Interrupt)?ABSOLUTE (__OC3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000048          0x4 LONG 0x776 DEFINED (__OC4Interrupt)?ABSOLUTE (__OC4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00004a          0x4 LONG 0x776 DEFINED (__T4Interrupt)?ABSOLUTE (__T4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00004c          0x4 LONG 0x776 DEFINED (__T5Interrupt)?ABSOLUTE (__T5Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00004e          0x4 LONG 0x65c DEFINED (__INT2Interrupt)?ABSOLUTE (__INT2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000050          0x4 LONG 0x3e0 DEFINED (__U2RXInterrupt)?ABSOLUTE (__U2RXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000052          0x4 LONG 0x776 DEFINED (__U2TXInterrupt)?ABSOLUTE (__U2TXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000054          0x4 LONG 0x776 DEFINED (__SPI2ErrInterrupt)?ABSOLUTE (__SPI2ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000056          0x4 LONG 0x776 DEFINED (__SPI2Interrupt)?ABSOLUTE (__SPI2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000058          0x4 LONG 0x776 DEFINED (__C1RxRdyInterrupt)?ABSOLUTE (__C1RxRdyInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00005a          0x4 LONG 0x714 DEFINED (__C1Interrupt)?ABSOLUTE (__C1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00005c          0x4 LONG 0x776 DEFINED (__DMA3Interrupt)?ABSOLUTE (__DMA3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00005e          0x4 LONG 0x776 DEFINED (__IC3Interrupt)?ABSOLUTE (__IC3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000060          0x4 LONG 0x776 DEFINED (__IC4Interrupt)?ABSOLUTE (__IC4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000062          0x4 LONG 0x776 DEFINED (__IC5Interrupt)?ABSOLUTE (__IC5Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000064          0x4 LONG 0x776 DEFINED (__IC6Interrupt)?ABSOLUTE (__IC6Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000066          0x4 LONG 0x776 DEFINED (__OC5Interrupt)?ABSOLUTE (__OC5Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000068          0x4 LONG 0x776 DEFINED (__OC6Interrupt)?ABSOLUTE (__OC6Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00006a          0x4 LONG 0x776 DEFINED (__OC7Interrupt)?ABSOLUTE (__OC7Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00006c          0x4 LONG 0x776 DEFINED (__OC8Interrupt)?ABSOLUTE (__OC8Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00006e          0x4 LONG 0x776 DEFINED (__PMPInterrupt)?ABSOLUTE (__PMPInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000070          0x4 LONG 0x776 DEFINED (__DMA4Interrupt)?ABSOLUTE (__DMA4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000072          0x4 LONG 0x776 DEFINED (__T6Interrupt)?ABSOLUTE (__T6Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000074          0x4 LONG 0x776 DEFINED (__T7Interrupt)?ABSOLUTE (__T7Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000076          0x4 LONG 0x776 DEFINED (__SI2C2Interrupt)?ABSOLUTE (__SI2C2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000078          0x4 LONG 0x776 DEFINED (__MI2C2Interrupt)?ABSOLUTE (__MI2C2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00007a          0x4 LONG 0x776 DEFINED (__T8Interrupt)?ABSOLUTE (__T8Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00007c          0x4 LONG 0x776 DEFINED (__T9Interrupt)?ABSOLUTE (__T9Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00007e          0x4 LONG 0x678 DEFINED (__INT3Interrupt)?ABSOLUTE (__INT3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000080          0x4 LONG 0x6be DEFINED (__INT4Interrupt)?ABSOLUTE (__INT4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000082          0x4 LONG 0x776 DEFINED (__C2RxRdyInterrupt)?ABSOLUTE (__C2RxRdyInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000084          0x4 LONG 0x776 DEFINED (__C2Interrupt)?ABSOLUTE (__C2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000086          0x4 LONG 0x776 DEFINED (__PWMSpEventMatchInterrupt)?ABSOLUTE (__PWMSpEventMatchInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000088          0x4 LONG 0x776 DEFINED (__QEI1Interrupt)?ABSOLUTE (__QEI1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00008a          0x4 LONG 0x776 DEFINED (__DCIEInterrupt)?ABSOLUTE (__DCIEInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00008c          0x4 LONG 0x776 DEFINED (__DCIInterrupt)?ABSOLUTE (__DCIInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00008e          0x4 LONG 0x776 DEFINED (__DMA5Interrupt)?ABSOLUTE (__DMA5Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000090          0x4 LONG 0x776 DEFINED (__RTCCInterrupt)?ABSOLUTE (__RTCCInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000092          0x4 LONG 0x776 DEFINED (__Interrupt63)?ABSOLUTE (__Interrupt63):ABSOLUTE (__DefaultInterrupt)
                  0x000094          0x4 LONG 0x776 DEFINED (__Interrupt64)?ABSOLUTE (__Interrupt64):ABSOLUTE (__DefaultInterrupt)
                  0x000096          0x4 LONG 0x776 DEFINED (__U1ErrInterrupt)?ABSOLUTE (__U1ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000098          0x4 LONG 0x776 DEFINED (__U2ErrInterrupt)?ABSOLUTE (__U2ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00009a          0x4 LONG 0x776 DEFINED (__CRCInterrupt)?ABSOLUTE (__CRCInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00009c          0x4 LONG 0x776 DEFINED (__DMA6Interrupt)?ABSOLUTE (__DMA6Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00009e          0x4 LONG 0x776 DEFINED (__DMA7Interrupt)?ABSOLUTE (__DMA7Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000a0          0x4 LONG 0x776 DEFINED (__C1TxReqInterrupt)?ABSOLUTE (__C1TxReqInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000a2          0x4 LONG 0x776 DEFINED (__C2TxReqInterrupt)?ABSOLUTE (__C2TxReqInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000a4          0x4 LONG 0x776 DEFINED (__Interrupt72)?ABSOLUTE (__Interrupt72):ABSOLUTE (__DefaultInterrupt)
                  0x0000a6          0x4 LONG 0x776 DEFINED (__PWMSecSpEventMatchInterrupt)?ABSOLUTE (__PWMSecSpEventMatchInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000a8          0x4 LONG 0x776 DEFINED (__Interrupt74)?ABSOLUTE (__Interrupt74):ABSOLUTE (__DefaultInterrupt)
                  0x0000aa          0x4 LONG 0x776 DEFINED (__QEI2Interrupt)?ABSOLUTE (__QEI2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000ac          0x4 LONG 0x776 DEFINED (__Interrupt76)?ABSOLUTE (__Interrupt76):ABSOLUTE (__DefaultInterrupt)
                  0x0000ae          0x4 LONG 0x776 DEFINED (__Interrupt77)?ABSOLUTE (__Interrupt77):ABSOLUTE (__DefaultInterrupt)
                  0x0000b0          0x4 LONG 0x776 DEFINED (__Interrupt78)?ABSOLUTE (__Interrupt78):ABSOLUTE (__DefaultInterrupt)
                  0x0000b2          0x4 LONG 0x776 DEFINED (__Interrupt79)?ABSOLUTE (__Interrupt79):ABSOLUTE (__DefaultInterrupt)
                  0x0000b4          0x4 LONG 0x776 DEFINED (__Interrupt80)?ABSOLUTE (__Interrupt80):ABSOLUTE (__DefaultInterrupt)
                  0x0000b6          0x4 LONG 0x776 DEFINED (__U3ErrInterrupt)?ABSOLUTE (__U3ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000b8          0x4 LONG 0x46a DEFINED (__U3RXInterrupt)?ABSOLUTE (__U3RXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000ba          0x4 LONG 0x776 DEFINED (__U3TXInterrupt)?ABSOLUTE (__U3TXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000bc          0x4 LONG 0x776 DEFINED (__Interrupt84)?ABSOLUTE (__Interrupt84):ABSOLUTE (__DefaultInterrupt)
                  0x0000be          0x4 LONG 0x776 DEFINED (__Interrupt85)?ABSOLUTE (__Interrupt85):ABSOLUTE (__DefaultInterrupt)
                  0x0000c0          0x4 LONG 0x6ec DEFINED (__USB1Interrupt)?ABSOLUTE (__USB1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000c2          0x4 LONG 0x776 DEFINED (__U4ErrInterrupt)?ABSOLUTE (__U4ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000c4          0x4 LONG 0x4f4 DEFINED (__U4RXInterrupt)?ABSOLUTE (__U4RXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000c6          0x4 LONG 0x776 DEFINED (__U4TXInterrupt)?ABSOLUTE (__U4TXInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000c8          0x4 LONG 0x776 DEFINED (__SPI3ErrInterrupt)?ABSOLUTE (__SPI3ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000ca          0x4 LONG 0x776 DEFINED (__SPI3Interrupt)?ABSOLUTE (__SPI3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000cc          0x4 LONG 0x776 DEFINED (__OC9Interrupt)?ABSOLUTE (__OC9Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000ce          0x4 LONG 0x776 DEFINED (__IC9Interrupt)?ABSOLUTE (__IC9Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000d0          0x4 LONG 0x776 DEFINED (__PWM1Interrupt)?ABSOLUTE (__PWM1Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000d2          0x4 LONG 0x776 DEFINED (__PWM2Interrupt)?ABSOLUTE (__PWM2Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000d4          0x4 LONG 0x776 DEFINED (__PWM3Interrupt)?ABSOLUTE (__PWM3Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000d6          0x4 LONG 0x776 DEFINED (__PWM4Interrupt)?ABSOLUTE (__PWM4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000d8          0x4 LONG 0x776 DEFINED (__PWM5Interrupt)?ABSOLUTE (__PWM5Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000da          0x4 LONG 0x776 DEFINED (__PWM6Interrupt)?ABSOLUTE (__PWM6Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x0000dc          0x4 LONG 0x776 DEFINED (__Interrupt100)?ABSOLUTE (__Interrupt100):ABSOLUTE (__DefaultInterrupt)
                  0x0000de          0x4 LONG 0x776 DEFINED (__Interrupt101)?ABSOLUTE (__Interrupt101):ABSOLUTE (__DefaultInterrupt)
                  0x0000e0          0x4 LONG 0x776 DEFINED (__Interrupt102)?ABSOLUTE (__Interrupt102):ABSOLUTE (__DefaultInterrupt)
                  0x0000e2          0x4 LONG 0x776 DEFINED (__Interrupt103)?ABSOLUTE (__Interrupt103):ABSOLUTE (__DefaultInterrupt)
                  0x0000e4          0x4 LONG 0x776 DEFINED (__Interrupt104)?ABSOLUTE (__Interrupt104):ABSOLUTE (__DefaultInterrupt)
                  0x0000e6          0x4 LONG 0x776 DEFINED (__Interrupt105)?ABSOLUTE (__Interrupt105):ABSOLUTE (__DefaultInterrupt)
                  0x0000e8          0x4 LONG 0x776 DEFINED (__Interrupt106)?ABSOLUTE (__Interrupt106):ABSOLUTE (__DefaultInterrupt)
                  0x0000ea          0x4 LONG 0x776 DEFINED (__Interrupt107)?ABSOLUTE (__Interrupt107):ABSOLUTE (__DefaultInterrupt)
                  0x0000ec          0x4 LONG 0x776 DEFINED (__Interrupt108)?ABSOLUTE (__Interrupt108):ABSOLUTE (__DefaultInterrupt)
                  0x0000ee          0x4 LONG 0x776 DEFINED (__Interrupt109)?ABSOLUTE (__Interrupt109):ABSOLUTE (__DefaultInterrupt)
                  0x0000f0          0x4 LONG 0x776 DEFINED (__Interrupt110)?ABSOLUTE (__Interrupt110):ABSOLUTE (__DefaultInterrupt)
                  0x0000f2          0x4 LONG 0x776 DEFINED (__Interrupt111)?ABSOLUTE (__Interrupt111):ABSOLUTE (__DefaultInterrupt)
                  0x0000f4          0x4 LONG 0x776 DEFINED (__Interrupt112)?ABSOLUTE (__Interrupt112):ABSOLUTE (__DefaultInterrupt)
                  0x0000f6          0x4 LONG 0x776 DEFINED (__Interrupt113)?ABSOLUTE (__Interrupt113):ABSOLUTE (__DefaultInterrupt)
                  0x0000f8          0x4 LONG 0x776 DEFINED (__Interrupt114)?ABSOLUTE (__Interrupt114):ABSOLUTE (__DefaultInterrupt)
                  0x0000fa          0x4 LONG 0x776 DEFINED (__Interrupt115)?ABSOLUTE (__Interrupt115):ABSOLUTE (__DefaultInterrupt)
                  0x0000fc          0x4 LONG 0x776 DEFINED (__Interrupt116)?ABSOLUTE (__Interrupt116):ABSOLUTE (__DefaultInterrupt)
                  0x0000fe          0x4 LONG 0x776 DEFINED (__Interrupt117)?ABSOLUTE (__Interrupt117):ABSOLUTE (__DefaultInterrupt)
                  0x000100          0x4 LONG 0x776 DEFINED (__DMA8Interrupt)?ABSOLUTE (__DMA8Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000102          0x4 LONG 0x776 DEFINED (__DMA9Interrupt)?ABSOLUTE (__DMA9Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000104          0x4 LONG 0x776 DEFINED (__DMA10Interrupt)?ABSOLUTE (__DMA10Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000106          0x4 LONG 0x776 DEFINED (__DMA11Interrupt)?ABSOLUTE (__DMA11Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000108          0x4 LONG 0x776 DEFINED (__SPI4ErrInterrupt)?ABSOLUTE (__SPI4ErrInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00010a          0x4 LONG 0x776 DEFINED (__SPI4Interrupt)?ABSOLUTE (__SPI4Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00010c          0x4 LONG 0x776 DEFINED (__OC10Interrupt)?ABSOLUTE (__OC10Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00010e          0x4 LONG 0x776 DEFINED (__IC10Interrupt)?ABSOLUTE (__IC10Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000110          0x4 LONG 0x776 DEFINED (__OC11Interrupt)?ABSOLUTE (__OC11Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000112          0x4 LONG 0x776 DEFINED (__IC11Interrupt)?ABSOLUTE (__IC11Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000114          0x4 LONG 0x776 DEFINED (__OC12Interrupt)?ABSOLUTE (__OC12Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000116          0x4 LONG 0x776 DEFINED (__IC12Interrupt)?ABSOLUTE (__IC12Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000118          0x4 LONG 0x776 DEFINED (__DMA12Interrupt)?ABSOLUTE (__DMA12Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00011a          0x4 LONG 0x776 DEFINED (__DMA13Interrupt)?ABSOLUTE (__DMA13Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00011c          0x4 LONG 0x776 DEFINED (__DMA14Interrupt)?ABSOLUTE (__DMA14Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00011e          0x4 LONG 0x776 DEFINED (__Interrupt133)?ABSOLUTE (__Interrupt133):ABSOLUTE (__DefaultInterrupt)
                  0x000120          0x4 LONG 0x776 DEFINED (__OC13Interrupt)?ABSOLUTE (__OC13Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000122          0x4 LONG 0x776 DEFINED (__IC13Interrupt)?ABSOLUTE (__IC13Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000124          0x4 LONG 0x776 DEFINED (__OC14Interrupt)?ABSOLUTE (__OC14Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000126          0x4 LONG 0x776 DEFINED (__IC14Interrupt)?ABSOLUTE (__IC14Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000128          0x4 LONG 0x776 DEFINED (__OC15Interrupt)?ABSOLUTE (__OC15Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00012a          0x4 LONG 0x776 DEFINED (__IC15Interrupt)?ABSOLUTE (__IC15Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00012c          0x4 LONG 0x776 DEFINED (__OC16Interrupt)?ABSOLUTE (__OC16Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x00012e          0x4 LONG 0x776 DEFINED (__IC16Interrupt)?ABSOLUTE (__IC16Interrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000130          0x4 LONG 0x776 DEFINED (__ICDInterrupt)?ABSOLUTE (__ICDInterrupt):ABSOLUTE (__DefaultInterrupt)
                  0x000132          0x4 LONG 0x776 DEFINED (__JTAGInterrupt)?ABSOLUTE (__JTAGInterrupt):ABSOLUTE (__DefaultInterrupt)
                    0x0000                  WREG0 = 0x0
                    0x0000                  _WREG0 = 0x0
                    0x0002                  WREG1 = 0x2
                    0x0002                  _WREG1 = 0x2
                    0x0004                  WREG2 = 0x4
                    0x0004                  _WREG2 = 0x4
                    0x0006                  WREG3 = 0x6
                    0x0006                  _WREG3 = 0x6
                    0x0008                  WREG4 = 0x8
                    0x0008                  _WREG4 = 0x8
                    0x000a                  WREG5 = 0xa
                    0x000a                  _WREG5 = 0xa
                    0x000c                  WREG6 = 0xc
                    0x000c                  _WREG6 = 0xc
                    0x000e                  WREG7 = 0xe
                    0x000e                  _WREG7 = 0xe
                    0x0010                  WREG8 = 0x10
                    0x0010                  _WREG8 = 0x10
                    0x0012                  WREG9 = 0x12
                    0x0012                  _WREG9 = 0x12
                    0x0014                  WREG10 = 0x14
                    0x0014                  _WREG10 = 0x14
                    0x0016                  WREG11 = 0x16
                    0x0016                  _WREG11 = 0x16
                    0x0018                  WREG12 = 0x18
                    0x0018                  _WREG12 = 0x18
                    0x001a                  WREG13 = 0x1a
                    0x001a                  _WREG13 = 0x1a
                    0x001c                  WREG14 = 0x1c
                    0x001c                  _WREG14 = 0x1c
                    0x001e                  WREG15 = 0x1e
                    0x001e                  _WREG15 = 0x1e
                    0x0020                  SPLIM = 0x20
                    0x0020                  _SPLIM = 0x20
                    0x0022                  ACCAL = 0x22
                    0x0022                  _ACCAL = 0x22
                    0x0024                  ACCAH = 0x24
                    0x0024                  _ACCAH = 0x24
                    0x0026                  ACCAU = 0x26
                    0x0026                  _ACCAU = 0x26
                    0x0028                  ACCBL = 0x28
                    0x0028                  _ACCBL = 0x28
                    0x002a                  ACCBH = 0x2a
                    0x002a                  _ACCBH = 0x2a
                    0x002c                  ACCBU = 0x2c
                    0x002c                  _ACCBU = 0x2c
                    0x002e                  PCL = 0x2e
                    0x002e                  _PCL = 0x2e
                    0x0030                  PCH = 0x30
                    0x0030                  _PCH = 0x30
                    0x0032                  DSRPAG = 0x32
                    0x0032                  _DSRPAG = 0x32
                    0x0032                  _DSRPAGbits = 0x32
                    0x0034                  DSWPAG = 0x34
                    0x0034                  _DSWPAG = 0x34
                    0x0034                  _DSWPAGbits = 0x34
                    0x0036                  RCOUNT = 0x36
                    0x0036                  _RCOUNT = 0x36
                    0x0038                  DCOUNT = 0x38
                    0x0038                  _DCOUNT = 0x38
                    0x003a                  DOSTARTL = 0x3a
                    0x003a                  _DOSTARTL = 0x3a
                    0x003c                  DOSTARTH = 0x3c
                    0x003c                  _DOSTARTH = 0x3c
                    0x003e                  DOENDL = 0x3e
                    0x003e                  _DOENDL = 0x3e
                    0x0040                  DOENDH = 0x40
                    0x0040                  _DOENDH = 0x40
                    0x0042                  SR = 0x42
                    0x0042                  _SR = 0x42
                    0x0042                  _SRbits = 0x42
                    0x0044                  CORCON = 0x44
                    0x0044                  _CORCON = 0x44
                    0x0044                  _CORCONbits = 0x44
                    0x0046                  MODCON = 0x46
                    0x0046                  _MODCON = 0x46
                    0x0046                  _MODCONbits = 0x46
                    0x0048                  XMODSRT = 0x48
                    0x0048                  _XMODSRT = 0x48
                    0x004a                  XMODEND = 0x4a
                    0x004a                  _XMODEND = 0x4a
                    0x004c                  YMODSRT = 0x4c
                    0x004c                  _YMODSRT = 0x4c
                    0x004e                  YMODEND = 0x4e
                    0x004e                  _YMODEND = 0x4e
                    0x0050                  XBREV = 0x50
                    0x0050                  _XBREV = 0x50
                    0x0050                  _XBREVbits = 0x50
                    0x0052                  DISICNT = 0x52
                    0x0052                  _DISICNT = 0x52
                    0x0054                  TBLPAG = 0x54
                    0x0054                  _TBLPAG = 0x54
                    0x0054                  _TBLPAGbits = 0x54
                    0x0058                  MSTRPR = 0x58
                    0x0058                  _MSTRPR = 0x58
                    0x0100                  TMR1 = 0x100
                    0x0100                  _TMR1 = 0x100
                    0x0102                  PR1 = 0x102
                    0x0102                  _PR1 = 0x102
                    0x0104                  T1CON = 0x104
                    0x0104                  _T1CON = 0x104
                    0x0104                  _T1CONbits = 0x104
                    0x0106                  TMR2 = 0x106
                    0x0106                  _TMR2 = 0x106
                    0x0108                  TMR3HLD = 0x108
                    0x0108                  _TMR3HLD = 0x108
                    0x010a                  TMR3 = 0x10a
                    0x010a                  _TMR3 = 0x10a
                    0x010c                  PR2 = 0x10c
                    0x010c                  _PR2 = 0x10c
                    0x010e                  PR3 = 0x10e
                    0x010e                  _PR3 = 0x10e
                    0x0110                  T2CON = 0x110
                    0x0110                  _T2CON = 0x110
                    0x0110                  _T2CONbits = 0x110
                    0x0112                  T3CON = 0x112
                    0x0112                  _T3CON = 0x112
                    0x0112                  _T3CONbits = 0x112
                    0x0114                  TMR4 = 0x114
                    0x0114                  _TMR4 = 0x114
                    0x0116                  TMR5HLD = 0x116
                    0x0116                  _TMR5HLD = 0x116
                    0x0118                  TMR5 = 0x118
                    0x0118                  _TMR5 = 0x118
                    0x011a                  PR4 = 0x11a
                    0x011a                  _PR4 = 0x11a
                    0x011c                  PR5 = 0x11c
                    0x011c                  _PR5 = 0x11c
                    0x011e                  T4CON = 0x11e
                    0x011e                  _T4CON = 0x11e
                    0x011e                  _T4CONbits = 0x11e
                    0x0120                  T5CON = 0x120
                    0x0120                  _T5CON = 0x120
                    0x0120                  _T5CONbits = 0x120
                    0x0122                  TMR6 = 0x122
                    0x0122                  _TMR6 = 0x122
                    0x0124                  TMR7HLD = 0x124
                    0x0124                  _TMR7HLD = 0x124
                    0x0126                  TMR7 = 0x126
                    0x0126                  _TMR7 = 0x126
                    0x0128                  PR6 = 0x128
                    0x0128                  _PR6 = 0x128
                    0x012a                  PR7 = 0x12a
                    0x012a                  _PR7 = 0x12a
                    0x012c                  T6CON = 0x12c
                    0x012c                  _T6CON = 0x12c
                    0x012c                  _T6CONbits = 0x12c
                    0x012e                  T7CON = 0x12e
                    0x012e                  _T7CON = 0x12e
                    0x012e                  _T7CONbits = 0x12e
                    0x0130                  TMR8 = 0x130
                    0x0130                  _TMR8 = 0x130
                    0x0132                  TMR9HLD = 0x132
                    0x0132                  _TMR9HLD = 0x132
                    0x0134                  TMR9 = 0x134
                    0x0134                  _TMR9 = 0x134
                    0x0136                  PR8 = 0x136
                    0x0136                  _PR8 = 0x136
                    0x0138                  PR9 = 0x138
                    0x0138                  _PR9 = 0x138
                    0x013a                  T8CON = 0x13a
                    0x013a                  _T8CON = 0x13a
                    0x013a                  _T8CONbits = 0x13a
                    0x013c                  T9CON = 0x13c
                    0x013c                  _T9CON = 0x13c
                    0x013c                  _T9CONbits = 0x13c
                    0x0140                  IC1CON1 = 0x140
                    0x0140                  _IC1CON1 = 0x140
                    0x0140                  _IC1CON1bits = 0x140
                    0x0142                  IC1CON2 = 0x142
                    0x0142                  _IC1CON2 = 0x142
                    0x0142                  _IC1CON2bits = 0x142
                    0x0144                  IC1BUF = 0x144
                    0x0144                  _IC1BUF = 0x144
                    0x0146                  IC1TMR = 0x146
                    0x0146                  _IC1TMR = 0x146
                    0x0148                  IC2CON1 = 0x148
                    0x0148                  _IC2CON1 = 0x148
                    0x0148                  _IC2CON1bits = 0x148
                    0x014a                  IC2CON2 = 0x14a
                    0x014a                  _IC2CON2 = 0x14a
                    0x014a                  _IC2CON2bits = 0x14a
                    0x014c                  IC2BUF = 0x14c
                    0x014c                  _IC2BUF = 0x14c
                    0x014e                  IC2TMR = 0x14e
                    0x014e                  _IC2TMR = 0x14e
                    0x0150                  IC3CON1 = 0x150
                    0x0150                  _IC3CON1 = 0x150
                    0x0150                  _IC3CON1bits = 0x150
                    0x0152                  IC3CON2 = 0x152
                    0x0152                  _IC3CON2 = 0x152
                    0x0152                  _IC3CON2bits = 0x152
                    0x0154                  IC3BUF = 0x154
                    0x0154                  _IC3BUF = 0x154
                    0x0156                  IC3TMR = 0x156
                    0x0156                  _IC3TMR = 0x156
                    0x0158                  IC4CON1 = 0x158
                    0x0158                  _IC4CON1 = 0x158
                    0x0158                  _IC4CON1bits = 0x158
                    0x015a                  IC4CON2 = 0x15a
                    0x015a                  _IC4CON2 = 0x15a
                    0x015a                  _IC4CON2bits = 0x15a
                    0x015c                  IC4BUF = 0x15c
                    0x015c                  _IC4BUF = 0x15c
                    0x015e                  IC4TMR = 0x15e
                    0x015e                  _IC4TMR = 0x15e
                    0x0160                  IC5CON1 = 0x160
                    0x0160                  _IC5CON1 = 0x160
                    0x0160                  _IC5CON1bits = 0x160
                    0x0162                  IC5CON2 = 0x162
                    0x0162                  _IC5CON2 = 0x162
                    0x0162                  _IC5CON2bits = 0x162
                    0x0164                  IC5BUF = 0x164
                    0x0164                  _IC5BUF = 0x164
                    0x0166                  IC5TMR = 0x166
                    0x0166                  _IC5TMR = 0x166
                    0x0168                  IC6CON1 = 0x168
                    0x0168                  _IC6CON1 = 0x168
                    0x0168                  _IC6CON1bits = 0x168
                    0x016a                  IC6CON2 = 0x16a
                    0x016a                  _IC6CON2 = 0x16a
                    0x016a                  _IC6CON2bits = 0x16a
                    0x016c                  IC6BUF = 0x16c
                    0x016c                  _IC6BUF = 0x16c
                    0x016e                  IC6TMR = 0x16e
                    0x016e                  _IC6TMR = 0x16e
                    0x0170                  IC7CON1 = 0x170
                    0x0170                  _IC7CON1 = 0x170
                    0x0170                  _IC7CON1bits = 0x170
                    0x0172                  IC7CON2 = 0x172
                    0x0172                  _IC7CON2 = 0x172
                    0x0172                  _IC7CON2bits = 0x172
                    0x0174                  IC7BUF = 0x174
                    0x0174                  _IC7BUF = 0x174
                    0x0176                  IC7TMR = 0x176
                    0x0176                  _IC7TMR = 0x176
                    0x0178                  IC8CON1 = 0x178
                    0x0178                  _IC8CON1 = 0x178
                    0x0178                  _IC8CON1bits = 0x178
                    0x017a                  IC8CON2 = 0x17a
                    0x017a                  _IC8CON2 = 0x17a
                    0x017a                  _IC8CON2bits = 0x17a
                    0x017c                  IC8BUF = 0x17c
                    0x017c                  _IC8BUF = 0x17c
                    0x017e                  IC8TMR = 0x17e
                    0x017e                  _IC8TMR = 0x17e
                    0x0180                  IC9CON1 = 0x180
                    0x0180                  _IC9CON1 = 0x180
                    0x0180                  _IC9CON1bits = 0x180
                    0x0182                  IC9CON2 = 0x182
                    0x0182                  _IC9CON2 = 0x182
                    0x0182                  _IC9CON2bits = 0x182
                    0x0184                  IC9BUF = 0x184
                    0x0184                  _IC9BUF = 0x184
                    0x0186                  IC9TMR = 0x186
                    0x0186                  _IC9TMR = 0x186
                    0x0188                  IC10CON1 = 0x188
                    0x0188                  _IC10CON1 = 0x188
                    0x0188                  _IC10CON1bits = 0x188
                    0x018a                  IC10CON2 = 0x18a
                    0x018a                  _IC10CON2 = 0x18a
                    0x018a                  _IC10CON2bits = 0x18a
                    0x018c                  IC10BUF = 0x18c
                    0x018c                  _IC10BUF = 0x18c
                    0x018e                  IC10TMR = 0x18e
                    0x018e                  _IC10TMR = 0x18e
                    0x0190                  IC11CON1 = 0x190
                    0x0190                  _IC11CON1 = 0x190
                    0x0190                  _IC11CON1bits = 0x190
                    0x0192                  IC11CON2 = 0x192
                    0x0192                  _IC11CON2 = 0x192
                    0x0192                  _IC11CON2bits = 0x192
                    0x0194                  IC11BUF = 0x194
                    0x0194                  _IC11BUF = 0x194
                    0x0196                  IC11TMR = 0x196
                    0x0196                  _IC11TMR = 0x196
                    0x0198                  IC12CON1 = 0x198
                    0x0198                  _IC12CON1 = 0x198
                    0x0198                  _IC12CON1bits = 0x198
                    0x019a                  IC12CON2 = 0x19a
                    0x019a                  _IC12CON2 = 0x19a
                    0x019a                  _IC12CON2bits = 0x19a
                    0x019c                  IC12BUF = 0x19c
                    0x019c                  _IC12BUF = 0x19c
                    0x019e                  IC12TMR = 0x19e
                    0x019e                  _IC12TMR = 0x19e
                    0x01a0                  IC13CON1 = 0x1a0
                    0x01a0                  _IC13CON1 = 0x1a0
                    0x01a0                  _IC13CON1bits = 0x1a0
                    0x01a2                  IC13CON2 = 0x1a2
                    0x01a2                  _IC13CON2 = 0x1a2
                    0x01a2                  _IC13CON2bits = 0x1a2
                    0x01a4                  IC13BUF = 0x1a4
                    0x01a4                  _IC13BUF = 0x1a4
                    0x01a6                  IC13TMR = 0x1a6
                    0x01a6                  _IC13TMR = 0x1a6
                    0x01a8                  IC14CON1 = 0x1a8
                    0x01a8                  _IC14CON1 = 0x1a8
                    0x01a8                  _IC14CON1bits = 0x1a8
                    0x01aa                  IC14CON2 = 0x1aa
                    0x01aa                  _IC14CON2 = 0x1aa
                    0x01aa                  _IC14CON2bits = 0x1aa
                    0x01ac                  IC14BUF = 0x1ac
                    0x01ac                  _IC14BUF = 0x1ac
                    0x01ae                  IC14TMR = 0x1ae
                    0x01ae                  _IC14TMR = 0x1ae
                    0x01b0                  IC15CON1 = 0x1b0
                    0x01b0                  _IC15CON1 = 0x1b0
                    0x01b0                  _IC15CON1bits = 0x1b0
                    0x01b2                  IC15CON2 = 0x1b2
                    0x01b2                  _IC15CON2 = 0x1b2
                    0x01b2                  _IC15CON2bits = 0x1b2
                    0x01b4                  IC15BUF = 0x1b4
                    0x01b4                  _IC15BUF = 0x1b4
                    0x01b6                  IC15TMR = 0x1b6
                    0x01b6                  _IC15TMR = 0x1b6
                    0x01b8                  IC16CON1 = 0x1b8
                    0x01b8                  _IC16CON1 = 0x1b8
                    0x01b8                  _IC16CON1bits = 0x1b8
                    0x01ba                  IC16CON2 = 0x1ba
                    0x01ba                  _IC16CON2 = 0x1ba
                    0x01ba                  _IC16CON2bits = 0x1ba
                    0x01bc                  IC16BUF = 0x1bc
                    0x01bc                  _IC16BUF = 0x1bc
                    0x01be                  IC16TMR = 0x1be
                    0x01be                  _IC16TMR = 0x1be
                    0x01c0                  QEI1CON = 0x1c0
                    0x01c0                  _QEI1CON = 0x1c0
                    0x01c0                  _QEI1CONbits = 0x1c0
                    0x01c2                  QEI1IOC = 0x1c2
                    0x01c2                  _QEI1IOC = 0x1c2
                    0x01c2                  _QEI1IOCbits = 0x1c2
                    0x01c4                  QEI1STAT = 0x1c4
                    0x01c4                  _QEI1STAT = 0x1c4
                    0x01c4                  _QEI1STATbits = 0x1c4
                    0x01c6                  POS1CNTL = 0x1c6
                    0x01c6                  _POS1CNTL = 0x1c6
                    0x01c8                  POS1CNTH = 0x1c8
                    0x01c8                  _POS1CNTH = 0x1c8
                    0x01ca                  POS1HLD = 0x1ca
                    0x01ca                  _POS1HLD = 0x1ca
                    0x01cc                  VEL1CNT = 0x1cc
                    0x01cc                  _VEL1CNT = 0x1cc
                    0x01ce                  INT1TMRL = 0x1ce
                    0x01ce                  _INT1TMRL = 0x1ce
                    0x01d0                  INT1TMRH = 0x1d0
                    0x01d0                  _INT1TMRH = 0x1d0
                    0x01d2                  INT1HLDL = 0x1d2
                    0x01d2                  _INT1HLDL = 0x1d2
                    0x01d4                  INT1HLDH = 0x1d4
                    0x01d4                  _INT1HLDH = 0x1d4
                    0x01d6                  INDX1CNTL = 0x1d6
                    0x01d6                  _INDX1CNTL = 0x1d6
                    0x01d8                  INDX1CNTH = 0x1d8
                    0x01d8                  _INDX1CNTH = 0x1d8
                    0x01da                  INDX1HLD = 0x1da
                    0x01da                  _INDX1HLD = 0x1da
                    0x01dc                  QEI1GECL = 0x1dc
                    0x01dc                  _QEI1GECL = 0x1dc
                    0x01dc                  QEI1ICL = 0x1dc
                    0x01dc                  _QEI1ICL = 0x1dc
                    0x01de                  QEI1GECH = 0x1de
                    0x01de                  _QEI1GECH = 0x1de
                    0x01de                  QEI1ICH = 0x1de
                    0x01de                  _QEI1ICH = 0x1de
                    0x01e0                  QEI1LECL = 0x1e0
                    0x01e0                  _QEI1LECL = 0x1e0
                    0x01e2                  QEI1LECH = 0x1e2
                    0x01e2                  _QEI1LECH = 0x1e2
                    0x0200                  I2C1RCV = 0x200
                    0x0200                  _I2C1RCV = 0x200
                    0x0202                  I2C1TRN = 0x202
                    0x0202                  _I2C1TRN = 0x202
                    0x0204                  I2C1BRG = 0x204
                    0x0204                  _I2C1BRG = 0x204
                    0x0206                  I2C1CON = 0x206
                    0x0206                  _I2C1CON = 0x206
                    0x0206                  _I2C1CONbits = 0x206
                    0x0208                  I2C1STAT = 0x208
                    0x0208                  _I2C1STAT = 0x208
                    0x0208                  _I2C1STATbits = 0x208
                    0x020a                  I2C1ADD = 0x20a
                    0x020a                  _I2C1ADD = 0x20a
                    0x020c                  I2C1MSK = 0x20c
                    0x020c                  _I2C1MSK = 0x20c
                    0x0210                  I2C2RCV = 0x210
                    0x0210                  _I2C2RCV = 0x210
                    0x0212                  I2C2TRN = 0x212
                    0x0212                  _I2C2TRN = 0x212
                    0x0214                  I2C2BRG = 0x214
                    0x0214                  _I2C2BRG = 0x214
                    0x0216                  I2C2CON = 0x216
                    0x0216                  _I2C2CON = 0x216
                    0x0216                  _I2C2CONbits = 0x216
                    0x0218                  I2C2STAT = 0x218
                    0x0218                  _I2C2STAT = 0x218
                    0x0218                  _I2C2STATbits = 0x218
                    0x021a                  I2C2ADD = 0x21a
                    0x021a                  _I2C2ADD = 0x21a
                    0x021c                  I2C2MSK = 0x21c
                    0x021c                  _I2C2MSK = 0x21c
                    0x0220                  U1MODE = 0x220
                    0x0220                  _U1MODE = 0x220
                    0x0220                  _U1MODEbits = 0x220
                    0x0222                  U1STA = 0x222
                    0x0222                  _U1STA = 0x222
                    0x0222                  _U1STAbits = 0x222
                    0x0224                  U1TXREG = 0x224
                    0x0224                  _U1TXREG = 0x224
                    0x0226                  U1RXREG = 0x226
                    0x0226                  _U1RXREG = 0x226
                    0x0228                  U1BRG = 0x228
                    0x0228                  _U1BRG = 0x228
                    0x0230                  U2MODE = 0x230
                    0x0230                  _U2MODE = 0x230
                    0x0230                  _U2MODEbits = 0x230
                    0x0232                  U2STA = 0x232
                    0x0232                  _U2STA = 0x232
                    0x0232                  _U2STAbits = 0x232
                    0x0234                  U2TXREG = 0x234
                    0x0234                  _U2TXREG = 0x234
                    0x0236                  U2RXREG = 0x236
                    0x0236                  _U2RXREG = 0x236
                    0x0238                  U2BRG = 0x238
                    0x0238                  _U2BRG = 0x238
                    0x0240                  SPI1STAT = 0x240
                    0x0240                  _SPI1STAT = 0x240
                    0x0240                  _SPI1STATbits = 0x240
                    0x0242                  SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1 = 0x242
                    0x0242                  _SPI1CON1bits = 0x242
                    0x0244                  SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2 = 0x244
                    0x0244                  _SPI1CON2bits = 0x244
                    0x0248                  SPI1BUF = 0x248
                    0x0248                  _SPI1BUF = 0x248
                    0x0250                  U3MODE = 0x250
                    0x0250                  _U3MODE = 0x250
                    0x0250                  _U3MODEbits = 0x250
                    0x0252                  U3STA = 0x252
                    0x0252                  _U3STA = 0x252
                    0x0252                  _U3STAbits = 0x252
                    0x0254                  U3TXREG = 0x254
                    0x0254                  _U3TXREG = 0x254
                    0x0256                  U3RXREG = 0x256
                    0x0256                  _U3RXREG = 0x256
                    0x0258                  U3BRG = 0x258
                    0x0258                  _U3BRG = 0x258
                    0x0260                  SPI2STAT = 0x260
                    0x0260                  _SPI2STAT = 0x260
                    0x0260                  _SPI2STATbits = 0x260
                    0x0262                  SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1 = 0x262
                    0x0262                  _SPI2CON1bits = 0x262
                    0x0264                  SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2 = 0x264
                    0x0264                  _SPI2CON2bits = 0x264
                    0x0268                  SPI2BUF = 0x268
                    0x0268                  _SPI2BUF = 0x268
                    0x0280                  DCICON1 = 0x280
                    0x0280                  _DCICON1 = 0x280
                    0x0280                  _DCICON1bits = 0x280
                    0x0282                  DCICON2 = 0x282
                    0x0282                  _DCICON2 = 0x282
                    0x0282                  _DCICON2bits = 0x282
                    0x0284                  DCICON3 = 0x284
                    0x0284                  _DCICON3 = 0x284
                    0x0284                  _DCICON3bits = 0x284
                    0x0286                  DCISTAT = 0x286
                    0x0286                  _DCISTAT = 0x286
                    0x0286                  _DCISTATbits = 0x286
                    0x0288                  TSCON = 0x288
                    0x0288                  _TSCON = 0x288
                    0x0288                  _TSCONbits = 0x288
                    0x028c                  RSCON = 0x28c
                    0x028c                  _RSCON = 0x28c
                    0x028c                  _RSCONbits = 0x28c
                    0x0290                  RXBUF0 = 0x290
                    0x0290                  _RXBUF0 = 0x290
                    0x0292                  RXBUF1 = 0x292
                    0x0292                  _RXBUF1 = 0x292
                    0x0294                  RXBUF2 = 0x294
                    0x0294                  _RXBUF2 = 0x294
                    0x0296                  RXBUF3 = 0x296
                    0x0296                  _RXBUF3 = 0x296
                    0x0298                  TXBUF0 = 0x298
                    0x0298                  _TXBUF0 = 0x298
                    0x029a                  TXBUF1 = 0x29a
                    0x029a                  _TXBUF1 = 0x29a
                    0x029c                  TXBUF2 = 0x29c
                    0x029c                  _TXBUF2 = 0x29c
                    0x029e                  TXBUF3 = 0x29e
                    0x029e                  _TXBUF3 = 0x29e
                    0x02a0                  SPI3STAT = 0x2a0
                    0x02a0                  _SPI3STAT = 0x2a0
                    0x02a0                  _SPI3STATbits = 0x2a0
                    0x02a2                  SPI3CON1 = 0x2a2
                    0x02a2                  _SPI3CON1 = 0x2a2
                    0x02a2                  _SPI3CON1bits = 0x2a2
                    0x02a4                  SPI3CON2 = 0x2a4
                    0x02a4                  _SPI3CON2 = 0x2a4
                    0x02a4                  _SPI3CON2bits = 0x2a4
                    0x02a8                  SPI3BUF = 0x2a8
                    0x02a8                  _SPI3BUF = 0x2a8
                    0x02b0                  U4MODE = 0x2b0
                    0x02b0                  _U4MODE = 0x2b0
                    0x02b0                  _U4MODEbits = 0x2b0
                    0x02b2                  U4STA = 0x2b2
                    0x02b2                  _U4STA = 0x2b2
                    0x02b2                  _U4STAbits = 0x2b2
                    0x02b4                  U4TXREG = 0x2b4
                    0x02b4                  _U4TXREG = 0x2b4
                    0x02b6                  U4RXREG = 0x2b6
                    0x02b6                  _U4RXREG = 0x2b6
                    0x02b8                  U4BRG = 0x2b8
                    0x02b8                  _U4BRG = 0x2b8
                    0x02c0                  SPI4STAT = 0x2c0
                    0x02c0                  _SPI4STAT = 0x2c0
                    0x02c0                  _SPI4STATbits = 0x2c0
                    0x02c2                  SPI4CON1 = 0x2c2
                    0x02c2                  _SPI4CON1 = 0x2c2
                    0x02c2                  _SPI4CON1bits = 0x2c2
                    0x02c4                  SPI4CON2 = 0x2c4
                    0x02c4                  _SPI4CON2 = 0x2c4
                    0x02c4                  _SPI4CON2bits = 0x2c4
                    0x02c8                  SPI4BUF = 0x2c8
                    0x02c8                  _SPI4BUF = 0x2c8
                    0x0300                  ADC1BUF0 = 0x300
                    0x0300                  _ADC1BUF0 = 0x300
                    0x0302                  ADC1BUF1 = 0x302
                    0x0302                  _ADC1BUF1 = 0x302
                    0x0304                  ADC1BUF2 = 0x304
                    0x0304                  _ADC1BUF2 = 0x304
                    0x0306                  ADC1BUF3 = 0x306
                    0x0306                  _ADC1BUF3 = 0x306
                    0x0308                  ADC1BUF4 = 0x308
                    0x0308                  _ADC1BUF4 = 0x308
                    0x030a                  ADC1BUF5 = 0x30a
                    0x030a                  _ADC1BUF5 = 0x30a
                    0x030c                  ADC1BUF6 = 0x30c
                    0x030c                  _ADC1BUF6 = 0x30c
                    0x030e                  ADC1BUF7 = 0x30e
                    0x030e                  _ADC1BUF7 = 0x30e
                    0x0310                  ADC1BUF8 = 0x310
                    0x0310                  _ADC1BUF8 = 0x310
                    0x0312                  ADC1BUF9 = 0x312
                    0x0312                  _ADC1BUF9 = 0x312
                    0x0314                  ADC1BUFA = 0x314
                    0x0314                  _ADC1BUFA = 0x314
                    0x0316                  ADC1BUFB = 0x316
                    0x0316                  _ADC1BUFB = 0x316
                    0x0318                  ADC1BUFC = 0x318
                    0x0318                  _ADC1BUFC = 0x318
                    0x031a                  ADC1BUFD = 0x31a
                    0x031a                  _ADC1BUFD = 0x31a
                    0x031c                  ADC1BUFE = 0x31c
                    0x031c                  _ADC1BUFE = 0x31c
                    0x031e                  ADC1BUFF = 0x31e
                    0x031e                  _ADC1BUFF = 0x31e
                    0x0320                  AD1CON1 = 0x320
                    0x0320                  _AD1CON1 = 0x320
                    0x0320                  _AD1CON1bits = 0x320
                    0x0322                  AD1CON2 = 0x322
                    0x0322                  _AD1CON2 = 0x322
                    0x0322                  _AD1CON2bits = 0x322
                    0x0324                  AD1CON3 = 0x324
                    0x0324                  _AD1CON3 = 0x324
                    0x0324                  _AD1CON3bits = 0x324
                    0x0326                  AD1CHS123 = 0x326
                    0x0326                  _AD1CHS123 = 0x326
                    0x0326                  _AD1CHS123bits = 0x326
                    0x0328                  AD1CHS0 = 0x328
                    0x0328                  _AD1CHS0 = 0x328
                    0x0328                  _AD1CHS0bits = 0x328
                    0x032e                  AD1CSSH = 0x32e
                    0x032e                  _AD1CSSH = 0x32e
                    0x032e                  _AD1CSSHbits = 0x32e
                    0x0330                  AD1CSSL = 0x330
                    0x0330                  _AD1CSSL = 0x330
                    0x0330                  _AD1CSSLbits = 0x330
                    0x0332                  AD1CON4 = 0x332
                    0x0332                  _AD1CON4 = 0x332
                    0x0332                  _AD1CON4bits = 0x332
                    0x0340                  ADC2BUF0 = 0x340
                    0x0340                  _ADC2BUF0 = 0x340
                    0x0342                  ADC2BUF1 = 0x342
                    0x0342                  _ADC2BUF1 = 0x342
                    0x0344                  ADC2BUF2 = 0x344
                    0x0344                  _ADC2BUF2 = 0x344
                    0x0346                  ADC2BUF3 = 0x346
                    0x0346                  _ADC2BUF3 = 0x346
                    0x0348                  ADC2BUF4 = 0x348
                    0x0348                  _ADC2BUF4 = 0x348
                    0x034a                  ADC2BUF5 = 0x34a
                    0x034a                  _ADC2BUF5 = 0x34a
                    0x034c                  ADC2BUF6 = 0x34c
                    0x034c                  _ADC2BUF6 = 0x34c
                    0x034e                  ADC2BUF7 = 0x34e
                    0x034e                  _ADC2BUF7 = 0x34e
                    0x0350                  ADC2BUF8 = 0x350
                    0x0350                  _ADC2BUF8 = 0x350
                    0x0352                  ADC2BUF9 = 0x352
                    0x0352                  _ADC2BUF9 = 0x352
                    0x0354                  ADC2BUFA = 0x354
                    0x0354                  _ADC2BUFA = 0x354
                    0x0356                  ADC2BUFB = 0x356
                    0x0356                  _ADC2BUFB = 0x356
                    0x0358                  ADC2BUFC = 0x358
                    0x0358                  _ADC2BUFC = 0x358
                    0x035a                  ADC2BUFD = 0x35a
                    0x035a                  _ADC2BUFD = 0x35a
                    0x035c                  ADC2BUFE = 0x35c
                    0x035c                  _ADC2BUFE = 0x35c
                    0x035e                  ADC2BUFF = 0x35e
                    0x035e                  _ADC2BUFF = 0x35e
                    0x0360                  AD2CON1 = 0x360
                    0x0360                  _AD2CON1 = 0x360
                    0x0360                  _AD2CON1bits = 0x360
                    0x0362                  AD2CON2 = 0x362
                    0x0362                  _AD2CON2 = 0x362
                    0x0362                  _AD2CON2bits = 0x362
                    0x0364                  AD2CON3 = 0x364
                    0x0364                  _AD2CON3 = 0x364
                    0x0364                  _AD2CON3bits = 0x364
                    0x0366                  AD2CHS123 = 0x366
                    0x0366                  _AD2CHS123 = 0x366
                    0x0366                  _AD2CHS123bits = 0x366
                    0x0368                  AD2CHS0 = 0x368
                    0x0368                  _AD2CHS0 = 0x368
                    0x0368                  _AD2CHS0bits = 0x368
                    0x0370                  AD2CSSL = 0x370
                    0x0370                  _AD2CSSL = 0x370
                    0x0370                  _AD2CSSLbits = 0x370
                    0x0372                  AD2CON4 = 0x372
                    0x0372                  _AD2CON4 = 0x372
                    0x0372                  _AD2CON4bits = 0x372
                    0x0400                  C1CTRL1 = 0x400
                    0x0400                  _C1CTRL1 = 0x400
                    0x0400                  _C1CTRL1bits = 0x400
                    0x0402                  C1CTRL2 = 0x402
                    0x0402                  _C1CTRL2 = 0x402
                    0x0402                  _C1CTRL2bits = 0x402
                    0x0404                  C1VEC = 0x404
                    0x0404                  _C1VEC = 0x404
                    0x0404                  _C1VECbits = 0x404
                    0x0406                  C1FCTRL = 0x406
                    0x0406                  _C1FCTRL = 0x406
                    0x0406                  _C1FCTRLbits = 0x406
                    0x0408                  C1FIFO = 0x408
                    0x0408                  _C1FIFO = 0x408
                    0x0408                  _C1FIFObits = 0x408
                    0x040a                  C1INTF = 0x40a
                    0x040a                  _C1INTF = 0x40a
                    0x040a                  _C1INTFbits = 0x40a
                    0x040c                  C1INTE = 0x40c
                    0x040c                  _C1INTE = 0x40c
                    0x040c                  _C1INTEbits = 0x40c
                    0x040e                  C1EC = 0x40e
                    0x040e                  _C1EC = 0x40e
                    0x040e                  _C1ECbits = 0x40e
                    0x040e                  C1RERRCNT = 0x40e
                    0x040e                  _C1RERRCNT = 0x40e
                    0x040f                  C1TERRCNT = 0x40f
                    0x040f                  _C1TERRCNT = 0x40f
                    0x0410                  C1CFG1 = 0x410
                    0x0410                  _C1CFG1 = 0x410
                    0x0410                  _C1CFG1bits = 0x410
                    0x0412                  C1CFG2 = 0x412
                    0x0412                  _C1CFG2 = 0x412
                    0x0412                  _C1CFG2bits = 0x412
                    0x0414                  C1FEN1 = 0x414
                    0x0414                  _C1FEN1 = 0x414
                    0x0414                  _C1FEN1bits = 0x414
                    0x0418                  C1FMSKSEL1 = 0x418
                    0x0418                  _C1FMSKSEL1 = 0x418
                    0x0418                  _C1FMSKSEL1bits = 0x418
                    0x041a                  C1FMSKSEL2 = 0x41a
                    0x041a                  _C1FMSKSEL2 = 0x41a
                    0x041a                  _C1FMSKSEL2bits = 0x41a
                    0x0420                  C1BUFPNT1 = 0x420
                    0x0420                  _C1BUFPNT1 = 0x420
                    0x0420                  _C1BUFPNT1bits = 0x420
                    0x0420                  C1RXFUL1 = 0x420
                    0x0420                  _C1RXFUL1 = 0x420
                    0x0420                  _C1RXFUL1bits = 0x420
                    0x0422                  C1BUFPNT2 = 0x422
                    0x0422                  _C1BUFPNT2 = 0x422
                    0x0422                  _C1BUFPNT2bits = 0x422
                    0x0422                  C1RXFUL2 = 0x422
                    0x0422                  _C1RXFUL2 = 0x422
                    0x0422                  _C1RXFUL2bits = 0x422
                    0x0424                  C1BUFPNT3 = 0x424
                    0x0424                  _C1BUFPNT3 = 0x424
                    0x0424                  _C1BUFPNT3bits = 0x424
                    0x0426                  C1BUFPNT4 = 0x426
                    0x0426                  _C1BUFPNT4 = 0x426
                    0x0426                  _C1BUFPNT4bits = 0x426
                    0x0428                  C1RXOVF1 = 0x428
                    0x0428                  _C1RXOVF1 = 0x428
                    0x0428                  _C1RXOVF1bits = 0x428
                    0x042a                  C1RXOVF2 = 0x42a
                    0x042a                  _C1RXOVF2 = 0x42a
                    0x042a                  _C1RXOVF2bits = 0x42a
                    0x0430                  C1RXM0SID = 0x430
                    0x0430                  _C1RXM0SID = 0x430
                    0x0430                  _C1RXM0SIDbits = 0x430
                    0x0430                  C1TR01CON = 0x430
                    0x0430                  _C1TR01CON = 0x430
                    0x0430                  _C1TR01CONbits = 0x430
                    0x0432                  C1RXM0EID = 0x432
                    0x0432                  _C1RXM0EID = 0x432
                    0x0432                  _C1RXM0EIDbits = 0x432
                    0x0432                  C1TR23CON = 0x432
                    0x0432                  _C1TR23CON = 0x432
                    0x0432                  _C1TR23CONbits = 0x432
                    0x0434                  C1RXM1SID = 0x434
                    0x0434                  _C1RXM1SID = 0x434
                    0x0434                  _C1RXM1SIDbits = 0x434
                    0x0434                  C1TR45CON = 0x434
                    0x0434                  _C1TR45CON = 0x434
                    0x0434                  _C1TR45CONbits = 0x434
                    0x0436                  C1RXM1EID = 0x436
                    0x0436                  _C1RXM1EID = 0x436
                    0x0436                  _C1RXM1EIDbits = 0x436
                    0x0436                  C1TR67CON = 0x436
                    0x0436                  _C1TR67CON = 0x436
                    0x0436                  _C1TR67CONbits = 0x436
                    0x0438                  C1RXM2SID = 0x438
                    0x0438                  _C1RXM2SID = 0x438
                    0x0438                  _C1RXM2SIDbits = 0x438
                    0x043a                  C1RXM2EID = 0x43a
                    0x043a                  _C1RXM2EID = 0x43a
                    0x043a                  _C1RXM2EIDbits = 0x43a
                    0x0440                  C1RXD = 0x440
                    0x0440                  _C1RXD = 0x440
                    0x0440                  C1RXF0SID = 0x440
                    0x0440                  _C1RXF0SID = 0x440
                    0x0440                  _C1RXF0SIDbits = 0x440
                    0x0442                  C1RXF0EID = 0x442
                    0x0442                  _C1RXF0EID = 0x442
                    0x0442                  _C1RXF0EIDbits = 0x442
                    0x0442                  C1TXD = 0x442
                    0x0442                  _C1TXD = 0x442
                    0x0442                  _C1TXDbits = 0x442
                    0x0444                  C1RXF1SID = 0x444
                    0x0444                  _C1RXF1SID = 0x444
                    0x0444                  _C1RXF1SIDbits = 0x444
                    0x0446                  C1RXF1EID = 0x446
                    0x0446                  _C1RXF1EID = 0x446
                    0x0446                  _C1RXF1EIDbits = 0x446
                    0x0448                  C1RXF2SID = 0x448
                    0x0448                  _C1RXF2SID = 0x448
                    0x0448                  _C1RXF2SIDbits = 0x448
                    0x044a                  C1RXF2EID = 0x44a
                    0x044a                  _C1RXF2EID = 0x44a
                    0x044a                  _C1RXF2EIDbits = 0x44a
                    0x044c                  C1RXF3SID = 0x44c
                    0x044c                  _C1RXF3SID = 0x44c
                    0x044c                  _C1RXF3SIDbits = 0x44c
                    0x044e                  C1RXF3EID = 0x44e
                    0x044e                  _C1RXF3EID = 0x44e
                    0x044e                  _C1RXF3EIDbits = 0x44e
                    0x0450                  C1RXF4SID = 0x450
                    0x0450                  _C1RXF4SID = 0x450
                    0x0450                  _C1RXF4SIDbits = 0x450
                    0x0452                  C1RXF4EID = 0x452
                    0x0452                  _C1RXF4EID = 0x452
                    0x0452                  _C1RXF4EIDbits = 0x452
                    0x0454                  C1RXF5SID = 0x454
                    0x0454                  _C1RXF5SID = 0x454
                    0x0454                  _C1RXF5SIDbits = 0x454
                    0x0456                  C1RXF5EID = 0x456
                    0x0456                  _C1RXF5EID = 0x456
                    0x0456                  _C1RXF5EIDbits = 0x456
                    0x0458                  C1RXF6SID = 0x458
                    0x0458                  _C1RXF6SID = 0x458
                    0x0458                  _C1RXF6SIDbits = 0x458
                    0x045a                  C1RXF6EID = 0x45a
                    0x045a                  _C1RXF6EID = 0x45a
                    0x045a                  _C1RXF6EIDbits = 0x45a
                    0x045c                  C1RXF7SID = 0x45c
                    0x045c                  _C1RXF7SID = 0x45c
                    0x045c                  _C1RXF7SIDbits = 0x45c
                    0x045e                  C1RXF7EID = 0x45e
                    0x045e                  _C1RXF7EID = 0x45e
                    0x045e                  _C1RXF7EIDbits = 0x45e
                    0x0460                  C1RXF8SID = 0x460
                    0x0460                  _C1RXF8SID = 0x460
                    0x0460                  _C1RXF8SIDbits = 0x460
                    0x0462                  C1RXF8EID = 0x462
                    0x0462                  _C1RXF8EID = 0x462
                    0x0462                  _C1RXF8EIDbits = 0x462
                    0x0464                  C1RXF9SID = 0x464
                    0x0464                  _C1RXF9SID = 0x464
                    0x0464                  _C1RXF9SIDbits = 0x464
                    0x0466                  C1RXF9EID = 0x466
                    0x0466                  _C1RXF9EID = 0x466
                    0x0466                  _C1RXF9EIDbits = 0x466
                    0x0468                  C1RXF10SID = 0x468
                    0x0468                  _C1RXF10SID = 0x468
                    0x0468                  _C1RXF10SIDbits = 0x468
                    0x046a                  C1RXF10EID = 0x46a
                    0x046a                  _C1RXF10EID = 0x46a
                    0x046a                  _C1RXF10EIDbits = 0x46a
                    0x046c                  C1RXF11SID = 0x46c
                    0x046c                  _C1RXF11SID = 0x46c
                    0x046c                  _C1RXF11SIDbits = 0x46c
                    0x046e                  C1RXF11EID = 0x46e
                    0x046e                  _C1RXF11EID = 0x46e
                    0x046e                  _C1RXF11EIDbits = 0x46e
                    0x0470                  C1RXF12SID = 0x470
                    0x0470                  _C1RXF12SID = 0x470
                    0x0470                  _C1RXF12SIDbits = 0x470
                    0x0472                  C1RXF12EID = 0x472
                    0x0472                  _C1RXF12EID = 0x472
                    0x0472                  _C1RXF12EIDbits = 0x472
                    0x0474                  C1RXF13SID = 0x474
                    0x0474                  _C1RXF13SID = 0x474
                    0x0474                  _C1RXF13SIDbits = 0x474
                    0x0476                  C1RXF13EID = 0x476
                    0x0476                  _C1RXF13EID = 0x476
                    0x0476                  _C1RXF13EIDbits = 0x476
                    0x0478                  C1RXF14SID = 0x478
                    0x0478                  _C1RXF14SID = 0x478
                    0x0478                  _C1RXF14SIDbits = 0x478
                    0x047a                  C1RXF14EID = 0x47a
                    0x047a                  _C1RXF14EID = 0x47a
                    0x047a                  _C1RXF14EIDbits = 0x47a
                    0x047c                  C1RXF15SID = 0x47c
                    0x047c                  _C1RXF15SID = 0x47c
                    0x047c                  _C1RXF15SIDbits = 0x47c
                    0x047e                  C1RXF15EID = 0x47e
                    0x047e                  _C1RXF15EID = 0x47e
                    0x047e                  _C1RXF15EIDbits = 0x47e
                    0x0488                  U1OTGIR = 0x488
                    0x0488                  _U1OTGIR = 0x488
                    0x0488                  _U1OTGIRbits = 0x488
                    0x048a                  U1OTGIE = 0x48a
                    0x048a                  _U1OTGIE = 0x48a
                    0x048a                  _U1OTGIEbits = 0x48a
                    0x048c                  U1OTGSTAT = 0x48c
                    0x048c                  _U1OTGSTAT = 0x48c
                    0x048c                  _U1OTGSTATbits = 0x48c
                    0x048e                  U1OTGCON = 0x48e
                    0x048e                  _U1OTGCON = 0x48e
                    0x048e                  _U1OTGCONbits = 0x48e
                    0x0490                  U1PWRC = 0x490
                    0x0490                  _U1PWRC = 0x490
                    0x0490                  _U1PWRCbits = 0x490
                    0x04c0                  U1IR = 0x4c0
                    0x04c0                  _U1IR = 0x4c0
                    0x04c0                  _U1IRbits = 0x4c0
                    0x04c2                  U1IE = 0x4c2
                    0x04c2                  _U1IE = 0x4c2
                    0x04c2                  _U1IEbits = 0x4c2
                    0x04c4                  U1EIR = 0x4c4
                    0x04c4                  _U1EIR = 0x4c4
                    0x04c4                  _U1EIRbits = 0x4c4
                    0x04c6                  U1EIE = 0x4c6
                    0x04c6                  _U1EIE = 0x4c6
                    0x04c6                  _U1EIEbits = 0x4c6
                    0x04c8                  U1STAT = 0x4c8
                    0x04c8                  _U1STAT = 0x4c8
                    0x04c8                  _U1STATbits = 0x4c8
                    0x04ca                  U1CON = 0x4ca
                    0x04ca                  _U1CON = 0x4ca
                    0x04ca                  _U1CONbits = 0x4ca
                    0x04cc                  U1ADDR = 0x4cc
                    0x04cc                  _U1ADDR = 0x4cc
                    0x04cc                  _U1ADDRbits = 0x4cc
                    0x04ce                  U1BDTP1 = 0x4ce
                    0x04ce                  _U1BDTP1 = 0x4ce
                    0x04ce                  _U1BDTP1bits = 0x4ce
                    0x04d0                  U1FRML = 0x4d0
                    0x04d0                  _U1FRML = 0x4d0
                    0x04d0                  _U1FRMLbits = 0x4d0
                    0x04d2                  U1FRMH = 0x4d2
                    0x04d2                  _U1FRMH = 0x4d2
                    0x04d2                  _U1FRMHbits = 0x4d2
                    0x04d4                  U1TOK = 0x4d4
                    0x04d4                  _U1TOK = 0x4d4
                    0x04d4                  _U1TOKbits = 0x4d4
                    0x04d6                  U1SOF = 0x4d6
                    0x04d6                  _U1SOF = 0x4d6
                    0x04d6                  _U1SOFbits = 0x4d6
                    0x04d8                  U1BDTP2 = 0x4d8
                    0x04d8                  _U1BDTP2 = 0x4d8
                    0x04d8                  _U1BDTP2bits = 0x4d8
                    0x04da                  U1BDTP3 = 0x4da
                    0x04da                  _U1BDTP3 = 0x4da
                    0x04da                  _U1BDTP3bits = 0x4da
                    0x04dc                  U1CNFG1 = 0x4dc
                    0x04dc                  _U1CNFG1 = 0x4dc
                    0x04dc                  _U1CNFG1bits = 0x4dc
                    0x04de                  U1CNFG2 = 0x4de
                    0x04de                  _U1CNFG2 = 0x4de
                    0x04de                  _U1CNFG2bits = 0x4de
                    0x04e0                  U1EP0 = 0x4e0
                    0x04e0                  _U1EP0 = 0x4e0
                    0x04e0                  _U1EP0bits = 0x4e0
                    0x04e2                  U1EP1 = 0x4e2
                    0x04e2                  _U1EP1 = 0x4e2
                    0x04e2                  _U1EP1bits = 0x4e2
                    0x04e4                  U1EP2 = 0x4e4
                    0x04e4                  _U1EP2 = 0x4e4
                    0x04e4                  _U1EP2bits = 0x4e4
                    0x04e6                  U1EP3 = 0x4e6
                    0x04e6                  _U1EP3 = 0x4e6
                    0x04e6                  _U1EP3bits = 0x4e6
                    0x04e8                  U1EP4 = 0x4e8
                    0x04e8                  _U1EP4 = 0x4e8
                    0x04e8                  _U1EP4bits = 0x4e8
                    0x04ea                  U1EP5 = 0x4ea
                    0x04ea                  _U1EP5 = 0x4ea
                    0x04ea                  _U1EP5bits = 0x4ea
                    0x04ec                  U1EP6 = 0x4ec
                    0x04ec                  _U1EP6 = 0x4ec
                    0x04ec                  _U1EP6bits = 0x4ec
                    0x04ee                  U1EP7 = 0x4ee
                    0x04ee                  _U1EP7 = 0x4ee
                    0x04ee                  _U1EP7bits = 0x4ee
                    0x04f0                  U1EP8 = 0x4f0
                    0x04f0                  _U1EP8 = 0x4f0
                    0x04f0                  _U1EP8bits = 0x4f0
                    0x04f2                  U1EP9 = 0x4f2
                    0x04f2                  _U1EP9 = 0x4f2
                    0x04f2                  _U1EP9bits = 0x4f2
                    0x04f4                  U1EP10 = 0x4f4
                    0x04f4                  _U1EP10 = 0x4f4
                    0x04f4                  _U1EP10bits = 0x4f4
                    0x04f6                  U1EP11 = 0x4f6
                    0x04f6                  _U1EP11 = 0x4f6
                    0x04f6                  _U1EP11bits = 0x4f6
                    0x04f8                  U1EP12 = 0x4f8
                    0x04f8                  _U1EP12 = 0x4f8
                    0x04f8                  _U1EP12bits = 0x4f8
                    0x04fa                  U1EP13 = 0x4fa
                    0x04fa                  _U1EP13 = 0x4fa
                    0x04fa                  _U1EP13bits = 0x4fa
                    0x04fc                  U1EP14 = 0x4fc
                    0x04fc                  _U1EP14 = 0x4fc
                    0x04fc                  _U1EP14bits = 0x4fc
                    0x04fe                  U1EP15 = 0x4fe
                    0x04fe                  _U1EP15 = 0x4fe
                    0x04fe                  _U1EP15bits = 0x4fe
                    0x0500                  C2CTRL1 = 0x500
                    0x0500                  _C2CTRL1 = 0x500
                    0x0500                  _C2CTRL1bits = 0x500
                    0x0502                  C2CTRL2 = 0x502
                    0x0502                  _C2CTRL2 = 0x502
                    0x0502                  _C2CTRL2bits = 0x502
                    0x0504                  C2VEC = 0x504
                    0x0504                  _C2VEC = 0x504
                    0x0504                  _C2VECbits = 0x504
                    0x0506                  C2FCTRL = 0x506
                    0x0506                  _C2FCTRL = 0x506
                    0x0506                  _C2FCTRLbits = 0x506
                    0x0508                  C2FIFO = 0x508
                    0x0508                  _C2FIFO = 0x508
                    0x0508                  _C2FIFObits = 0x508
                    0x050a                  C2INTF = 0x50a
                    0x050a                  _C2INTF = 0x50a
                    0x050a                  _C2INTFbits = 0x50a
                    0x050c                  C2INTE = 0x50c
                    0x050c                  _C2INTE = 0x50c
                    0x050c                  _C2INTEbits = 0x50c
                    0x050e                  C2EC = 0x50e
                    0x050e                  _C2EC = 0x50e
                    0x050e                  _C2ECbits = 0x50e
                    0x050e                  C2RERRCNT = 0x50e
                    0x050e                  _C2RERRCNT = 0x50e
                    0x050f                  C2TERRCNT = 0x50f
                    0x050f                  _C2TERRCNT = 0x50f
                    0x0510                  C2CFG1 = 0x510
                    0x0510                  _C2CFG1 = 0x510
                    0x0510                  _C2CFG1bits = 0x510
                    0x0512                  C2CFG2 = 0x512
                    0x0512                  _C2CFG2 = 0x512
                    0x0512                  _C2CFG2bits = 0x512
                    0x0514                  C2FEN1 = 0x514
                    0x0514                  _C2FEN1 = 0x514
                    0x0514                  _C2FEN1bits = 0x514
                    0x0518                  C2FMSKSEL1 = 0x518
                    0x0518                  _C2FMSKSEL1 = 0x518
                    0x0518                  _C2FMSKSEL1bits = 0x518
                    0x051a                  C2FMSKSEL2 = 0x51a
                    0x051a                  _C2FMSKSEL2 = 0x51a
                    0x051a                  _C2FMSKSEL2bits = 0x51a
                    0x0520                  C2BUFPNT1 = 0x520
                    0x0520                  _C2BUFPNT1 = 0x520
                    0x0520                  _C2BUFPNT1bits = 0x520
                    0x0520                  C2RXFUL1 = 0x520
                    0x0520                  _C2RXFUL1 = 0x520
                    0x0520                  _C2RXFUL1bits = 0x520
                    0x0522                  C2BUFPNT2 = 0x522
                    0x0522                  _C2BUFPNT2 = 0x522
                    0x0522                  _C2BUFPNT2bits = 0x522
                    0x0522                  C2RXFUL2 = 0x522
                    0x0522                  _C2RXFUL2 = 0x522
                    0x0522                  _C2RXFUL2bits = 0x522
                    0x0524                  C2BUFPNT3 = 0x524
                    0x0524                  _C2BUFPNT3 = 0x524
                    0x0524                  _C2BUFPNT3bits = 0x524
                    0x0526                  C2BUFPNT4 = 0x526
                    0x0526                  _C2BUFPNT4 = 0x526
                    0x0526                  _C2BUFPNT4bits = 0x526
                    0x0528                  C2RXOVF1 = 0x528
                    0x0528                  _C2RXOVF1 = 0x528
                    0x0528                  _C2RXOVF1bits = 0x528
                    0x052a                  C2RXOVF2 = 0x52a
                    0x052a                  _C2RXOVF2 = 0x52a
                    0x052a                  _C2RXOVF2bits = 0x52a
                    0x0530                  C2RXM0SID = 0x530
                    0x0530                  _C2RXM0SID = 0x530
                    0x0530                  _C2RXM0SIDbits = 0x530
                    0x0530                  C2TR01CON = 0x530
                    0x0530                  _C2TR01CON = 0x530
                    0x0530                  _C2TR01CONbits = 0x530
                    0x0532                  C2RXM0EID = 0x532
                    0x0532                  _C2RXM0EID = 0x532
                    0x0532                  _C2RXM0EIDbits = 0x532
                    0x0532                  C2TR23CON = 0x532
                    0x0532                  _C2TR23CON = 0x532
                    0x0532                  _C2TR23CONbits = 0x532
                    0x0534                  C2RXM1SID = 0x534
                    0x0534                  _C2RXM1SID = 0x534
                    0x0534                  _C2RXM1SIDbits = 0x534
                    0x0534                  C2TR45CON = 0x534
                    0x0534                  _C2TR45CON = 0x534
                    0x0534                  _C2TR45CONbits = 0x534
                    0x0536                  C2RXM1EID = 0x536
                    0x0536                  _C2RXM1EID = 0x536
                    0x0536                  _C2RXM1EIDbits = 0x536
                    0x0536                  C2TR67CON = 0x536
                    0x0536                  _C2TR67CON = 0x536
                    0x0536                  _C2TR67CONbits = 0x536
                    0x0538                  C2RXM2SID = 0x538
                    0x0538                  _C2RXM2SID = 0x538
                    0x0538                  _C2RXM2SIDbits = 0x538
                    0x053a                  C2RXM2EID = 0x53a
                    0x053a                  _C2RXM2EID = 0x53a
                    0x053a                  _C2RXM2EIDbits = 0x53a
                    0x0540                  C2RXD = 0x540
                    0x0540                  _C2RXD = 0x540
                    0x0540                  C2RXF0SID = 0x540
                    0x0540                  _C2RXF0SID = 0x540
                    0x0540                  _C2RXF0SIDbits = 0x540
                    0x0542                  C2RXF0EID = 0x542
                    0x0542                  _C2RXF0EID = 0x542
                    0x0542                  _C2RXF0EIDbits = 0x542
                    0x0542                  C2TXD = 0x542
                    0x0542                  _C2TXD = 0x542
                    0x0542                  _C2TXDbits = 0x542
                    0x0544                  C2RXF1SID = 0x544
                    0x0544                  _C2RXF1SID = 0x544
                    0x0544                  _C2RXF1SIDbits = 0x544
                    0x0546                  C2RXF1EID = 0x546
                    0x0546                  _C2RXF1EID = 0x546
                    0x0546                  _C2RXF1EIDbits = 0x546
                    0x0548                  C2RXF2SID = 0x548
                    0x0548                  _C2RXF2SID = 0x548
                    0x0548                  _C2RXF2SIDbits = 0x548
                    0x054a                  C2RXF2EID = 0x54a
                    0x054a                  _C2RXF2EID = 0x54a
                    0x054a                  _C2RXF2EIDbits = 0x54a
                    0x054c                  C2RXF3SID = 0x54c
                    0x054c                  _C2RXF3SID = 0x54c
                    0x054c                  _C2RXF3SIDbits = 0x54c
                    0x054e                  C2RXF3EID = 0x54e
                    0x054e                  _C2RXF3EID = 0x54e
                    0x054e                  _C2RXF3EIDbits = 0x54e
                    0x0550                  C2RXF4SID = 0x550
                    0x0550                  _C2RXF4SID = 0x550
                    0x0550                  _C2RXF4SIDbits = 0x550
                    0x0552                  C2RXF4EID = 0x552
                    0x0552                  _C2RXF4EID = 0x552
                    0x0552                  _C2RXF4EIDbits = 0x552
                    0x0554                  C2RXF5SID = 0x554
                    0x0554                  _C2RXF5SID = 0x554
                    0x0554                  _C2RXF5SIDbits = 0x554
                    0x0556                  C2RXF5EID = 0x556
                    0x0556                  _C2RXF5EID = 0x556
                    0x0556                  _C2RXF5EIDbits = 0x556
                    0x0558                  C2RXF6SID = 0x558
                    0x0558                  _C2RXF6SID = 0x558
                    0x0558                  _C2RXF6SIDbits = 0x558
                    0x055a                  C2RXF6EID = 0x55a
                    0x055a                  _C2RXF6EID = 0x55a
                    0x055a                  _C2RXF6EIDbits = 0x55a
                    0x055c                  C2RXF7SID = 0x55c
                    0x055c                  _C2RXF7SID = 0x55c
                    0x055c                  _C2RXF7SIDbits = 0x55c
                    0x055e                  C2RXF7EID = 0x55e
                    0x055e                  _C2RXF7EID = 0x55e
                    0x055e                  _C2RXF7EIDbits = 0x55e
                    0x0560                  C2RXF8SID = 0x560
                    0x0560                  _C2RXF8SID = 0x560
                    0x0560                  _C2RXF8SIDbits = 0x560
                    0x0562                  C2RXF8EID = 0x562
                    0x0562                  _C2RXF8EID = 0x562
                    0x0562                  _C2RXF8EIDbits = 0x562
                    0x0564                  C2RXF9SID = 0x564
                    0x0564                  _C2RXF9SID = 0x564
                    0x0564                  _C2RXF9SIDbits = 0x564
                    0x0566                  C2RXF9EID = 0x566
                    0x0566                  _C2RXF9EID = 0x566
                    0x0566                  _C2RXF9EIDbits = 0x566
                    0x0568                  C2RXF10SID = 0x568
                    0x0568                  _C2RXF10SID = 0x568
                    0x0568                  _C2RXF10SIDbits = 0x568
                    0x056a                  C2RXF10EID = 0x56a
                    0x056a                  _C2RXF10EID = 0x56a
                    0x056a                  _C2RXF10EIDbits = 0x56a
                    0x056c                  C2RXF11SID = 0x56c
                    0x056c                  _C2RXF11SID = 0x56c
                    0x056c                  _C2RXF11SIDbits = 0x56c
                    0x056e                  C2RXF11EID = 0x56e
                    0x056e                  _C2RXF11EID = 0x56e
                    0x056e                  _C2RXF11EIDbits = 0x56e
                    0x0570                  C2RXF12SID = 0x570
                    0x0570                  _C2RXF12SID = 0x570
                    0x0570                  _C2RXF12SIDbits = 0x570
                    0x0572                  C2RXF12EID = 0x572
                    0x0572                  _C2RXF12EID = 0x572
                    0x0572                  _C2RXF12EIDbits = 0x572
                    0x0574                  C2RXF13SID = 0x574
                    0x0574                  _C2RXF13SID = 0x574
                    0x0574                  _C2RXF13SIDbits = 0x574
                    0x0576                  C2RXF13EID = 0x576
                    0x0576                  _C2RXF13EID = 0x576
                    0x0576                  _C2RXF13EIDbits = 0x576
                    0x0578                  C2RXF14SID = 0x578
                    0x0578                  _C2RXF14SID = 0x578
                    0x0578                  _C2RXF14SIDbits = 0x578
                    0x057a                  C2RXF14EID = 0x57a
                    0x057a                  _C2RXF14EID = 0x57a
                    0x057a                  _C2RXF14EIDbits = 0x57a
                    0x057c                  C2RXF15SID = 0x57c
                    0x057c                  _C2RXF15SID = 0x57c
                    0x057c                  _C2RXF15SIDbits = 0x57c
                    0x057e                  C2RXF15EID = 0x57e
                    0x057e                  _C2RXF15EID = 0x57e
                    0x057e                  _C2RXF15EIDbits = 0x57e
                    0x0580                  U1PWMRRS = 0x580
                    0x0580                  _U1PWMRRS = 0x580
                    0x0580                  _U1PWMRRSbits = 0x580
                    0x0582                  U1PWMCON = 0x582
                    0x0582                  _U1PWMCON = 0x582
                    0x0582                  _U1PWMCONbits = 0x582
                    0x05c0                  QEI2CON = 0x5c0
                    0x05c0                  _QEI2CON = 0x5c0
                    0x05c0                  _QEI2CONbits = 0x5c0
                    0x05c2                  QEI2IOC = 0x5c2
                    0x05c2                  _QEI2IOC = 0x5c2
                    0x05c2                  _QEI2IOCbits = 0x5c2
                    0x05c4                  QEI2STAT = 0x5c4
                    0x05c4                  _QEI2STAT = 0x5c4
                    0x05c4                  _QEI2STATbits = 0x5c4
                    0x05c6                  POS2CNTL = 0x5c6
                    0x05c6                  _POS2CNTL = 0x5c6
                    0x05c8                  POS2CNTH = 0x5c8
                    0x05c8                  _POS2CNTH = 0x5c8
                    0x05ca                  POS2HLD = 0x5ca
                    0x05ca                  _POS2HLD = 0x5ca
                    0x05cc                  VEL2CNT = 0x5cc
                    0x05cc                  _VEL2CNT = 0x5cc
                    0x05ce                  INT2TMRL = 0x5ce
                    0x05ce                  _INT2TMRL = 0x5ce
                    0x05d0                  INT2TMRH = 0x5d0
                    0x05d0                  _INT2TMRH = 0x5d0
                    0x05d2                  INT2HLDL = 0x5d2
                    0x05d2                  _INT2HLDL = 0x5d2
                    0x05d4                  INT2HLDH = 0x5d4
                    0x05d4                  _INT2HLDH = 0x5d4
                    0x05d6                  INDX2CNTL = 0x5d6
                    0x05d6                  _INDX2CNTL = 0x5d6
                    0x05d8                  INDX2CNTH = 0x5d8
                    0x05d8                  _INDX2CNTH = 0x5d8
                    0x05da                  INDX2HLD = 0x5da
                    0x05da                  _INDX2HLD = 0x5da
                    0x05dc                  QEI2GECL = 0x5dc
                    0x05dc                  _QEI2GECL = 0x5dc
                    0x05dc                  QEI2ICL = 0x5dc
                    0x05dc                  _QEI2ICL = 0x5dc
                    0x05de                  QEI2GECH = 0x5de
                    0x05de                  _QEI2GECH = 0x5de
                    0x05de                  QEI2ICH = 0x5de
                    0x05de                  _QEI2ICH = 0x5de
                    0x05e0                  QEI2LECL = 0x5e0
                    0x05e0                  _QEI2LECL = 0x5e0
                    0x05e2                  QEI2LECH = 0x5e2
                    0x05e2                  _QEI2LECH = 0x5e2
                    0x0600                  PMCON = 0x600
                    0x0600                  _PMCON = 0x600
                    0x0600                  _PMCONbits = 0x600
                    0x0602                  PMMODE = 0x602
                    0x0602                  _PMMODE = 0x602
                    0x0602                  _PMMODEbits = 0x602
                    0x0604                  PMADDR = 0x604
                    0x0604                  _PMADDR = 0x604
                    0x0604                  _PMADDRbits = 0x604
                    0x0604                  PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1 = 0x604
                    0x0604                  _PMDOUT1bits = 0x604
                    0x0606                  PMDOUT2 = 0x606
                    0x0606                  _PMDOUT2 = 0x606
                    0x0608                  PMDIN1 = 0x608
                    0x0608                  _PMDIN1 = 0x608
                    0x060a                  PMDIN2 = 0x60a
                    0x060a                  _PMDIN2 = 0x60a
                    0x060c                  PMAEN = 0x60c
                    0x060c                  _PMAEN = 0x60c
                    0x060c                  _PMAENbits = 0x60c
                    0x060e                  PMSTAT = 0x60e
                    0x060e                  _PMSTAT = 0x60e
                    0x060e                  _PMSTATbits = 0x60e
                    0x0620                  ALRMVAL = 0x620
                    0x0620                  _ALRMVAL = 0x620
                    0x0622                  ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPT = 0x622
                    0x0622                  _ALCFGRPTbits = 0x622
                    0x0624                  RTCVAL = 0x624
                    0x0624                  _RTCVAL = 0x624
                    0x0626                  RCFGCAL = 0x626
                    0x0626                  _RCFGCAL = 0x626
                    0x0626                  _RCFGCALbits = 0x626
                    0x0640                  CRCCON1 = 0x640
                    0x0640                  _CRCCON1 = 0x640
                    0x0640                  _CRCCON1bits = 0x640
                    0x0642                  CRCCON2 = 0x642
                    0x0642                  _CRCCON2 = 0x642
                    0x0642                  _CRCCON2bits = 0x642
                    0x0644                  CRCXORL = 0x644
                    0x0644                  _CRCXORL = 0x644
                    0x0644                  _CRCXORLbits = 0x644
                    0x0646                  CRCXORH = 0x646
                    0x0646                  _CRCXORH = 0x646
                    0x0646                  _CRCXORHbits = 0x646
                    0x0648                  CRCDAT = 0x648
                    0x0648                  _CRCDAT = 0x648
                    0x0648                  CRCDATL = 0x648
                    0x0648                  _CRCDATL = 0x648
                    0x064a                  CRCDATH = 0x64a
                    0x064a                  _CRCDATH = 0x64a
                    0x064c                  CRCWDAT = 0x64c
                    0x064c                  _CRCWDAT = 0x64c
                    0x064c                  CRCWDATL = 0x64c
                    0x064c                  _CRCWDATL = 0x64c
                    0x064e                  CRCWDATH = 0x64e
                    0x064e                  _CRCWDATH = 0x64e
                    0x0680                  RPOR0 = 0x680
                    0x0680                  _RPOR0 = 0x680
                    0x0680                  _RPOR0bits = 0x680
                    0x0682                  RPOR1 = 0x682
                    0x0682                  _RPOR1 = 0x682
                    0x0682                  _RPOR1bits = 0x682
                    0x0684                  RPOR2 = 0x684
                    0x0684                  _RPOR2 = 0x684
                    0x0684                  _RPOR2bits = 0x684
                    0x0686                  RPOR3 = 0x686
                    0x0686                  _RPOR3 = 0x686
                    0x0686                  _RPOR3bits = 0x686
                    0x0688                  RPOR4 = 0x688
                    0x0688                  _RPOR4 = 0x688
                    0x0688                  _RPOR4bits = 0x688
                    0x068a                  RPOR5 = 0x68a
                    0x068a                  _RPOR5 = 0x68a
                    0x068a                  _RPOR5bits = 0x68a
                    0x068c                  RPOR6 = 0x68c
                    0x068c                  _RPOR6 = 0x68c
                    0x068c                  _RPOR6bits = 0x68c
                    0x068e                  RPOR7 = 0x68e
                    0x068e                  _RPOR7 = 0x68e
                    0x068e                  _RPOR7bits = 0x68e
                    0x0690                  RPOR8 = 0x690
                    0x0690                  _RPOR8 = 0x690
                    0x0690                  _RPOR8bits = 0x690
                    0x0692                  RPOR9 = 0x692
                    0x0692                  _RPOR9 = 0x692
                    0x0692                  _RPOR9bits = 0x692
                    0x0696                  RPOR11 = 0x696
                    0x0696                  _RPOR11 = 0x696
                    0x0696                  _RPOR11bits = 0x696
                    0x0698                  RPOR12 = 0x698
                    0x0698                  _RPOR12 = 0x698
                    0x0698                  _RPOR12bits = 0x698
                    0x069a                  RPOR13 = 0x69a
                    0x069a                  _RPOR13 = 0x69a
                    0x069a                  _RPOR13bits = 0x69a
                    0x069c                  RPOR14 = 0x69c
                    0x069c                  _RPOR14 = 0x69c
                    0x069c                  _RPOR14bits = 0x69c
                    0x069e                  RPOR15 = 0x69e
                    0x069e                  _RPOR15 = 0x69e
                    0x069e                  _RPOR15bits = 0x69e
                    0x06a0                  RPINR0 = 0x6a0
                    0x06a0                  _RPINR0 = 0x6a0
                    0x06a0                  _RPINR0bits = 0x6a0
                    0x06a2                  RPINR1 = 0x6a2
                    0x06a2                  _RPINR1 = 0x6a2
                    0x06a2                  _RPINR1bits = 0x6a2
                    0x06a4                  RPINR2 = 0x6a4
                    0x06a4                  _RPINR2 = 0x6a4
                    0x06a4                  _RPINR2bits = 0x6a4
                    0x06a6                  RPINR3 = 0x6a6
                    0x06a6                  _RPINR3 = 0x6a6
                    0x06a6                  _RPINR3bits = 0x6a6
                    0x06a8                  RPINR4 = 0x6a8
                    0x06a8                  _RPINR4 = 0x6a8
                    0x06a8                  _RPINR4bits = 0x6a8
                    0x06aa                  RPINR5 = 0x6aa
                    0x06aa                  _RPINR5 = 0x6aa
                    0x06aa                  _RPINR5bits = 0x6aa
                    0x06ac                  RPINR6 = 0x6ac
                    0x06ac                  _RPINR6 = 0x6ac
                    0x06ac                  _RPINR6bits = 0x6ac
                    0x06ae                  RPINR7 = 0x6ae
                    0x06ae                  _RPINR7 = 0x6ae
                    0x06ae                  _RPINR7bits = 0x6ae
                    0x06b0                  RPINR8 = 0x6b0
                    0x06b0                  _RPINR8 = 0x6b0
                    0x06b0                  _RPINR8bits = 0x6b0
                    0x06b2                  RPINR9 = 0x6b2
                    0x06b2                  _RPINR9 = 0x6b2
                    0x06b2                  _RPINR9bits = 0x6b2
                    0x06b4                  RPINR10 = 0x6b4
                    0x06b4                  _RPINR10 = 0x6b4
                    0x06b4                  _RPINR10bits = 0x6b4
                    0x06b6                  RPINR11 = 0x6b6
                    0x06b6                  _RPINR11 = 0x6b6
                    0x06b6                  _RPINR11bits = 0x6b6
                    0x06b8                  RPINR12 = 0x6b8
                    0x06b8                  _RPINR12 = 0x6b8
                    0x06b8                  _RPINR12bits = 0x6b8
                    0x06ba                  RPINR13 = 0x6ba
                    0x06ba                  _RPINR13 = 0x6ba
                    0x06ba                  _RPINR13bits = 0x6ba
                    0x06bc                  RPINR14 = 0x6bc
                    0x06bc                  _RPINR14 = 0x6bc
                    0x06bc                  _RPINR14bits = 0x6bc
                    0x06be                  RPINR15 = 0x6be
                    0x06be                  _RPINR15 = 0x6be
                    0x06be                  _RPINR15bits = 0x6be
                    0x06c0                  RPINR16 = 0x6c0
                    0x06c0                  _RPINR16 = 0x6c0
                    0x06c0                  _RPINR16bits = 0x6c0
                    0x06c2                  RPINR17 = 0x6c2
                    0x06c2                  _RPINR17 = 0x6c2
                    0x06c2                  _RPINR17bits = 0x6c2
                    0x06c4                  RPINR18 = 0x6c4
                    0x06c4                  _RPINR18 = 0x6c4
                    0x06c4                  _RPINR18bits = 0x6c4
                    0x06c6                  RPINR19 = 0x6c6
                    0x06c6                  _RPINR19 = 0x6c6
                    0x06c6                  _RPINR19bits = 0x6c6
                    0x06c8                  RPINR20 = 0x6c8
                    0x06c8                  _RPINR20 = 0x6c8
                    0x06c8                  _RPINR20bits = 0x6c8
                    0x06ca                  RPINR21 = 0x6ca
                    0x06ca                  _RPINR21 = 0x6ca
                    0x06ca                  _RPINR21bits = 0x6ca
                    0x06ce                  RPINR23 = 0x6ce
                    0x06ce                  _RPINR23 = 0x6ce
                    0x06ce                  _RPINR23bits = 0x6ce
                    0x06d0                  RPINR24 = 0x6d0
                    0x06d0                  _RPINR24 = 0x6d0
                    0x06d0                  _RPINR24bits = 0x6d0
                    0x06d2                  RPINR25 = 0x6d2
                    0x06d2                  _RPINR25 = 0x6d2
                    0x06d2                  _RPINR25bits = 0x6d2
                    0x06d4                  RPINR26 = 0x6d4
                    0x06d4                  _RPINR26 = 0x6d4
                    0x06d4                  _RPINR26bits = 0x6d4
                    0x06d6                  RPINR27 = 0x6d6
                    0x06d6                  _RPINR27 = 0x6d6
                    0x06d6                  _RPINR27bits = 0x6d6
                    0x06d8                  RPINR28 = 0x6d8
                    0x06d8                  _RPINR28 = 0x6d8
                    0x06d8                  _RPINR28bits = 0x6d8
                    0x06da                  RPINR29 = 0x6da
                    0x06da                  _RPINR29 = 0x6da
                    0x06da                  _RPINR29bits = 0x6da
                    0x06dc                  RPINR30 = 0x6dc
                    0x06dc                  _RPINR30 = 0x6dc
                    0x06dc                  _RPINR30bits = 0x6dc
                    0x06de                  RPINR31 = 0x6de
                    0x06de                  _RPINR31 = 0x6de
                    0x06de                  _RPINR31bits = 0x6de
                    0x06e0                  RPINR32 = 0x6e0
                    0x06e0                  _RPINR32 = 0x6e0
                    0x06e0                  _RPINR32bits = 0x6e0
                    0x06e2                  RPINR33 = 0x6e2
                    0x06e2                  _RPINR33 = 0x6e2
                    0x06e2                  _RPINR33bits = 0x6e2
                    0x06e4                  RPINR34 = 0x6e4
                    0x06e4                  _RPINR34 = 0x6e4
                    0x06e4                  _RPINR34bits = 0x6e4
                    0x06e6                  RPINR35 = 0x6e6
                    0x06e6                  _RPINR35 = 0x6e6
                    0x06e6                  _RPINR35bits = 0x6e6
                    0x06e8                  RPINR36 = 0x6e8
                    0x06e8                  _RPINR36 = 0x6e8
                    0x06e8                  _RPINR36bits = 0x6e8
                    0x06ea                  RPINR37 = 0x6ea
                    0x06ea                  _RPINR37 = 0x6ea
                    0x06ea                  _RPINR37bits = 0x6ea
                    0x06ec                  RPINR38 = 0x6ec
                    0x06ec                  _RPINR38 = 0x6ec
                    0x06ec                  _RPINR38bits = 0x6ec
                    0x06ee                  RPINR39 = 0x6ee
                    0x06ee                  _RPINR39 = 0x6ee
                    0x06ee                  _RPINR39bits = 0x6ee
                    0x06f0                  RPINR40 = 0x6f0
                    0x06f0                  _RPINR40 = 0x6f0
                    0x06f0                  _RPINR40bits = 0x6f0
                    0x06f2                  RPINR41 = 0x6f2
                    0x06f2                  _RPINR41 = 0x6f2
                    0x06f2                  _RPINR41bits = 0x6f2
                    0x06f4                  RPINR42 = 0x6f4
                    0x06f4                  _RPINR42 = 0x6f4
                    0x06f4                  _RPINR42bits = 0x6f4
                    0x06f6                  RPINR43 = 0x6f6
                    0x06f6                  _RPINR43 = 0x6f6
                    0x06f6                  _RPINR43bits = 0x6f6
                    0x0728                  NVMCON = 0x728
                    0x0728                  _NVMCON = 0x728
                    0x0728                  _NVMCONbits = 0x728
                    0x072a                  NVMADR = 0x72a
                    0x072a                  _NVMADR = 0x72a
                    0x072c                  NVMADRU = 0x72c
                    0x072c                  _NVMADRU = 0x72c
                    0x072c                  _NVMADRUbits = 0x72c
                    0x072e                  NVMKEY = 0x72e
                    0x072e                  _NVMKEY = 0x72e
                    0x0740                  RCON = 0x740
                    0x0740                  _RCON = 0x740
                    0x0740                  _RCONbits = 0x740
                    0x0742                  OSCCON = 0x742
                    0x0742                  _OSCCON = 0x742
                    0x0742                  _OSCCONbits = 0x742
                    0x0742                  OSCCONL = 0x742
                    0x0742                  _OSCCONL = 0x742
                    0x0743                  OSCCONH = 0x743
                    0x0743                  _OSCCONH = 0x743
                    0x0744                  CLKDIV = 0x744
                    0x0744                  _CLKDIV = 0x744
                    0x0744                  _CLKDIVbits = 0x744
                    0x0746                  PLLFBD = 0x746
                    0x0746                  _PLLFBD = 0x746
                    0x0746                  _PLLFBDbits = 0x746
                    0x0748                  OSCTUN = 0x748
                    0x0748                  _OSCTUN = 0x748
                    0x0748                  _OSCTUNbits = 0x748
                    0x074e                  REFOCON = 0x74e
                    0x074e                  _REFOCON = 0x74e
                    0x074e                  _REFOCONbits = 0x74e
                    0x0758                  ACLKCON3 = 0x758
                    0x0758                  _ACLKCON3 = 0x758
                    0x0758                  _ACLKCON3bits = 0x758
                    0x075a                  ACLKDIV3 = 0x75a
                    0x075a                  _ACLKDIV3 = 0x75a
                    0x075a                  _ACLKDIV3bits = 0x75a
                    0x0760                  PMD1 = 0x760
                    0x0760                  _PMD1 = 0x760
                    0x0760                  _PMD1bits = 0x760
                    0x0762                  PMD2 = 0x762
                    0x0762                  _PMD2 = 0x762
                    0x0762                  _PMD2bits = 0x762
                    0x0764                  PMD3 = 0x764
                    0x0764                  _PMD3 = 0x764
                    0x0764                  _PMD3bits = 0x764
                    0x0766                  PMD4 = 0x766
                    0x0766                  _PMD4 = 0x766
                    0x0766                  _PMD4bits = 0x766
                    0x0768                  PMD5 = 0x768
                    0x0768                  _PMD5 = 0x768
                    0x0768                  _PMD5bits = 0x768
                    0x076a                  PMD6 = 0x76a
                    0x076a                  _PMD6 = 0x76a
                    0x076a                  _PMD6bits = 0x76a
                    0x076c                  PMD7 = 0x76c
                    0x076c                  _PMD7 = 0x76c
                    0x076c                  _PMD7bits = 0x76c
                    0x0800                  IFS0 = 0x800
                    0x0800                  _IFS0 = 0x800
                    0x0800                  _IFS0bits = 0x800
                    0x0802                  IFS1 = 0x802
                    0x0802                  _IFS1 = 0x802
                    0x0802                  _IFS1bits = 0x802
                    0x0804                  IFS2 = 0x804
                    0x0804                  _IFS2 = 0x804
                    0x0804                  _IFS2bits = 0x804
                    0x0806                  IFS3 = 0x806
                    0x0806                  _IFS3 = 0x806
                    0x0806                  _IFS3bits = 0x806
                    0x0808                  IFS4 = 0x808
                    0x0808                  _IFS4 = 0x808
                    0x0808                  _IFS4bits = 0x808
                    0x080a                  IFS5 = 0x80a
                    0x080a                  _IFS5 = 0x80a
                    0x080a                  _IFS5bits = 0x80a
                    0x080c                  IFS6 = 0x80c
                    0x080c                  _IFS6 = 0x80c
                    0x080c                  _IFS6bits = 0x80c
                    0x080e                  IFS7 = 0x80e
                    0x080e                  _IFS7 = 0x80e
                    0x080e                  _IFS7bits = 0x80e
                    0x0810                  IFS8 = 0x810
                    0x0810                  _IFS8 = 0x810
                    0x0810                  _IFS8bits = 0x810
                    0x0820                  IEC0 = 0x820
                    0x0820                  _IEC0 = 0x820
                    0x0820                  _IEC0bits = 0x820
                    0x0822                  IEC1 = 0x822
                    0x0822                  _IEC1 = 0x822
                    0x0822                  _IEC1bits = 0x822
                    0x0824                  IEC2 = 0x824
                    0x0824                  _IEC2 = 0x824
                    0x0824                  _IEC2bits = 0x824
                    0x0826                  IEC3 = 0x826
                    0x0826                  _IEC3 = 0x826
                    0x0826                  _IEC3bits = 0x826
                    0x0828                  IEC4 = 0x828
                    0x0828                  _IEC4 = 0x828
                    0x0828                  _IEC4bits = 0x828
                    0x082a                  IEC5 = 0x82a
                    0x082a                  _IEC5 = 0x82a
                    0x082a                  _IEC5bits = 0x82a
                    0x082c                  IEC6 = 0x82c
                    0x082c                  _IEC6 = 0x82c
                    0x082c                  _IEC6bits = 0x82c
                    0x082e                  IEC7 = 0x82e
                    0x082e                  _IEC7 = 0x82e
                    0x082e                  _IEC7bits = 0x82e
                    0x0830                  IEC8 = 0x830
                    0x0830                  _IEC8 = 0x830
                    0x0830                  _IEC8bits = 0x830
                    0x0840                  IPC0 = 0x840
                    0x0840                  _IPC0 = 0x840
                    0x0840                  _IPC0bits = 0x840
                    0x0842                  IPC1 = 0x842
                    0x0842                  _IPC1 = 0x842
                    0x0842                  _IPC1bits = 0x842
                    0x0844                  IPC2 = 0x844
                    0x0844                  _IPC2 = 0x844
                    0x0844                  _IPC2bits = 0x844
                    0x0846                  IPC3 = 0x846
                    0x0846                  _IPC3 = 0x846
                    0x0846                  _IPC3bits = 0x846
                    0x0848                  IPC4 = 0x848
                    0x0848                  _IPC4 = 0x848
                    0x0848                  _IPC4bits = 0x848
                    0x084a                  IPC5 = 0x84a
                    0x084a                  _IPC5 = 0x84a
                    0x084a                  _IPC5bits = 0x84a
                    0x084c                  IPC6 = 0x84c
                    0x084c                  _IPC6 = 0x84c
                    0x084c                  _IPC6bits = 0x84c
                    0x084e                  IPC7 = 0x84e
                    0x084e                  _IPC7 = 0x84e
                    0x084e                  _IPC7bits = 0x84e
                    0x0850                  IPC8 = 0x850
                    0x0850                  _IPC8 = 0x850
                    0x0850                  _IPC8bits = 0x850
                    0x0852                  IPC9 = 0x852
                    0x0852                  _IPC9 = 0x852
                    0x0852                  _IPC9bits = 0x852
                    0x0854                  IPC10 = 0x854
                    0x0854                  _IPC10 = 0x854
                    0x0854                  _IPC10bits = 0x854
                    0x0856                  IPC11 = 0x856
                    0x0856                  _IPC11 = 0x856
                    0x0856                  _IPC11bits = 0x856
                    0x0858                  IPC12 = 0x858
                    0x0858                  _IPC12 = 0x858
                    0x0858                  _IPC12bits = 0x858
                    0x085a                  IPC13 = 0x85a
                    0x085a                  _IPC13 = 0x85a
                    0x085a                  _IPC13bits = 0x85a
                    0x085c                  IPC14 = 0x85c
                    0x085c                  _IPC14 = 0x85c
                    0x085c                  _IPC14bits = 0x85c
                    0x085e                  IPC15 = 0x85e
                    0x085e                  _IPC15 = 0x85e
                    0x085e                  _IPC15bits = 0x85e
                    0x0860                  IPC16 = 0x860
                    0x0860                  _IPC16 = 0x860
                    0x0860                  _IPC16bits = 0x860
                    0x0862                  IPC17 = 0x862
                    0x0862                  _IPC17 = 0x862
                    0x0862                  _IPC17bits = 0x862
                    0x0864                  IPC18 = 0x864
                    0x0864                  _IPC18 = 0x864
                    0x0864                  _IPC18bits = 0x864
                    0x0868                  IPC20 = 0x868
                    0x0868                  _IPC20 = 0x868
                    0x0868                  _IPC20bits = 0x868
                    0x086a                  IPC21 = 0x86a
                    0x086a                  _IPC21 = 0x86a
                    0x086a                  _IPC21bits = 0x86a
                    0x086c                  IPC22 = 0x86c
                    0x086c                  _IPC22 = 0x86c
                    0x086c                  _IPC22bits = 0x86c
                    0x086e                  IPC23 = 0x86e
                    0x086e                  _IPC23 = 0x86e
                    0x086e                  _IPC23bits = 0x86e
                    0x0870                  IPC24 = 0x870
                    0x0870                  _IPC24 = 0x870
                    0x0870                  _IPC24bits = 0x870
                    0x087a                  IPC29 = 0x87a
                    0x087a                  _IPC29 = 0x87a
                    0x087a                  _IPC29bits = 0x87a
                    0x087c                  IPC30 = 0x87c
                    0x087c                  _IPC30 = 0x87c
                    0x087c                  _IPC30bits = 0x87c
                    0x087e                  IPC31 = 0x87e
                    0x087e                  _IPC31 = 0x87e
                    0x087e                  _IPC31bits = 0x87e
                    0x0880                  IPC32 = 0x880
                    0x0880                  _IPC32 = 0x880
                    0x0880                  _IPC32bits = 0x880
                    0x0882                  IPC33 = 0x882
                    0x0882                  _IPC33 = 0x882
                    0x0882                  _IPC33bits = 0x882
                    0x0884                  IPC34 = 0x884
                    0x0884                  _IPC34 = 0x884
                    0x0884                  _IPC34bits = 0x884
                    0x0886                  IPC35 = 0x886
                    0x0886                  _IPC35 = 0x886
                    0x0886                  _IPC35bits = 0x886
                    0x08c0                  INTCON1 = 0x8c0
                    0x08c0                  _INTCON1 = 0x8c0
                    0x08c0                  _INTCON1bits = 0x8c0
                    0x08c2                  INTCON2 = 0x8c2
                    0x08c2                  _INTCON2 = 0x8c2
                    0x08c2                  _INTCON2bits = 0x8c2
                    0x08c4                  INTCON3 = 0x8c4
                    0x08c4                  _INTCON3 = 0x8c4
                    0x08c4                  _INTCON3bits = 0x8c4
                    0x08c6                  INTCON4 = 0x8c6
                    0x08c6                  _INTCON4 = 0x8c6
                    0x08c6                  _INTCON4bits = 0x8c6
                    0x08c8                  INTTREG = 0x8c8
                    0x08c8                  _INTTREG = 0x8c8
                    0x08c8                  _INTTREGbits = 0x8c8
                    0x0900                  OC1CON1 = 0x900
                    0x0900                  _OC1CON1 = 0x900
                    0x0900                  _OC1CON1bits = 0x900
                    0x0902                  OC1CON2 = 0x902
                    0x0902                  _OC1CON2 = 0x902
                    0x0902                  _OC1CON2bits = 0x902
                    0x0904                  OC1RS = 0x904
                    0x0904                  _OC1RS = 0x904
                    0x0906                  OC1R = 0x906
                    0x0906                  _OC1R = 0x906
                    0x0908                  OC1TMR = 0x908
                    0x0908                  _OC1TMR = 0x908
                    0x090a                  OC2CON1 = 0x90a
                    0x090a                  _OC2CON1 = 0x90a
                    0x090a                  _OC2CON1bits = 0x90a
                    0x090c                  OC2CON2 = 0x90c
                    0x090c                  _OC2CON2 = 0x90c
                    0x090c                  _OC2CON2bits = 0x90c
                    0x090e                  OC2RS = 0x90e
                    0x090e                  _OC2RS = 0x90e
                    0x0910                  OC2R = 0x910
                    0x0910                  _OC2R = 0x910
                    0x0912                  OC2TMR = 0x912
                    0x0912                  _OC2TMR = 0x912
                    0x0914                  OC3CON1 = 0x914
                    0x0914                  _OC3CON1 = 0x914
                    0x0914                  _OC3CON1bits = 0x914
                    0x0916                  OC3CON2 = 0x916
                    0x0916                  _OC3CON2 = 0x916
                    0x0916                  _OC3CON2bits = 0x916
                    0x0918                  OC3RS = 0x918
                    0x0918                  _OC3RS = 0x918
                    0x091a                  OC3R = 0x91a
                    0x091a                  _OC3R = 0x91a
                    0x091c                  OC3TMR = 0x91c
                    0x091c                  _OC3TMR = 0x91c
                    0x091e                  OC4CON1 = 0x91e
                    0x091e                  _OC4CON1 = 0x91e
                    0x091e                  _OC4CON1bits = 0x91e
                    0x0920                  OC4CON2 = 0x920
                    0x0920                  _OC4CON2 = 0x920
                    0x0920                  _OC4CON2bits = 0x920
                    0x0922                  OC4RS = 0x922
                    0x0922                  _OC4RS = 0x922
                    0x0924                  OC4R = 0x924
                    0x0924                  _OC4R = 0x924
                    0x0926                  OC4TMR = 0x926
                    0x0926                  _OC4TMR = 0x926
                    0x0928                  OC5CON1 = 0x928
                    0x0928                  _OC5CON1 = 0x928
                    0x0928                  _OC5CON1bits = 0x928
                    0x092a                  OC5CON2 = 0x92a
                    0x092a                  _OC5CON2 = 0x92a
                    0x092a                  _OC5CON2bits = 0x92a
                    0x092c                  OC5RS = 0x92c
                    0x092c                  _OC5RS = 0x92c
                    0x092e                  OC5R = 0x92e
                    0x092e                  _OC5R = 0x92e
                    0x0930                  OC5TMR = 0x930
                    0x0930                  _OC5TMR = 0x930
                    0x0932                  OC6CON1 = 0x932
                    0x0932                  _OC6CON1 = 0x932
                    0x0932                  _OC6CON1bits = 0x932
                    0x0934                  OC6CON2 = 0x934
                    0x0934                  _OC6CON2 = 0x934
                    0x0934                  _OC6CON2bits = 0x934
                    0x0936                  OC6RS = 0x936
                    0x0936                  _OC6RS = 0x936
                    0x0938                  OC6R = 0x938
                    0x0938                  _OC6R = 0x938
                    0x093a                  OC6TMR = 0x93a
                    0x093a                  _OC6TMR = 0x93a
                    0x093c                  OC7CON1 = 0x93c
                    0x093c                  _OC7CON1 = 0x93c
                    0x093c                  _OC7CON1bits = 0x93c
                    0x093e                  OC7CON2 = 0x93e
                    0x093e                  _OC7CON2 = 0x93e
                    0x093e                  _OC7CON2bits = 0x93e
                    0x0940                  OC7RS = 0x940
                    0x0940                  _OC7RS = 0x940
                    0x0942                  OC7R = 0x942
                    0x0942                  _OC7R = 0x942
                    0x0944                  OC7TMR = 0x944
                    0x0944                  _OC7TMR = 0x944
                    0x0946                  OC8CON1 = 0x946
                    0x0946                  _OC8CON1 = 0x946
                    0x0946                  _OC8CON1bits = 0x946
                    0x0948                  OC8CON2 = 0x948
                    0x0948                  _OC8CON2 = 0x948
                    0x0948                  _OC8CON2bits = 0x948
                    0x094a                  OC8RS = 0x94a
                    0x094a                  _OC8RS = 0x94a
                    0x094c                  OC8R = 0x94c
                    0x094c                  _OC8R = 0x94c
                    0x094e                  OC8TMR = 0x94e
                    0x094e                  _OC8TMR = 0x94e
                    0x0950                  OC9CON1 = 0x950
                    0x0950                  _OC9CON1 = 0x950
                    0x0950                  _OC9CON1bits = 0x950
                    0x0952                  OC9CON2 = 0x952
                    0x0952                  _OC9CON2 = 0x952
                    0x0952                  _OC9CON2bits = 0x952
                    0x0954                  OC9RS = 0x954
                    0x0954                  _OC9RS = 0x954
                    0x0956                  OC9R = 0x956
                    0x0956                  _OC9R = 0x956
                    0x0958                  OC9TMR = 0x958
                    0x0958                  _OC9TMR = 0x958
                    0x095a                  OC10CON1 = 0x95a
                    0x095a                  _OC10CON1 = 0x95a
                    0x095a                  _OC10CON1bits = 0x95a
                    0x095c                  OC10CON2 = 0x95c
                    0x095c                  _OC10CON2 = 0x95c
                    0x095c                  _OC10CON2bits = 0x95c
                    0x095e                  OC10RS = 0x95e
                    0x095e                  _OC10RS = 0x95e
                    0x0960                  OC10R = 0x960
                    0x0960                  _OC10R = 0x960
                    0x0962                  OC10TMR = 0x962
                    0x0962                  _OC10TMR = 0x962
                    0x0964                  OC11CON1 = 0x964
                    0x0964                  _OC11CON1 = 0x964
                    0x0964                  _OC11CON1bits = 0x964
                    0x0966                  OC11CON2 = 0x966
                    0x0966                  _OC11CON2 = 0x966
                    0x0966                  _OC11CON2bits = 0x966
                    0x0968                  OC11RS = 0x968
                    0x0968                  _OC11RS = 0x968
                    0x096a                  OC11R = 0x96a
                    0x096a                  _OC11R = 0x96a
                    0x096c                  OC11TMR = 0x96c
                    0x096c                  _OC11TMR = 0x96c
                    0x096e                  OC12CON1 = 0x96e
                    0x096e                  _OC12CON1 = 0x96e
                    0x096e                  _OC12CON1bits = 0x96e
                    0x0970                  OC12CON2 = 0x970
                    0x0970                  _OC12CON2 = 0x970
                    0x0970                  _OC12CON2bits = 0x970
                    0x0972                  OC12RS = 0x972
                    0x0972                  _OC12RS = 0x972
                    0x0974                  OC12R = 0x974
                    0x0974                  _OC12R = 0x974
                    0x0976                  OC12TMR = 0x976
                    0x0976                  _OC12TMR = 0x976
                    0x0978                  OC13CON1 = 0x978
                    0x0978                  _OC13CON1 = 0x978
                    0x0978                  _OC13CON1bits = 0x978
                    0x097a                  OC13CON2 = 0x97a
                    0x097a                  _OC13CON2 = 0x97a
                    0x097a                  _OC13CON2bits = 0x97a
                    0x097c                  OC13RS = 0x97c
                    0x097c                  _OC13RS = 0x97c
                    0x097e                  OC13R = 0x97e
                    0x097e                  _OC13R = 0x97e
                    0x0980                  OC13TMR = 0x980
                    0x0980                  _OC13TMR = 0x980
                    0x0982                  OC14CON1 = 0x982
                    0x0982                  _OC14CON1 = 0x982
                    0x0982                  _OC14CON1bits = 0x982
                    0x0984                  OC14CON2 = 0x984
                    0x0984                  _OC14CON2 = 0x984
                    0x0984                  _OC14CON2bits = 0x984
                    0x0986                  OC14RS = 0x986
                    0x0986                  _OC14RS = 0x986
                    0x0988                  OC14R = 0x988
                    0x0988                  _OC14R = 0x988
                    0x098a                  OC14TMR = 0x98a
                    0x098a                  _OC14TMR = 0x98a
                    0x098c                  OC15CON1 = 0x98c
                    0x098c                  _OC15CON1 = 0x98c
                    0x098c                  _OC15CON1bits = 0x98c
                    0x098e                  OC15CON2 = 0x98e
                    0x098e                  _OC15CON2 = 0x98e
                    0x098e                  _OC15CON2bits = 0x98e
                    0x0990                  OC15RS = 0x990
                    0x0990                  _OC15RS = 0x990
                    0x0992                  OC15R = 0x992
                    0x0992                  _OC15R = 0x992
                    0x0994                  OC15TMR = 0x994
                    0x0994                  _OC15TMR = 0x994
                    0x0996                  OC16CON1 = 0x996
                    0x0996                  _OC16CON1 = 0x996
                    0x0996                  _OC16CON1bits = 0x996
                    0x0998                  OC16CON2 = 0x998
                    0x0998                  _OC16CON2 = 0x998
                    0x0998                  _OC16CON2bits = 0x998
                    0x099a                  OC16RS = 0x99a
                    0x099a                  _OC16RS = 0x99a
                    0x099c                  OC16R = 0x99c
                    0x099c                  _OC16R = 0x99c
                    0x099e                  OC16TMR = 0x99e
                    0x099e                  _OC16TMR = 0x99e
                    0x0a80                  CMSTAT = 0xa80
                    0x0a80                  _CMSTAT = 0xa80
                    0x0a80                  _CMSTATbits = 0xa80
                    0x0a82                  CVRCON = 0xa82
                    0x0a82                  _CVRCON = 0xa82
                    0x0a82                  _CVRCONbits = 0xa82
                    0x0a84                  CM1CON = 0xa84
                    0x0a84                  _CM1CON = 0xa84
                    0x0a84                  _CM1CONbits = 0xa84
                    0x0a86                  CM1MSKSRC = 0xa86
                    0x0a86                  _CM1MSKSRC = 0xa86
                    0x0a86                  _CM1MSKSRCbits = 0xa86
                    0x0a88                  CM1MSKCON = 0xa88
                    0x0a88                  _CM1MSKCON = 0xa88
                    0x0a88                  _CM1MSKCONbits = 0xa88
                    0x0a8a                  CM1FLTR = 0xa8a
                    0x0a8a                  _CM1FLTR = 0xa8a
                    0x0a8a                  _CM1FLTRbits = 0xa8a
                    0x0a8c                  CM2CON = 0xa8c
                    0x0a8c                  _CM2CON = 0xa8c
                    0x0a8c                  _CM2CONbits = 0xa8c
                    0x0a8e                  CM2MSKSRC = 0xa8e
                    0x0a8e                  _CM2MSKSRC = 0xa8e
                    0x0a8e                  _CM2MSKSRCbits = 0xa8e
                    0x0a90                  CM2MSKCON = 0xa90
                    0x0a90                  _CM2MSKCON = 0xa90
                    0x0a90                  _CM2MSKCONbits = 0xa90
                    0x0a92                  CM2FLTR = 0xa92
                    0x0a92                  _CM2FLTR = 0xa92
                    0x0a92                  _CM2FLTRbits = 0xa92
                    0x0a94                  CM3CON = 0xa94
                    0x0a94                  _CM3CON = 0xa94
                    0x0a94                  _CM3CONbits = 0xa94
                    0x0a96                  CM3MSKSRC = 0xa96
                    0x0a96                  _CM3MSKSRC = 0xa96
                    0x0a96                  _CM3MSKSRCbits = 0xa96
                    0x0a98                  CM3MSKCON = 0xa98
                    0x0a98                  _CM3MSKCON = 0xa98
                    0x0a98                  _CM3MSKCONbits = 0xa98
                    0x0a9a                  CM3FLTR = 0xa9a
                    0x0a9a                  _CM3FLTR = 0xa9a
                    0x0a9a                  _CM3FLTRbits = 0xa9a
                    0x0b00                  DMA0CON = 0xb00
                    0x0b00                  _DMA0CON = 0xb00
                    0x0b00                  _DMA0CONbits = 0xb00
                    0x0b02                  DMA0REQ = 0xb02
                    0x0b02                  _DMA0REQ = 0xb02
                    0x0b02                  _DMA0REQbits = 0xb02
                    0x0b04                  DMA0STAL = 0xb04
                    0x0b04                  _DMA0STAL = 0xb04
                    0x0b06                  DMA0STAH = 0xb06
                    0x0b06                  _DMA0STAH = 0xb06
                    0x0b06                  _DMA0STAHbits = 0xb06
                    0x0b08                  DMA0STBL = 0xb08
                    0x0b08                  _DMA0STBL = 0xb08
                    0x0b0a                  DMA0STBH = 0xb0a
                    0x0b0a                  _DMA0STBH = 0xb0a
                    0x0b0a                  _DMA0STBHbits = 0xb0a
                    0x0b0c                  DMA0PAD = 0xb0c
                    0x0b0c                  _DMA0PAD = 0xb0c
                    0x0b0e                  DMA0CNT = 0xb0e
                    0x0b0e                  _DMA0CNT = 0xb0e
                    0x0b0e                  _DMA0CNTbits = 0xb0e
                    0x0b10                  DMA1CON = 0xb10
                    0x0b10                  _DMA1CON = 0xb10
                    0x0b10                  _DMA1CONbits = 0xb10
                    0x0b12                  DMA1REQ = 0xb12
                    0x0b12                  _DMA1REQ = 0xb12
                    0x0b12                  _DMA1REQbits = 0xb12
                    0x0b14                  DMA1STAL = 0xb14
                    0x0b14                  _DMA1STAL = 0xb14
                    0x0b16                  DMA1STAH = 0xb16
                    0x0b16                  _DMA1STAH = 0xb16
                    0x0b16                  _DMA1STAHbits = 0xb16
                    0x0b18                  DMA1STBL = 0xb18
                    0x0b18                  _DMA1STBL = 0xb18
                    0x0b1a                  DMA1STBH = 0xb1a
                    0x0b1a                  _DMA1STBH = 0xb1a
                    0x0b1a                  _DMA1STBHbits = 0xb1a
                    0x0b1c                  DMA1PAD = 0xb1c
                    0x0b1c                  _DMA1PAD = 0xb1c
                    0x0b1e                  DMA1CNT = 0xb1e
                    0x0b1e                  _DMA1CNT = 0xb1e
                    0x0b1e                  _DMA1CNTbits = 0xb1e
                    0x0b20                  DMA2CON = 0xb20
                    0x0b20                  _DMA2CON = 0xb20
                    0x0b20                  _DMA2CONbits = 0xb20
                    0x0b22                  DMA2REQ = 0xb22
                    0x0b22                  _DMA2REQ = 0xb22
                    0x0b22                  _DMA2REQbits = 0xb22
                    0x0b24                  DMA2STAL = 0xb24
                    0x0b24                  _DMA2STAL = 0xb24
                    0x0b26                  DMA2STAH = 0xb26
                    0x0b26                  _DMA2STAH = 0xb26
                    0x0b26                  _DMA2STAHbits = 0xb26
                    0x0b28                  DMA2STBL = 0xb28
                    0x0b28                  _DMA2STBL = 0xb28
                    0x0b2a                  DMA2STBH = 0xb2a
                    0x0b2a                  _DMA2STBH = 0xb2a
                    0x0b2a                  _DMA2STBHbits = 0xb2a
                    0x0b2c                  DMA2PAD = 0xb2c
                    0x0b2c                  _DMA2PAD = 0xb2c
                    0x0b2e                  DMA2CNT = 0xb2e
                    0x0b2e                  _DMA2CNT = 0xb2e
                    0x0b2e                  _DMA2CNTbits = 0xb2e
                    0x0b30                  DMA3CON = 0xb30
                    0x0b30                  _DMA3CON = 0xb30
                    0x0b30                  _DMA3CONbits = 0xb30
                    0x0b32                  DMA3REQ = 0xb32
                    0x0b32                  _DMA3REQ = 0xb32
                    0x0b32                  _DMA3REQbits = 0xb32
                    0x0b34                  DMA3STAL = 0xb34
                    0x0b34                  _DMA3STAL = 0xb34
                    0x0b36                  DMA3STAH = 0xb36
                    0x0b36                  _DMA3STAH = 0xb36
                    0x0b36                  _DMA3STAHbits = 0xb36
                    0x0b38                  DMA3STBL = 0xb38
                    0x0b38                  _DMA3STBL = 0xb38
                    0x0b3a                  DMA3STBH = 0xb3a
                    0x0b3a                  _DMA3STBH = 0xb3a
                    0x0b3a                  _DMA3STBHbits = 0xb3a
                    0x0b3c                  DMA3PAD = 0xb3c
                    0x0b3c                  _DMA3PAD = 0xb3c
                    0x0b3e                  DMA3CNT = 0xb3e
                    0x0b3e                  _DMA3CNT = 0xb3e
                    0x0b3e                  _DMA3CNTbits = 0xb3e
                    0x0b40                  DMA4CON = 0xb40
                    0x0b40                  _DMA4CON = 0xb40
                    0x0b40                  _DMA4CONbits = 0xb40
                    0x0b42                  DMA4REQ = 0xb42
                    0x0b42                  _DMA4REQ = 0xb42
                    0x0b42                  _DMA4REQbits = 0xb42
                    0x0b44                  DMA4STAL = 0xb44
                    0x0b44                  _DMA4STAL = 0xb44
                    0x0b46                  DMA4STAH = 0xb46
                    0x0b46                  _DMA4STAH = 0xb46
                    0x0b46                  _DMA4STAHbits = 0xb46
                    0x0b48                  DMA4STBL = 0xb48
                    0x0b48                  _DMA4STBL = 0xb48
                    0x0b4a                  DMA4STBH = 0xb4a
                    0x0b4a                  _DMA4STBH = 0xb4a
                    0x0b4a                  _DMA4STBHbits = 0xb4a
                    0x0b4c                  DMA4PAD = 0xb4c
                    0x0b4c                  _DMA4PAD = 0xb4c
                    0x0b4e                  DMA4CNT = 0xb4e
                    0x0b4e                  _DMA4CNT = 0xb4e
                    0x0b4e                  _DMA4CNTbits = 0xb4e
                    0x0b50                  DMA5CON = 0xb50
                    0x0b50                  _DMA5CON = 0xb50
                    0x0b50                  _DMA5CONbits = 0xb50
                    0x0b52                  DMA5REQ = 0xb52
                    0x0b52                  _DMA5REQ = 0xb52
                    0x0b52                  _DMA5REQbits = 0xb52
                    0x0b54                  DMA5STAL = 0xb54
                    0x0b54                  _DMA5STAL = 0xb54
                    0x0b56                  DMA5STAH = 0xb56
                    0x0b56                  _DMA5STAH = 0xb56
                    0x0b56                  _DMA5STAHbits = 0xb56
                    0x0b58                  DMA5STBL = 0xb58
                    0x0b58                  _DMA5STBL = 0xb58
                    0x0b5a                  DMA5STBH = 0xb5a
                    0x0b5a                  _DMA5STBH = 0xb5a
                    0x0b5a                  _DMA5STBHbits = 0xb5a
                    0x0b5c                  DMA5PAD = 0xb5c
                    0x0b5c                  _DMA5PAD = 0xb5c
                    0x0b5e                  DMA5CNT = 0xb5e
                    0x0b5e                  _DMA5CNT = 0xb5e
                    0x0b5e                  _DMA5CNTbits = 0xb5e
                    0x0b60                  DMA6CON = 0xb60
                    0x0b60                  _DMA6CON = 0xb60
                    0x0b60                  _DMA6CONbits = 0xb60
                    0x0b62                  DMA6REQ = 0xb62
                    0x0b62                  _DMA6REQ = 0xb62
                    0x0b62                  _DMA6REQbits = 0xb62
                    0x0b64                  DMA6STAL = 0xb64
                    0x0b64                  _DMA6STAL = 0xb64
                    0x0b66                  DMA6STAH = 0xb66
                    0x0b66                  _DMA6STAH = 0xb66
                    0x0b66                  _DMA6STAHbits = 0xb66
                    0x0b68                  DMA6STBL = 0xb68
                    0x0b68                  _DMA6STBL = 0xb68
                    0x0b6a                  DMA6STBH = 0xb6a
                    0x0b6a                  _DMA6STBH = 0xb6a
                    0x0b6a                  _DMA6STBHbits = 0xb6a
                    0x0b6c                  DMA6PAD = 0xb6c
                    0x0b6c                  _DMA6PAD = 0xb6c
                    0x0b6e                  DMA6CNT = 0xb6e
                    0x0b6e                  _DMA6CNT = 0xb6e
                    0x0b6e                  _DMA6CNTbits = 0xb6e
                    0x0b70                  DMA7CON = 0xb70
                    0x0b70                  _DMA7CON = 0xb70
                    0x0b70                  _DMA7CONbits = 0xb70
                    0x0b72                  DMA7REQ = 0xb72
                    0x0b72                  _DMA7REQ = 0xb72
                    0x0b72                  _DMA7REQbits = 0xb72
                    0x0b74                  DMA7STAL = 0xb74
                    0x0b74                  _DMA7STAL = 0xb74
                    0x0b76                  DMA7STAH = 0xb76
                    0x0b76                  _DMA7STAH = 0xb76
                    0x0b76                  _DMA7STAHbits = 0xb76
                    0x0b78                  DMA7STBL = 0xb78
                    0x0b78                  _DMA7STBL = 0xb78
                    0x0b7a                  DMA7STBH = 0xb7a
                    0x0b7a                  _DMA7STBH = 0xb7a
                    0x0b7a                  _DMA7STBHbits = 0xb7a
                    0x0b7c                  DMA7PAD = 0xb7c
                    0x0b7c                  _DMA7PAD = 0xb7c
                    0x0b7e                  DMA7CNT = 0xb7e
                    0x0b7e                  _DMA7CNT = 0xb7e
                    0x0b7e                  _DMA7CNTbits = 0xb7e
                    0x0b80                  DMA8CON = 0xb80
                    0x0b80                  _DMA8CON = 0xb80
                    0x0b80                  _DMA8CONbits = 0xb80
                    0x0b82                  DMA8REQ = 0xb82
                    0x0b82                  _DMA8REQ = 0xb82
                    0x0b82                  _DMA8REQbits = 0xb82
                    0x0b84                  DMA8STAL = 0xb84
                    0x0b84                  _DMA8STAL = 0xb84
                    0x0b86                  DMA8STAH = 0xb86
                    0x0b86                  _DMA8STAH = 0xb86
                    0x0b86                  _DMA8STAHbits = 0xb86
                    0x0b88                  DMA8STBL = 0xb88
                    0x0b88                  _DMA8STBL = 0xb88
                    0x0b8a                  DMA8STBH = 0xb8a
                    0x0b8a                  _DMA8STBH = 0xb8a
                    0x0b8a                  _DMA8STBHbits = 0xb8a
                    0x0b8c                  DMA8PAD = 0xb8c
                    0x0b8c                  _DMA8PAD = 0xb8c
                    0x0b8e                  DMA8CNT = 0xb8e
                    0x0b8e                  _DMA8CNT = 0xb8e
                    0x0b8e                  _DMA8CNTbits = 0xb8e
                    0x0b90                  DMA9CON = 0xb90
                    0x0b90                  _DMA9CON = 0xb90
                    0x0b90                  _DMA9CONbits = 0xb90
                    0x0b92                  DMA9REQ = 0xb92
                    0x0b92                  _DMA9REQ = 0xb92
                    0x0b92                  _DMA9REQbits = 0xb92
                    0x0b94                  DMA9STAL = 0xb94
                    0x0b94                  _DMA9STAL = 0xb94
                    0x0b96                  DMA9STAH = 0xb96
                    0x0b96                  _DMA9STAH = 0xb96
                    0x0b96                  _DMA9STAHbits = 0xb96
                    0x0b98                  DMA9STBL = 0xb98
                    0x0b98                  _DMA9STBL = 0xb98
                    0x0b9a                  DMA9STBH = 0xb9a
                    0x0b9a                  _DMA9STBH = 0xb9a
                    0x0b9a                  _DMA9STBHbits = 0xb9a
                    0x0b9c                  DMA9PAD = 0xb9c
                    0x0b9c                  _DMA9PAD = 0xb9c
                    0x0b9e                  DMA9CNT = 0xb9e
                    0x0b9e                  _DMA9CNT = 0xb9e
                    0x0b9e                  _DMA9CNTbits = 0xb9e
                    0x0ba0                  DMA10CON = 0xba0
                    0x0ba0                  _DMA10CON = 0xba0
                    0x0ba0                  _DMA10CONbits = 0xba0
                    0x0ba2                  DMA10REQ = 0xba2
                    0x0ba2                  _DMA10REQ = 0xba2
                    0x0ba2                  _DMA10REQbits = 0xba2
                    0x0ba4                  DMA10STAL = 0xba4
                    0x0ba4                  _DMA10STAL = 0xba4
                    0x0ba6                  DMA10STAH = 0xba6
                    0x0ba6                  _DMA10STAH = 0xba6
                    0x0ba6                  _DMA10STAHbits = 0xba6
                    0x0ba8                  DMA10STBL = 0xba8
                    0x0ba8                  _DMA10STBL = 0xba8
                    0x0baa                  DMA10STBH = 0xbaa
                    0x0baa                  _DMA10STBH = 0xbaa
                    0x0baa                  _DMA10STBHbits = 0xbaa
                    0x0bac                  DMA10PAD = 0xbac
                    0x0bac                  _DMA10PAD = 0xbac
                    0x0bae                  DMA10CNT = 0xbae
                    0x0bae                  _DMA10CNT = 0xbae
                    0x0bae                  _DMA10CNTbits = 0xbae
                    0x0bb0                  DMA11CON = 0xbb0
                    0x0bb0                  _DMA11CON = 0xbb0
                    0x0bb0                  _DMA11CONbits = 0xbb0
                    0x0bb2                  DMA11REQ = 0xbb2
                    0x0bb2                  _DMA11REQ = 0xbb2
                    0x0bb2                  _DMA11REQbits = 0xbb2
                    0x0bb4                  DMA11STAL = 0xbb4
                    0x0bb4                  _DMA11STAL = 0xbb4
                    0x0bb6                  DMA11STAH = 0xbb6
                    0x0bb6                  _DMA11STAH = 0xbb6
                    0x0bb6                  _DMA11STAHbits = 0xbb6
                    0x0bb8                  DMA11STBL = 0xbb8
                    0x0bb8                  _DMA11STBL = 0xbb8
                    0x0bba                  DMA11STBH = 0xbba
                    0x0bba                  _DMA11STBH = 0xbba
                    0x0bba                  _DMA11STBHbits = 0xbba
                    0x0bbc                  DMA11PAD = 0xbbc
                    0x0bbc                  _DMA11PAD = 0xbbc
                    0x0bbe                  DMA11CNT = 0xbbe
                    0x0bbe                  _DMA11CNT = 0xbbe
                    0x0bbe                  _DMA11CNTbits = 0xbbe
                    0x0bc0                  DMA12CON = 0xbc0
                    0x0bc0                  _DMA12CON = 0xbc0
                    0x0bc0                  _DMA12CONbits = 0xbc0
                    0x0bc2                  DMA12REQ = 0xbc2
                    0x0bc2                  _DMA12REQ = 0xbc2
                    0x0bc2                  _DMA12REQbits = 0xbc2
                    0x0bc4                  DMA12STAL = 0xbc4
                    0x0bc4                  _DMA12STAL = 0xbc4
                    0x0bc6                  DMA12STAH = 0xbc6
                    0x0bc6                  _DMA12STAH = 0xbc6
                    0x0bc6                  _DMA12STAHbits = 0xbc6
                    0x0bc8                  DMA12STBL = 0xbc8
                    0x0bc8                  _DMA12STBL = 0xbc8
                    0x0bca                  DMA12STBH = 0xbca
                    0x0bca                  _DMA12STBH = 0xbca
                    0x0bca                  _DMA12STBHbits = 0xbca
                    0x0bcc                  DMA12PAD = 0xbcc
                    0x0bcc                  _DMA12PAD = 0xbcc
                    0x0bce                  DMA12CNT = 0xbce
                    0x0bce                  _DMA12CNT = 0xbce
                    0x0bce                  _DMA12CNTbits = 0xbce
                    0x0bd0                  DMA13CON = 0xbd0
                    0x0bd0                  _DMA13CON = 0xbd0
                    0x0bd0                  _DMA13CONbits = 0xbd0
                    0x0bd2                  DMA13REQ = 0xbd2
                    0x0bd2                  _DMA13REQ = 0xbd2
                    0x0bd2                  _DMA13REQbits = 0xbd2
                    0x0bd4                  DMA13STAL = 0xbd4
                    0x0bd4                  _DMA13STAL = 0xbd4
                    0x0bd6                  DMA13STAH = 0xbd6
                    0x0bd6                  _DMA13STAH = 0xbd6
                    0x0bd6                  _DMA13STAHbits = 0xbd6
                    0x0bd8                  DMA13STBL = 0xbd8
                    0x0bd8                  _DMA13STBL = 0xbd8
                    0x0bda                  DMA13STBH = 0xbda
                    0x0bda                  _DMA13STBH = 0xbda
                    0x0bda                  _DMA13STBHbits = 0xbda
                    0x0bdc                  DMA13PAD = 0xbdc
                    0x0bdc                  _DMA13PAD = 0xbdc
                    0x0bde                  DMA13CNT = 0xbde
                    0x0bde                  _DMA13CNT = 0xbde
                    0x0bde                  _DMA13CNTbits = 0xbde
                    0x0be0                  DMA14CON = 0xbe0
                    0x0be0                  _DMA14CON = 0xbe0
                    0x0be0                  _DMA14CONbits = 0xbe0
                    0x0be2                  DMA14REQ = 0xbe2
                    0x0be2                  _DMA14REQ = 0xbe2
                    0x0be2                  _DMA14REQbits = 0xbe2
                    0x0be4                  DMA14STAL = 0xbe4
                    0x0be4                  _DMA14STAL = 0xbe4
                    0x0be6                  DMA14STAH = 0xbe6
                    0x0be6                  _DMA14STAH = 0xbe6
                    0x0be6                  _DMA14STAHbits = 0xbe6
                    0x0be8                  DMA14STBL = 0xbe8
                    0x0be8                  _DMA14STBL = 0xbe8
                    0x0bea                  DMA14STBH = 0xbea
                    0x0bea                  _DMA14STBH = 0xbea
                    0x0bea                  _DMA14STBHbits = 0xbea
                    0x0bec                  DMA14PAD = 0xbec
                    0x0bec                  _DMA14PAD = 0xbec
                    0x0bee                  DMA14CNT = 0xbee
                    0x0bee                  _DMA14CNT = 0xbee
                    0x0bee                  _DMA14CNTbits = 0xbee
                    0x0bf0                  DMAPWC = 0xbf0
                    0x0bf0                  _DMAPWC = 0xbf0
                    0x0bf0                  _DMAPWCbits = 0xbf0
                    0x0bf2                  DMARQC = 0xbf2
                    0x0bf2                  _DMARQC = 0xbf2
                    0x0bf2                  _DMARQCbits = 0xbf2
                    0x0bf4                  DMAPPS = 0xbf4
                    0x0bf4                  _DMAPPS = 0xbf4
                    0x0bf4                  _DMAPPSbits = 0xbf4
                    0x0bf6                  DMALCA = 0xbf6
                    0x0bf6                  _DMALCA = 0xbf6
                    0x0bf6                  _DMALCAbits = 0xbf6
                    0x0bf8                  DSADRL = 0xbf8
                    0x0bf8                  _DSADRL = 0xbf8
                    0x0bfa                  DSADRH = 0xbfa
                    0x0bfa                  _DSADRH = 0xbfa
                    0x0bfa                  _DSADRHbits = 0xbfa
                    0x0c00                  PTCON = 0xc00
                    0x0c00                  _PTCON = 0xc00
                    0x0c00                  _PTCONbits = 0xc00
                    0x0c02                  PTCON2 = 0xc02
                    0x0c02                  _PTCON2 = 0xc02
                    0x0c02                  _PTCON2bits = 0xc02
                    0x0c04                  PTPER = 0xc04
                    0x0c04                  _PTPER = 0xc04
                    0x0c06                  SEVTCMP = 0xc06
                    0x0c06                  _SEVTCMP = 0xc06
                    0x0c06                  _SEVTCMPbits = 0xc06
                    0x0c0a                  MDC = 0xc0a
                    0x0c0a                  _MDC = 0xc0a
                    0x0c0e                  STCON = 0xc0e
                    0x0c0e                  _STCON = 0xc0e
                    0x0c0e                  _STCONbits = 0xc0e
                    0x0c10                  STCON2 = 0xc10
                    0x0c10                  _STCON2 = 0xc10
                    0x0c10                  _STCON2bits = 0xc10
                    0x0c12                  STPER = 0xc12
                    0x0c12                  _STPER = 0xc12
                    0x0c14                  SSEVTCMP = 0xc14
                    0x0c14                  _SSEVTCMP = 0xc14
                    0x0c14                  _SSEVTCMPbits = 0xc14
                    0x0c1a                  CHOP = 0xc1a
                    0x0c1a                  _CHOP = 0xc1a
                    0x0c1a                  _CHOPbits = 0xc1a
                    0x0c20                  PWMCON1 = 0xc20
                    0x0c20                  _PWMCON1 = 0xc20
                    0x0c20                  _PWMCON1bits = 0xc20
                    0x0c22                  IOCON1 = 0xc22
                    0x0c22                  _IOCON1 = 0xc22
                    0x0c22                  _IOCON1bits = 0xc22
                    0x0c24                  FCLCON1 = 0xc24
                    0x0c24                  _FCLCON1 = 0xc24
                    0x0c24                  _FCLCON1bits = 0xc24
                    0x0c26                  PDC1 = 0xc26
                    0x0c26                  _PDC1 = 0xc26
                    0x0c28                  PHASE1 = 0xc28
                    0x0c28                  _PHASE1 = 0xc28
                    0x0c2a                  DTR1 = 0xc2a
                    0x0c2a                  _DTR1 = 0xc2a
                    0x0c2c                  ALTDTR1 = 0xc2c
                    0x0c2c                  _ALTDTR1 = 0xc2c
                    0x0c2e                  SDC1 = 0xc2e
                    0x0c2e                  _SDC1 = 0xc2e
                    0x0c30                  SPHASE1 = 0xc30
                    0x0c30                  _SPHASE1 = 0xc30
                    0x0c32                  TRIG1 = 0xc32
                    0x0c32                  _TRIG1 = 0xc32
                    0x0c32                  _TRIG1bits = 0xc32
                    0x0c34                  TRGCON1 = 0xc34
                    0x0c34                  _TRGCON1 = 0xc34
                    0x0c34                  _TRGCON1bits = 0xc34
                    0x0c38                  PWMCAP1 = 0xc38
                    0x0c38                  _PWMCAP1 = 0xc38
                    0x0c38                  _PWMCAP1bits = 0xc38
                    0x0c3a                  LEBCON1 = 0xc3a
                    0x0c3a                  _LEBCON1 = 0xc3a
                    0x0c3a                  _LEBCON1bits = 0xc3a
                    0x0c3c                  LEBDLY1 = 0xc3c
                    0x0c3c                  _LEBDLY1 = 0xc3c
                    0x0c3c                  _LEBDLY1bits = 0xc3c
                    0x0c3e                  AUXCON1 = 0xc3e
                    0x0c3e                  _AUXCON1 = 0xc3e
                    0x0c3e                  _AUXCON1bits = 0xc3e
                    0x0c40                  PWMCON2 = 0xc40
                    0x0c40                  _PWMCON2 = 0xc40
                    0x0c40                  _PWMCON2bits = 0xc40
                    0x0c42                  IOCON2 = 0xc42
                    0x0c42                  _IOCON2 = 0xc42
                    0x0c42                  _IOCON2bits = 0xc42
                    0x0c44                  FCLCON2 = 0xc44
                    0x0c44                  _FCLCON2 = 0xc44
                    0x0c44                  _FCLCON2bits = 0xc44
                    0x0c46                  PDC2 = 0xc46
                    0x0c46                  _PDC2 = 0xc46
                    0x0c48                  PHASE2 = 0xc48
                    0x0c48                  _PHASE2 = 0xc48
                    0x0c4a                  DTR2 = 0xc4a
                    0x0c4a                  _DTR2 = 0xc4a
                    0x0c4c                  ALTDTR2 = 0xc4c
                    0x0c4c                  _ALTDTR2 = 0xc4c
                    0x0c4e                  SDC2 = 0xc4e
                    0x0c4e                  _SDC2 = 0xc4e
                    0x0c50                  SPHASE2 = 0xc50
                    0x0c50                  _SPHASE2 = 0xc50
                    0x0c52                  TRIG2 = 0xc52
                    0x0c52                  _TRIG2 = 0xc52
                    0x0c52                  _TRIG2bits = 0xc52
                    0x0c54                  TRGCON2 = 0xc54
                    0x0c54                  _TRGCON2 = 0xc54
                    0x0c54                  _TRGCON2bits = 0xc54
                    0x0c58                  PWMCAP2 = 0xc58
                    0x0c58                  _PWMCAP2 = 0xc58
                    0x0c58                  _PWMCAP2bits = 0xc58
                    0x0c5a                  LEBCON2 = 0xc5a
                    0x0c5a                  _LEBCON2 = 0xc5a
                    0x0c5a                  _LEBCON2bits = 0xc5a
                    0x0c5c                  LEBDLY2 = 0xc5c
                    0x0c5c                  _LEBDLY2 = 0xc5c
                    0x0c5c                  _LEBDLY2bits = 0xc5c
                    0x0c5e                  AUXCON2 = 0xc5e
                    0x0c5e                  _AUXCON2 = 0xc5e
                    0x0c5e                  _AUXCON2bits = 0xc5e
                    0x0c60                  PWMCON3 = 0xc60
                    0x0c60                  _PWMCON3 = 0xc60
                    0x0c60                  _PWMCON3bits = 0xc60
                    0x0c62                  IOCON3 = 0xc62
                    0x0c62                  _IOCON3 = 0xc62
                    0x0c62                  _IOCON3bits = 0xc62
                    0x0c64                  FCLCON3 = 0xc64
                    0x0c64                  _FCLCON3 = 0xc64
                    0x0c64                  _FCLCON3bits = 0xc64
                    0x0c66                  PDC3 = 0xc66
                    0x0c66                  _PDC3 = 0xc66
                    0x0c68                  PHASE3 = 0xc68
                    0x0c68                  _PHASE3 = 0xc68
                    0x0c6a                  DTR3 = 0xc6a
                    0x0c6a                  _DTR3 = 0xc6a
                    0x0c6c                  ALTDTR3 = 0xc6c
                    0x0c6c                  _ALTDTR3 = 0xc6c
                    0x0c6e                  SDC3 = 0xc6e
                    0x0c6e                  _SDC3 = 0xc6e
                    0x0c70                  SPHASE3 = 0xc70
                    0x0c70                  _SPHASE3 = 0xc70
                    0x0c72                  TRIG3 = 0xc72
                    0x0c72                  _TRIG3 = 0xc72
                    0x0c72                  _TRIG3bits = 0xc72
                    0x0c74                  TRGCON3 = 0xc74
                    0x0c74                  _TRGCON3 = 0xc74
                    0x0c74                  _TRGCON3bits = 0xc74
                    0x0c78                  PWMCAP3 = 0xc78
                    0x0c78                  _PWMCAP3 = 0xc78
                    0x0c78                  _PWMCAP3bits = 0xc78
                    0x0c7a                  LEBCON3 = 0xc7a
                    0x0c7a                  _LEBCON3 = 0xc7a
                    0x0c7a                  _LEBCON3bits = 0xc7a
                    0x0c7c                  LEBDLY3 = 0xc7c
                    0x0c7c                  _LEBDLY3 = 0xc7c
                    0x0c7c                  _LEBDLY3bits = 0xc7c
                    0x0c7e                  AUXCON3 = 0xc7e
                    0x0c7e                  _AUXCON3 = 0xc7e
                    0x0c7e                  _AUXCON3bits = 0xc7e
                    0x0c80                  PWMCON4 = 0xc80
                    0x0c80                  _PWMCON4 = 0xc80
                    0x0c80                  _PWMCON4bits = 0xc80
                    0x0c82                  IOCON4 = 0xc82
                    0x0c82                  _IOCON4 = 0xc82
                    0x0c82                  _IOCON4bits = 0xc82
                    0x0c84                  FCLCON4 = 0xc84
                    0x0c84                  _FCLCON4 = 0xc84
                    0x0c84                  _FCLCON4bits = 0xc84
                    0x0c86                  PDC4 = 0xc86
                    0x0c86                  _PDC4 = 0xc86
                    0x0c88                  PHASE4 = 0xc88
                    0x0c88                  _PHASE4 = 0xc88
                    0x0c8a                  DTR4 = 0xc8a
                    0x0c8a                  _DTR4 = 0xc8a
                    0x0c8c                  ALTDTR4 = 0xc8c
                    0x0c8c                  _ALTDTR4 = 0xc8c
                    0x0c8e                  SDC4 = 0xc8e
                    0x0c8e                  _SDC4 = 0xc8e
                    0x0c90                  SPHASE4 = 0xc90
                    0x0c90                  _SPHASE4 = 0xc90
                    0x0c92                  TRIG4 = 0xc92
                    0x0c92                  _TRIG4 = 0xc92
                    0x0c92                  _TRIG4bits = 0xc92
                    0x0c94                  TRGCON4 = 0xc94
                    0x0c94                  _TRGCON4 = 0xc94
                    0x0c94                  _TRGCON4bits = 0xc94
                    0x0c98                  PWMCAP4 = 0xc98
                    0x0c98                  _PWMCAP4 = 0xc98
                    0x0c98                  _PWMCAP4bits = 0xc98
                    0x0c9a                  LEBCON4 = 0xc9a
                    0x0c9a                  _LEBCON4 = 0xc9a
                    0x0c9a                  _LEBCON4bits = 0xc9a
                    0x0c9c                  LEBDLY4 = 0xc9c
                    0x0c9c                  _LEBDLY4 = 0xc9c
                    0x0c9c                  _LEBDLY4bits = 0xc9c
                    0x0c9e                  AUXCON4 = 0xc9e
                    0x0c9e                  _AUXCON4 = 0xc9e
                    0x0c9e                  _AUXCON4bits = 0xc9e
                    0x0ca0                  PWMCON5 = 0xca0
                    0x0ca0                  _PWMCON5 = 0xca0
                    0x0ca0                  _PWMCON5bits = 0xca0
                    0x0ca2                  IOCON5 = 0xca2
                    0x0ca2                  _IOCON5 = 0xca2
                    0x0ca2                  _IOCON5bits = 0xca2
                    0x0ca4                  FCLCON5 = 0xca4
                    0x0ca4                  _FCLCON5 = 0xca4
                    0x0ca4                  _FCLCON5bits = 0xca4
                    0x0ca6                  PDC5 = 0xca6
                    0x0ca6                  _PDC5 = 0xca6
                    0x0ca8                  PHASE5 = 0xca8
                    0x0ca8                  _PHASE5 = 0xca8
                    0x0caa                  DTR5 = 0xcaa
                    0x0caa                  _DTR5 = 0xcaa
                    0x0cac                  ALTDTR5 = 0xcac
                    0x0cac                  _ALTDTR5 = 0xcac
                    0x0cae                  SDC5 = 0xcae
                    0x0cae                  _SDC5 = 0xcae
                    0x0cb0                  SPHASE5 = 0xcb0
                    0x0cb0                  _SPHASE5 = 0xcb0
                    0x0cb2                  TRIG5 = 0xcb2
                    0x0cb2                  _TRIG5 = 0xcb2
                    0x0cb2                  _TRIG5bits = 0xcb2
                    0x0cb4                  TRGCON5 = 0xcb4
                    0x0cb4                  _TRGCON5 = 0xcb4
                    0x0cb4                  _TRGCON5bits = 0xcb4
                    0x0cb8                  PWMCAP5 = 0xcb8
                    0x0cb8                  _PWMCAP5 = 0xcb8
                    0x0cb8                  _PWMCAP5bits = 0xcb8
                    0x0cba                  LEBCON5 = 0xcba
                    0x0cba                  _LEBCON5 = 0xcba
                    0x0cba                  _LEBCON5bits = 0xcba
                    0x0cbc                  LEBDLY5 = 0xcbc
                    0x0cbc                  _LEBDLY5 = 0xcbc
                    0x0cbc                  _LEBDLY5bits = 0xcbc
                    0x0cbe                  AUXCON5 = 0xcbe
                    0x0cbe                  _AUXCON5 = 0xcbe
                    0x0cbe                  _AUXCON5bits = 0xcbe
                    0x0cc0                  PWMCON6 = 0xcc0
                    0x0cc0                  _PWMCON6 = 0xcc0
                    0x0cc0                  _PWMCON6bits = 0xcc0
                    0x0cc2                  IOCON6 = 0xcc2
                    0x0cc2                  _IOCON6 = 0xcc2
                    0x0cc2                  _IOCON6bits = 0xcc2
                    0x0cc4                  FCLCON6 = 0xcc4
                    0x0cc4                  _FCLCON6 = 0xcc4
                    0x0cc4                  _FCLCON6bits = 0xcc4
                    0x0cc6                  PDC6 = 0xcc6
                    0x0cc6                  _PDC6 = 0xcc6
                    0x0cc8                  PHASE6 = 0xcc8
                    0x0cc8                  _PHASE6 = 0xcc8
                    0x0cca                  DTR6 = 0xcca
                    0x0cca                  _DTR6 = 0xcca
                    0x0ccc                  ALTDTR6 = 0xccc
                    0x0ccc                  _ALTDTR6 = 0xccc
                    0x0cce                  SDC6 = 0xcce
                    0x0cce                  _SDC6 = 0xcce
                    0x0cd0                  SPHASE6 = 0xcd0
                    0x0cd0                  _SPHASE6 = 0xcd0
                    0x0cd2                  TRIG6 = 0xcd2
                    0x0cd2                  _TRIG6 = 0xcd2
                    0x0cd2                  _TRIG6bits = 0xcd2
                    0x0cd4                  TRGCON6 = 0xcd4
                    0x0cd4                  _TRGCON6 = 0xcd4
                    0x0cd4                  _TRGCON6bits = 0xcd4
                    0x0cd8                  PWMCAP6 = 0xcd8
                    0x0cd8                  _PWMCAP6 = 0xcd8
                    0x0cd8                  _PWMCAP6bits = 0xcd8
                    0x0cda                  LEBCON6 = 0xcda
                    0x0cda                  _LEBCON6 = 0xcda
                    0x0cda                  _LEBCON6bits = 0xcda
                    0x0cdc                  LEBDLY6 = 0xcdc
                    0x0cdc                  _LEBDLY6 = 0xcdc
                    0x0cdc                  _LEBDLY6bits = 0xcdc
                    0x0cde                  AUXCON6 = 0xcde
                    0x0cde                  _AUXCON6 = 0xcde
                    0x0cde                  _AUXCON6bits = 0xcde
                    0x0e00                  TRISA = 0xe00
                    0x0e00                  _TRISA = 0xe00
                    0x0e00                  _TRISAbits = 0xe00
                    0x0e02                  PORTA = 0xe02
                    0x0e02                  _PORTA = 0xe02
                    0x0e02                  _PORTAbits = 0xe02
                    0x0e04                  LATA = 0xe04
                    0x0e04                  _LATA = 0xe04
                    0x0e04                  _LATAbits = 0xe04
                    0x0e06                  ODCA = 0xe06
                    0x0e06                  _ODCA = 0xe06
                    0x0e06                  _ODCAbits = 0xe06
                    0x0e08                  CNENA = 0xe08
                    0x0e08                  _CNENA = 0xe08
                    0x0e08                  _CNENAbits = 0xe08
                    0x0e0a                  CNPUA = 0xe0a
                    0x0e0a                  _CNPUA = 0xe0a
                    0x0e0a                  _CNPUAbits = 0xe0a
                    0x0e0c                  CNPDA = 0xe0c
                    0x0e0c                  _CNPDA = 0xe0c
                    0x0e0c                  _CNPDAbits = 0xe0c
                    0x0e0e                  ANSELA = 0xe0e
                    0x0e0e                  _ANSELA = 0xe0e
                    0x0e0e                  _ANSELAbits = 0xe0e
                    0x0e10                  TRISB = 0xe10
                    0x0e10                  _TRISB = 0xe10
                    0x0e10                  _TRISBbits = 0xe10
                    0x0e12                  PORTB = 0xe12
                    0x0e12                  _PORTB = 0xe12
                    0x0e12                  _PORTBbits = 0xe12
                    0x0e14                  LATB = 0xe14
                    0x0e14                  _LATB = 0xe14
                    0x0e14                  _LATBbits = 0xe14
                    0x0e18                  CNENB = 0xe18
                    0x0e18                  _CNENB = 0xe18
                    0x0e18                  _CNENBbits = 0xe18
                    0x0e1a                  CNPUB = 0xe1a
                    0x0e1a                  _CNPUB = 0xe1a
                    0x0e1a                  _CNPUBbits = 0xe1a
                    0x0e1c                  CNPDB = 0xe1c
                    0x0e1c                  _CNPDB = 0xe1c
                    0x0e1c                  _CNPDBbits = 0xe1c
                    0x0e1e                  ANSELB = 0xe1e
                    0x0e1e                  _ANSELB = 0xe1e
                    0x0e1e                  _ANSELBbits = 0xe1e
                    0x0e20                  TRISC = 0xe20
                    0x0e20                  _TRISC = 0xe20
                    0x0e20                  _TRISCbits = 0xe20
                    0x0e22                  PORTC = 0xe22
                    0x0e22                  _PORTC = 0xe22
                    0x0e22                  _PORTCbits = 0xe22
                    0x0e24                  LATC = 0xe24
                    0x0e24                  _LATC = 0xe24
                    0x0e24                  _LATCbits = 0xe24
                    0x0e28                  CNENC = 0xe28
                    0x0e28                  _CNENC = 0xe28
                    0x0e28                  _CNENCbits = 0xe28
                    0x0e2a                  CNPUC = 0xe2a
                    0x0e2a                  _CNPUC = 0xe2a
                    0x0e2a                  _CNPUCbits = 0xe2a
                    0x0e2c                  CNPDC = 0xe2c
                    0x0e2c                  _CNPDC = 0xe2c
                    0x0e2c                  _CNPDCbits = 0xe2c
                    0x0e2e                  ANSELC = 0xe2e
                    0x0e2e                  _ANSELC = 0xe2e
                    0x0e2e                  _ANSELCbits = 0xe2e
                    0x0e30                  TRISD = 0xe30
                    0x0e30                  _TRISD = 0xe30
                    0x0e30                  _TRISDbits = 0xe30
                    0x0e32                  PORTD = 0xe32
                    0x0e32                  _PORTD = 0xe32
                    0x0e32                  _PORTDbits = 0xe32
                    0x0e34                  LATD = 0xe34
                    0x0e34                  _LATD = 0xe34
                    0x0e34                  _LATDbits = 0xe34
                    0x0e36                  ODCD = 0xe36
                    0x0e36                  _ODCD = 0xe36
                    0x0e36                  _ODCDbits = 0xe36
                    0x0e38                  CNEND = 0xe38
                    0x0e38                  _CNEND = 0xe38
                    0x0e38                  _CNENDbits = 0xe38
                    0x0e3a                  CNPUD = 0xe3a
                    0x0e3a                  _CNPUD = 0xe3a
                    0x0e3a                  _CNPUDbits = 0xe3a
                    0x0e3c                  CNPDD = 0xe3c
                    0x0e3c                  _CNPDD = 0xe3c
                    0x0e3c                  _CNPDDbits = 0xe3c
                    0x0e3e                  ANSELD = 0xe3e
                    0x0e3e                  _ANSELD = 0xe3e
                    0x0e3e                  _ANSELDbits = 0xe3e
                    0x0e40                  TRISE = 0xe40
                    0x0e40                  _TRISE = 0xe40
                    0x0e40                  _TRISEbits = 0xe40
                    0x0e42                  PORTE = 0xe42
                    0x0e42                  _PORTE = 0xe42
                    0x0e42                  _PORTEbits = 0xe42
                    0x0e44                  LATE = 0xe44
                    0x0e44                  _LATE = 0xe44
                    0x0e44                  _LATEbits = 0xe44
                    0x0e48                  CNENE = 0xe48
                    0x0e48                  _CNENE = 0xe48
                    0x0e48                  _CNENEbits = 0xe48
                    0x0e4a                  CNPUE = 0xe4a
                    0x0e4a                  _CNPUE = 0xe4a
                    0x0e4a                  _CNPUEbits = 0xe4a
                    0x0e4c                  CNPDE = 0xe4c
                    0x0e4c                  _CNPDE = 0xe4c
                    0x0e4c                  _CNPDEbits = 0xe4c
                    0x0e4e                  ANSELE = 0xe4e
                    0x0e4e                  _ANSELE = 0xe4e
                    0x0e4e                  _ANSELEbits = 0xe4e
                    0x0e50                  TRISF = 0xe50
                    0x0e50                  _TRISF = 0xe50
                    0x0e50                  _TRISFbits = 0xe50
                    0x0e52                  PORTF = 0xe52
                    0x0e52                  _PORTF = 0xe52
                    0x0e52                  _PORTFbits = 0xe52
                    0x0e54                  LATF = 0xe54
                    0x0e54                  _LATF = 0xe54
                    0x0e54                  _LATFbits = 0xe54
                    0x0e56                  ODCF = 0xe56
                    0x0e56                  _ODCF = 0xe56
                    0x0e56                  _ODCFbits = 0xe56
                    0x0e58                  CNENF = 0xe58
                    0x0e58                  _CNENF = 0xe58
                    0x0e58                  _CNENFbits = 0xe58
                    0x0e5a                  CNPUF = 0xe5a
                    0x0e5a                  _CNPUF = 0xe5a
                    0x0e5a                  _CNPUFbits = 0xe5a
                    0x0e5c                  CNPDF = 0xe5c
                    0x0e5c                  _CNPDF = 0xe5c
                    0x0e5c                  _CNPDFbits = 0xe5c
                    0x0e60                  TRISG = 0xe60
                    0x0e60                  _TRISG = 0xe60
                    0x0e60                  _TRISGbits = 0xe60
                    0x0e62                  PORTG = 0xe62
                    0x0e62                  _PORTG = 0xe62
                    0x0e62                  _PORTGbits = 0xe62
                    0x0e64                  LATG = 0xe64
                    0x0e64                  _LATG = 0xe64
                    0x0e64                  _LATGbits = 0xe64
                    0x0e66                  ODCG = 0xe66
                    0x0e66                  _ODCG = 0xe66
                    0x0e66                  _ODCGbits = 0xe66
                    0x0e68                  CNENG = 0xe68
                    0x0e68                  _CNENG = 0xe68
                    0x0e68                  _CNENGbits = 0xe68
                    0x0e6a                  CNPUG = 0xe6a
                    0x0e6a                  _CNPUG = 0xe6a
                    0x0e6a                  _CNPUGbits = 0xe6a
                    0x0e6c                  CNPDG = 0xe6c
                    0x0e6c                  _CNPDG = 0xe6c
                    0x0e6c                  _CNPDGbits = 0xe6c
                    0x0e6e                  ANSELG = 0xe6e
                    0x0e6e                  _ANSELG = 0xe6e
                    0x0e6e                  _ANSELGbits = 0xe6e
                    0x0efe                  PADCFG1 = 0xefe
                    0x0efe                  _PADCFG1 = 0xefe
                    0x0efe                  _PADCFG1bits = 0xefe
                    0x0022                  ACCA = 0x22
                    0x0022                  _ACCA = 0x22
                    0x0028                  ACCB = 0x28
                    0x0028                  _ACCB = 0x28
                    0x0440                  CAN1 = 0x440
                    0x0440                  _CAN1 = 0x440
                    0x0540                  CAN2 = 0x540
                    0x0540                  _CAN2 = 0x540
                    0x0144                  IC1 = 0x144
                    0x0144                  _IC1 = 0x144
                    0x014c                  IC2 = 0x14c
                    0x014c                  _IC2 = 0x14c
                    0x0154                  IC3 = 0x154
                    0x0154                  _IC3 = 0x154
                    0x015c                  IC4 = 0x15c
                    0x015c                  _IC4 = 0x15c
                    0x0164                  IC5 = 0x164
                    0x0164                  _IC5 = 0x164
                    0x016c                  IC6 = 0x16c
                    0x016c                  _IC6 = 0x16c
                    0x0174                  IC7 = 0x174
                    0x0174                  _IC7 = 0x174
                    0x017c                  IC8 = 0x17c
                    0x017c                  _IC8 = 0x17c
                    0x0904                  OC1 = 0x904
                    0x0904                  _OC1 = 0x904
                    0x090e                  OC2 = 0x90e
                    0x090e                  _OC2 = 0x90e
                    0x0918                  OC3 = 0x918
                    0x0918                  _OC3 = 0x918
                    0x0922                  OC4 = 0x922
                    0x0922                  _OC4 = 0x922
                    0x092c                  OC5 = 0x92c
                    0x092c                  _OC5 = 0x92c
                    0x0936                  OC6 = 0x936
                    0x0936                  _OC6 = 0x936
                    0x0940                  OC7 = 0x940
                    0x0940                  _OC7 = 0x940
                    0x094a                  OC8 = 0x94a
                    0x094a                  _OC8 = 0x94a
                    0x0240                  SPI1 = 0x240
                    0x0240                  _SPI1 = 0x240
                    0x0260                  SPI2 = 0x260
                    0x0260                  _SPI2 = 0x260
                    0x0220                  UART1 = 0x220
                    0x0220                  _UART1 = 0x220
                    0x0230                  UART2 = 0x230
                    0x0230                  _UART2 = 0x230
START GROUP
LOAD c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a
LOAD c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a
LOAD c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a
END GROUP
OUTPUT(dist/XC16_dsPIC33EP512MU810/debug/PLCD_P01V49.debug.elf elf32-pic30)
LOAD jump_table
LOAD data_init

.debug_pubtypes
                  0x0005c0       0x45a8
 .debug_pubtypes
                  0x0005c0         0x12 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
 .debug_pubtypes
                  0x0005d2         0x12 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
 .debug_pubtypes
                  0x0005e4         0x32 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 .debug_pubtypes
                  0x000616         0xcf build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .debug_pubtypes
                  0x0006e5        0x206 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .debug_pubtypes
                  0x0008eb        0x2ba build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .debug_pubtypes
                  0x000ba5         0x8e build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 .debug_pubtypes
                  0x000c33        0x1f7 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .debug_pubtypes
                  0x000e2a        0x1a7 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .debug_pubtypes
                  0x000fd1         0x3f build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 .debug_pubtypes
                  0x001010         0x8a build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 .debug_pubtypes
                  0x00109a        0x359 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .debug_pubtypes
                  0x0013f3        0x142 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 .debug_pubtypes
                  0x001535        0x12b build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .debug_pubtypes
                  0x001660        0x315 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .debug_pubtypes
                  0x001975        0x11c build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 .debug_pubtypes
                  0x001a91        0x100 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 .debug_pubtypes
                  0x001b91        0x1e8 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .debug_pubtypes
                  0x001d79         0x8e build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .debug_pubtypes
                  0x001e07        0x224 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 .debug_pubtypes
                  0x00202b         0x9c build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .debug_pubtypes
                  0x0020c7         0x72 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 .debug_pubtypes
                  0x002139         0x9f build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .debug_pubtypes
                  0x0021d8         0x53 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 .debug_pubtypes
                  0x00222b         0x33 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 .debug_pubtypes
                  0x00225e         0x33 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 .debug_pubtypes
                  0x002291        0x1e1 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .debug_pubtypes
                  0x002472         0x33 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 .debug_pubtypes
                  0x0024a5         0x33 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 .debug_pubtypes
                  0x0024d8         0xc5 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .debug_pubtypes
                  0x00259d         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
 .debug_pubtypes
                  0x0025af         0xa9 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .debug_pubtypes
                  0x002658         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
 .debug_pubtypes
                  0x00266a        0x146 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 .debug_pubtypes
                  0x0027b0         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
 .debug_pubtypes
                  0x0027c2         0x25 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 .debug_pubtypes
                  0x0027e7         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
 .debug_pubtypes
                  0x0027f9         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
 .debug_pubtypes
                  0x00280b         0xd8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .debug_pubtypes
                  0x0028e3         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
 .debug_pubtypes
                  0x0028f5         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
 .debug_pubtypes
                  0x002907        0x166 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 .debug_pubtypes
                  0x002a6d         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
 .debug_pubtypes
                  0x002a7f         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
 .debug_pubtypes
                  0x002a91         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
 .debug_pubtypes
                  0x002aa3         0x90 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 .debug_pubtypes
                  0x002b33         0xef build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .debug_pubtypes
                  0x002c22         0x9a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .debug_pubtypes
                  0x002cbc         0xb7 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .debug_pubtypes
                  0x002d73         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
 .debug_pubtypes
                  0x002d85         0xae build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .debug_pubtypes
                  0x002e33         0xe6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .debug_pubtypes
                  0x002f19         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
 .debug_pubtypes
                  0x002f2b         0xb3 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .debug_pubtypes
                  0x002fde         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
 .debug_pubtypes
                  0x002ff0         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
 .debug_pubtypes
                  0x003002         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
 .debug_pubtypes
                  0x003014         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
 .debug_pubtypes
                  0x003026         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
 .debug_pubtypes
                  0x003038         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
 .debug_pubtypes
                  0x00304a         0xf8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .debug_pubtypes
                  0x003142         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
 .debug_pubtypes
                  0x003154         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
 .debug_pubtypes
                  0x003166         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
 .debug_pubtypes
                  0x003178         0xa7 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 .debug_pubtypes
                  0x00321f        0x14f build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .debug_pubtypes
                  0x00336e         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
 .debug_pubtypes
                  0x003380         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
 .debug_pubtypes
                  0x003392         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
 .debug_pubtypes
                  0x0033a4         0xb1 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 .debug_pubtypes
                  0x003455         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
 .debug_pubtypes
                  0x003467         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
 .debug_pubtypes
                  0x003479        0x116 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 .debug_pubtypes
                  0x00358f         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
 .debug_pubtypes
                  0x0035a1         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
 .debug_pubtypes
                  0x0035b3         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
 .debug_pubtypes
                  0x0035c5         0x12 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
 .debug_pubtypes
                  0x0035d7        0x295 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 .debug_pubtypes
                  0x00386c        0x15f build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 .debug_pubtypes
                  0x0039cb         0x6f build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 .debug_pubtypes
                  0x003a3a         0x12 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
 .debug_pubtypes
                  0x003a4c        0x17b build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 .debug_pubtypes
                  0x003bc7        0x685 build/XC16_dsPIC33EP512MU810/debug/main.o
 .debug_pubtypes
                  0x00424c         0x96 build/XC16_dsPIC33EP512MU810/debug/system.o
 .debug_pubtypes
                  0x0042e2         0x35 build/XC16_dsPIC33EP512MU810/debug/traps.o
 .debug_pubtypes
                  0x004317        0x1ed build/XC16_dsPIC33EP512MU810/debug/user.o
 .debug_pubtypes
                  0x004504        0x146 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .debug_pubtypes
                  0x00464a         0x90 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .debug_pubtypes
                  0x0046da         0x56 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 .debug_pubtypes
                  0x004730         0x85 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 .debug_pubtypes
                  0x0047b5         0x65 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 .debug_pubtypes
                  0x00481a        0x146 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 .debug_pubtypes
                  0x004960         0xca build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .debug_pubtypes
                  0x004a2a         0x60 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 .debug_pubtypes
                  0x004a8a         0xde build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

__c30_signature
                  0x004b68        0x4c8
 __c30_signature
                  0x004b68          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_handler_par.o
 __c30_signature
                  0x004b6e          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/par/abcc_par_drv.o
 __c30_signature
                  0x004b74          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
 __c30_signature
                  0x004b7a          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 __c30_signature
                  0x004b80          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 __c30_signature
                  0x004b86          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 __c30_signature
                  0x004b8c          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
 __c30_signature
                  0x004b92          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 __c30_signature
                  0x004b98          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 __c30_signature
                  0x004b9e          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
 __c30_signature
                  0x004ba4          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
 __c30_signature
                  0x004baa          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 __c30_signature
                  0x004bb0          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
 __c30_signature
                  0x004bb6          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 __c30_signature
                  0x004bbc          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 __c30_signature
                  0x004bc2          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
 __c30_signature
                  0x004bc8          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
 __c30_signature
                  0x004bce          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 __c30_signature
                  0x004bd4          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 __c30_signature
                  0x004bda          0x6 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
 __c30_signature
                  0x004be0          0x6 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 __c30_signature
                  0x004be6          0x6 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
 __c30_signature
                  0x004bec          0x6 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 __c30_signature
                  0x004bf2          0x6 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
 __c30_signature
                  0x004bf8          0x6 build/XC16_dsPIC33EP512MU810/debug/Regul.o
 __c30_signature
                  0x004bfe          0x6 build/XC16_dsPIC33EP512MU810/debug/Pesage.o
 __c30_signature
                  0x004c04          0x6 build/XC16_dsPIC33EP512MU810/debug/Process.o
 __c30_signature
                  0x004c0a          0x6 build/XC16_dsPIC33EP512MU810/debug/BdC.o
 __c30_signature
                  0x004c10          0x6 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
 __c30_signature
                  0x004c16          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 __c30_signature
                  0x004c1c          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARCFOUR.o
 __c30_signature
                  0x004c22          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 __c30_signature
                  0x004c28          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/AutoIP.o
 __c30_signature
                  0x004c2e          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
 __c30_signature
                  0x004c34          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BigInt.o
 __c30_signature
                  0x004c3a          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
 __c30_signature
                  0x004c40          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCP.o
 __c30_signature
                  0x004c46          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DHCPs.o
 __c30_signature
                  0x004c4c          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 __c30_signature
                  0x004c52          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNSs.o
 __c30_signature
                  0x004c58          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DynDNS.o
 __c30_signature
                  0x004c5e          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
 __c30_signature
                  0x004c64          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FileSystem.o
 __c30_signature
                  0x004c6a          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/FTP.o
 __c30_signature
                  0x004c70          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Hashes.o
 __c30_signature
                  0x004c76          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
 __c30_signature
                  0x004c7c          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 __c30_signature
                  0x004c82          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 __c30_signature
                  0x004c88          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 __c30_signature
                  0x004c8e          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/LCDBlocking.o
 __c30_signature
                  0x004c94          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 __c30_signature
                  0x004c9a          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 __c30_signature
                  0x004ca0          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Random.o
 __c30_signature
                  0x004ca6          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 __c30_signature
                  0x004cac          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/RSA.o
 __c30_signature
                  0x004cb2          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SMTP.o
 __c30_signature
                  0x004cb8          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMP.o
 __c30_signature
                  0x004cbe          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3.o
 __c30_signature
                  0x004cc4          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNMPv3USM.o
 __c30_signature
                  0x004cca          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SNTP.o
 __c30_signature
                  0x004cd0          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 __c30_signature
                  0x004cd6          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIFlash.o
 __c30_signature
                  0x004cdc          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIRAM.o
 __c30_signature
                  0x004ce2          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SSL.o
 __c30_signature
                  0x004ce8          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
 __c30_signature
                  0x004cee          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 __c30_signature
                  0x004cf4          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCPPerformanceTest.o
 __c30_signature
                  0x004cfa          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Telnet.o
 __c30_signature
                  0x004d00          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TFTPc.o
 __c30_signature
                  0x004d06          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
 __c30_signature
                  0x004d0c          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART.o
 __c30_signature
                  0x004d12          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UART2TCPBridge.o
 __c30_signature
                  0x004d18          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
 __c30_signature
                  0x004d1e          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDPPerformanceTest.o
 __c30_signature
                  0x004d24          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfHelper.o
 __c30_signature
                  0x004d2a          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfLinkLocal.o
 __c30_signature
                  0x004d30          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ZeroconfMulticastDNS.o
 __c30_signature
                  0x004d36          0x6 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
 __c30_signature
                  0x004d3c          0x6 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
 __c30_signature
                  0x004d42          0x6 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
 __c30_signature
                  0x004d48          0x6 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o
 __c30_signature
                  0x004d4e          0x6 build/XC16_dsPIC33EP512MU810/debug/interrupts.o
 __c30_signature
                  0x004d54          0x6 build/XC16_dsPIC33EP512MU810/debug/main.o
 __c30_signature
                  0x004d5a          0x6 build/XC16_dsPIC33EP512MU810/debug/system.o
 __c30_signature
                  0x004d60          0x6 build/XC16_dsPIC33EP512MU810/debug/traps.o
 __c30_signature
                  0x004d66          0x6 build/XC16_dsPIC33EP512MU810/debug/user.o
 __c30_signature
                  0x004d6c          0x6 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 __c30_signature
                  0x004d72          0x6 build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 __c30_signature
                  0x004d78          0x6 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
 __c30_signature
                  0x004d7e          0x6 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
 __c30_signature
                  0x004d84          0x6 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
 __c30_signature
                  0x004d8a          0x6 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
 __c30_signature
                  0x004d90          0x6 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 __c30_signature
                  0x004d96          0x6 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
 __c30_signature
                  0x004d9c          0x6 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o
 __c30_signature
                  0x004da2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI1.o)
 __c30_signature
                  0x004da8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseSPI3.o)
 __c30_signature
                  0x004dae          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI1.o)
 __c30_signature
                  0x004db4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdySPI3.o)
 __c30_signature
                  0x004dba          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI1.o)
 __c30_signature
                  0x004dc0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenSPI3.o)
 __c30_signature
                  0x004dc6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI1.o)
 __c30_signature
                  0x004dcc          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadSPI3.o)
 __c30_signature
                  0x004dd2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI1.o)
 __c30_signature
                  0x004dd8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(WriteSPI3.o)
 __c30_signature
                  0x004dde          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART2.o)
 __c30_signature
                  0x004de4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART3.o)
 __c30_signature
                  0x004dea          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(BusyUART4.o)
 __c30_signature
                  0x004df0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART1.o)
 __c30_signature
                  0x004df6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART2.o)
 __c30_signature
                  0x004dfc          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART3.o)
 __c30_signature
                  0x004e02          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(CloseUART4.o)
 __c30_signature
                  0x004e08          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART1.o)
 __c30_signature
                  0x004e0e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART2.o)
 __c30_signature
                  0x004e14          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART3.o)
 __c30_signature
                  0x004e1a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ConfigIntUART4.o)
 __c30_signature
                  0x004e20          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART1.o)
 __c30_signature
                  0x004e26          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART2.o)
 __c30_signature
                  0x004e2c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART3.o)
 __c30_signature
                  0x004e32          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(DataRdyUART4.o)
 __c30_signature
                  0x004e38          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART1.o)
 __c30_signature
                  0x004e3e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART2.o)
 __c30_signature
                  0x004e44          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART3.o)
 __c30_signature
                  0x004e4a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(OpenUART4.o)
 __c30_signature
                  0x004e50          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART1.o)
 __c30_signature
                  0x004e56          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART2.o)
 __c30_signature
                  0x004e5c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART3.o)
 __c30_signature
                  0x004e62          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(putsUART4.o)
 __c30_signature
                  0x004e68          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART1.o)
 __c30_signature
                  0x004e6e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART2.o)
 __c30_signature
                  0x004e74          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART3.o)
 __c30_signature
                  0x004e7a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib/dsPIC33E\libp33EP512MU810-elf.a(ReadUART4.o)
 __c30_signature
                  0x004e80          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(crt0_extendedep.o)
 __c30_signature
                  0x004e86          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(data_init_extendedep.o)
 __c30_signature
                  0x004e8c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(addsf3.epeo)
 __c30_signature
                  0x004e92          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsf3.epeo)
 __c30_signature
                  0x004e98          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divsi3.epeo)
 __c30_signature
                  0x004e9e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(feqltle.epeo)
 __c30_signature
                  0x004ea4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fgtge.epeo)
 __c30_signature
                  0x004eaa          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixsfsi.epeo)
 __c30_signature
                  0x004eb0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunssfsi.epeo)
 __c30_signature
                  0x004eb6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatsisf.epeo)
 __c30_signature
                  0x004ebc          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsisf.epeo)
 __c30_signature
                  0x004ec2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fpack.epeo)
 __c30_signature
                  0x004ec8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack.epeo)
 __c30_signature
                  0x004ece          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(funpack2.epeo)
 __c30_signature
                  0x004ed4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(futil.epeo)
 __c30_signature
                  0x004eda          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsf3.epeo)
 __c30_signature
                  0x004ee0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(udivsi3.epeo)
 __c30_signature
                  0x004ee6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umodsi3.epeo)
 __c30_signature
                  0x004eec          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fcompare.epeo)
 __c30_signature
                  0x004ef2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatdisf.epeo)
 __c30_signature
                  0x004ef8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundisf.epeo)
 __c30_signature
                  0x004efe          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atof.epeo)
 __c30_signature
                  0x004f04          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atoi.epeo)
 __c30_signature
                  0x004f0a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(atol.epeo)
 __c30_signature
                  0x004f10          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(errno.epeo)
 __c30_signature
                  0x004f16          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(ltoa.epeo)
 __c30_signature
                  0x004f1c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcmp.epeo)
 __c30_signature
                  0x004f22          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memcpy.epeo)
 __c30_signature
                  0x004f28          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(memset.epeo)
 __c30_signature
                  0x004f2e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)
 __c30_signature
                  0x004f34          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf.epeo)
 __c30_signature
                  0x004f3a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcmp.epeo)
 __c30_signature
                  0x004f40          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcpy.epeo)
 __c30_signature
                  0x004f46          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strlen.epeo)
 __c30_signature
                  0x004f4c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strncpy.epeo)
 __c30_signature
                  0x004f52          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo)
 __c30_signature
                  0x004f58          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(putchar.epeo)
 __c30_signature
                  0x004f5e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
 __c30_signature
                  0x004f64          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(sprintf_cdfFnopsuxX.EPeo)
 __c30_signature
                  0x004f6a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
 __c30_signature
                  0x004f70          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(printf_cdnopsuxX.EPeo)
 __c30_signature
                  0x004f76          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)
 __c30_signature
                  0x004f7c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(fputc.epeo)
 __c30_signature
                  0x004f82          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(powers.epeo)
 __c30_signature
                  0x004f88          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strcspn.epeo)
 __c30_signature
                  0x004f8e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strspn.epeo)
 __c30_signature
                  0x004f94          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strchr.epelo)
 __c30_signature
                  0x004f9a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(flsbuf.epeo)
 __c30_signature
                  0x004fa0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libpic30-elf.a(writeep.eo)
 __c30_signature
                  0x004fa6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(adddf3.epeo)
 __c30_signature
                  0x004fac          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(deqltle.epeo)
 __c30_signature
                  0x004fb2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dgtge.epeo)
 __c30_signature
                  0x004fb8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divdf3.epeo)
 __c30_signature
                  0x004fbe          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dne.epeo)
 __c30_signature
                  0x004fc4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpack.epeo)
 __c30_signature
                  0x004fca          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack2.epeo)
 __c30_signature
                  0x004fd0          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(extendsfdf.epeo)
 __c30_signature
                  0x004fd6          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfdi.epeo)
 __c30_signature
                  0x004fdc          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(fixunsdfsi.epeo)
 __c30_signature
                  0x004fe2          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatundidf.epeo)
 __c30_signature
                  0x004fe8          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(floatunsidf.epeo)
 __c30_signature
                  0x004fee          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(frexp.epeo)
 __c30_signature
                  0x004ff4          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldf3.epeo)
 __c30_signature
                  0x004ffa          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(subdf3.epeo)
 __c30_signature
                  0x005000          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(mulsi3.epeo)
 __c30_signature
                  0x005006          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(divmoddi3.epeo)
 __c30_signature
                  0x00500c          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(muldi3.epeo)
 __c30_signature
                  0x005012          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dcompare.epeo)
 __c30_signature
                  0x005018          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dpropagateNaN.epeo)
 __c30_signature
                  0x00501e          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dtype.epeo)
 __c30_signature
                  0x005024          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(dunpack.epeo)
 __c30_signature
                  0x00502a          0x6 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libm-elf.a(umuldi3.epeo)

_0478984056823da3
                    0xdc00        0x210
 _0478984056823da3
                    0xdc00        0x210 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
                    0xdc00                  _BufferA

_04789A2056823da3
                    0xd800        0x210
 _04789A2056823da3
                    0xd800        0x210 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
                    0xd800                  _BufferB

_047D69C056823d8b
                    0xdf00         0x80
 _047D69C056823d8b
                    0xdf00         0x80 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
                    0xdf00                  _ecanRxMsgBuffer

_047D678056823d8b
                    0xdb00          0xe
 _047D678056823d8b
                    0xdb00          0xe build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
                    0xdb00                  _ecanTxMsgBuffer

.bss                0x1050       0x208e
 .bss               0x1050        0x906 build/XC16_dsPIC33EP512MU810/debug/Process.o
                    0x1050                  _PAR
                    0x1452                  _EXP
                    0x18d8                  _sorTOR
                    0x18e2                  _entTOR
                    0x18ec                  _Cav_USR1
                    0x18ee                  _Cav_CLR
                    0x18f0                  _T100
                    0x192c                  _T10
                    0x1940                  _AD7190_PoidsPret
                    0x1942                  _Compteur
                    0x1944                  _NbTopTotal
                    0x1948                  _CompteurTot
                    0x194c                  _entreeTorVitesseMem
 .bss               0x1956        0x820 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
                    0x1956                  _U1Baudvalue
                    0x1958                  _U2Baudvalue
                    0x195a                  _U3Baudvalue
                    0x195c                  _U4Baudvalue
                    0x195e                  _U1MODEvalue
                    0x1960                  _U1STAvalue
                    0x1962                  _U2MODEvalue
                    0x1964                  _U2STAvalue
                    0x1966                  _U3MODEvalue
                    0x1968                  _U3STAvalue
                    0x196a                  _U4MODEvalue
                    0x196c                  _U4STAvalue
                    0x196e                  _TrameU1
                    0x1b70                  _TrameU2
                    0x1d72                  _TrameU3
                    0x1f74                  _TrameU4
 .bss               0x2176        0x48e build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .bss               0x2604        0x46e build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
                    0x2606                  _link_bPool
 .bss               0x2a72        0x418 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
                    0x2a72                  _MODBUS_COMMAND
                    0x2a7e                  _WriteByteReverse
                    0x2a80                  _MODBUS_RX
                    0x2c80                  _MODBUS_TX
                    0x2e80                  _COIL
                    0x2e82                  _COIL_REG
 .bss               0x2e8a        0x142 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
 .bss               0x2fcc        0x112 build/XC16_dsPIC33EP512MU810/debug/user.o
                    0x2fcc                  _USB_In_Buffer
                    0x300c                  _USB_Mess_head
                    0x300e                  _USB_Mess
                    0x30da                  _USB_list_count

.data._powers_      0x30de         0xb0
 .data._powers_
                    0x30de         0xb0 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(powers.epeo)
                    0x30de                  __powers_

.data._npowers_
                    0x318e         0xb0
 .data._npowers_
                    0x318e         0xb0 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(powers.epeo)
                    0x318e                  __npowers_

.bss                0x323e         0xac
 .bss               0x323e         0xac build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
                    0x323e                  _cdc_data_tx
                    0x327e                  _cdc_data_rx
                    0x32be                  _line_coding
                    0x32c6                  _cdc_notice
                    0x32d0                  _cdc_rx_len
                    0x32d1                  _cdc_trf_state
                    0x32d2                  _pCDCSrc
                    0x32d4                  _pCDCDst
                    0x32d6                  _cdc_tx_len
                    0x32d7                  _cdc_mem_type
                    0x32d8                  _CDCDataOutHandle
                    0x32da                  _CDCDataInHandle
                    0x32dc                  _control_signal_bitmap
                    0x32de                  _BaudRateGen
                    0x32e2                  _dummy_encapsulated_cmd_response

.data.dpowers       0x32ea        0x140
 .data.dpowers      0x32ea         0xa0 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)
 .data.dpowers      0x338a         0xa0 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)

_04CAD60056823d9e
                    0x3600         0x60
 _04CAD60056823d9e
                    0x3600         0x60 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
                    0x3600                  _BDT

.bss                0x342a         0xfc
 .bss               0x342a         0xfc build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
                    0x342a                  _UDPSocketInfo
                    0x351a                  _activeUDPSocket
                    0x351c                  _UDPTxCount
                    0x351e                  _UDPRxCount

.bss                0x3660         0xe6
 .bss               0x3660         0xe6 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
                    0x3660                  _AD_asDefaultMap
                    0x3662                  _AD_asADIEntryList

.bss                0x3526         0x94
 .bss               0x3526         0x94 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o

.bss                0x3746         0x8c
 .bss               0x3746         0x8c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
                    0x3746                  _curHTTP
                    0x37c8                  _httpStubs
                    0x37d0                  _curHTTPID

.data               0x37d2         0x70
 .data              0x37d2         0x70 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o

.bss                0x3842         0x6c
 .bss               0x3842         0x6c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o

.data               0x38ae         0x66
 .data              0x38ae         0x66 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
                    0x38ae                  _ReadByteReverse
                    0x38af                  _InputByteReverse
                    0x38b0                  _HOLDING_REG
                    0x38e2                  _INPUT_REG

.bss                0x3914         0x9a
 .bss               0x3914         0x50 build/XC16_dsPIC33EP512MU810/debug/main.o
                    0x3914                  _fResetABCC
                    0x3916                  _ABCCPowerState
                    0x3918                  _address
                    0x391c                  _AppConfig
 .bss               0x3964         0x4a build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
                    0x3964                  _USBDeviceState
                    0x3966                  _USBActiveConfiguration
                    0x3967                  _USBAlternateInterface
                    0x396a                  _pBDTEntryEP0OutCurrent
                    0x396c                  _pBDTEntryEP0OutNext
                    0x396e                  _pBDTEntryOut
                    0x3974                  _pBDTEntryIn
                    0x397a                  _shortPacketStatus
                    0x397b                  _controlTransferState
                    0x397c                  _inPipes
                    0x3982                  _outPipes
                    0x398a                  _pDst
                    0x398c                  _RemoteWakeup
                    0x398d                  _USBBusIsSuspended
                    0x398e                  _USTATcopy
                    0x398f                  _endpoint_number
                    0x3990                  _BothEP0OutUOWNsSet
                    0x3991                  _ep_data_in
                    0x3994                  _ep_data_out
                    0x3997                  _USBStatusStageTimeoutCounter
                    0x3998                  _USBDeferStatusStagePacket
                    0x3999                  _USBStatusStageEnabledFlag1
                    0x399a                  _USBStatusStageEnabledFlag2
                    0x399b                  _USBDeferINDataStagePackets
                    0x399c                  _USBDeferOUTDataStagePackets
                    0x399d                  _SetupPkt
                    0x39a5                  _CtrlTrfData

.data               0x35ba         0x2a
 .data              0x35ba         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt_cdfFnopsuxX.EPeo)

.data               0x39ae         0x2a
 .data              0x39ae         0x2a c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(doprnt.epeo)

.bss                0x39d8         0x24
 .bss               0x39d8         0x24 build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o

.data._iob          0x39fc         0x24
 .data._iob         0x39fc         0x24 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                    0x39fc                  __iob

.bss                0x35e4         0x18
 .bss               0x35e4         0x18 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o

.bss                0x3a20         0x68
 .bss               0x3a20         0x16 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
 .bss               0x3a36         0x16 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
 .bss               0x3a4c         0x16 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
 .bss               0x3a62         0x14 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
 .bss               0x3a76         0x12 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o

.data               0x3a88         0x74
 .data              0x3a88         0x74 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o

.bss                0x3afc         0x90
 .bss               0x3afc         0x3e build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
                    0x3afc                  _ABCC_RunDriver
                    0x3afe                  _ABCC_ISR
                    0x3b00                  _pnABCC_DrvInit
                    0x3b02                  _pnABCC_DrvISR
                    0x3b04                  _pnABCC_DrvRunDriverTx
                    0x3b06                  _pnABCC_DrvRunDriverRx
                    0x3b08                  _pnABCC_DrvWriteMessage
                    0x3b0a                  _pnABCC_DrvWriteProcessData
                    0x3b0c                  _pnABCC_DrvISReadyForWrPd
                    0x3b0e                  _pnABCC_DrvISReadyForWriteMessage
                    0x3b10                  _pnABCC_DrvISReadyForCmd
                    0x3b12                  _pnABCC_DrvSetNbrOfCmds
                    0x3b14                  _pnABCC_DrvSetAppStatus
                    0x3b16                  _pnABCC_DrvSetPdSize
                    0x3b18                  _pnABCC_DrvSetMsgReceiverBuffer
                    0x3b1a                  _pnABCC_DrvSetIntMask
                    0x3b1c                  _pnABCC_DrvGetWrPdBuffer
                    0x3b1e                  _pnABCC_DrvGetModCap
                    0x3b20                  _pnABCC_DrvGetLedStatus
                    0x3b22                  _pnABCC_DrvGetIntStatus
                    0x3b24                  _pnABCC_DrvGetAnybusState
                    0x3b26                  _pnABCC_DrvReadProcessData
                    0x3b28                  _pnABCC_DrvReadMessage
                    0x3b2a                  _pnABCC_DrvIsSupervised
                    0x3b2c                  _pnABCC_DrvGetAnbStatus
 .bss               0x3b3a         0x26 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
                    0x3b3a                  _ADI_DebitInstan
                    0x3b3e                  _ADI_PoidsInstan
                    0x3b42                  _ADI_PoidsMetre
                    0x3b46                  _ADI_Vitesse
                    0x3b4a                  _ADI_TotalPartiel
                    0x3b4e                  _ADI_TotalGlobal
                    0x3b52                  _ADI_Tare
                    0x3b56                  _ADI_EtatBascule
                    0x3b5a                  _ADI_CmdsBascule
                    0x3b5e                  _ADI_DigitalInput
                    0x3b5f                  _ADI_DigitalOutput
 .bss               0x3b60         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .bss               0x3b78         0x14 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o

.data               0x3b8c         0x10
 .data              0x3b8c         0x10 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o

.bss                0x3b9c         0x28
 .bss               0x3b9c          0xe build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
                    0x3b9e                  _remoteNode
 .bss               0x3baa          0xa build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
                    0x3baa                  _receivedECANmsg
                    0x3bac                  _transmitNextECANmsg
                    0x3bae                  _sentPacketECANMSG
                    0x3bb0                  _rxECANIndex
                    0x3bb2                  _txECANBufferIndex
 .bss               0x3bb4          0x8 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
                    0x3bb4                  _SPI3CON1Value
                    0x3bb6                  _SPI3CON2Value
                    0x3bb8                  _SPI3STATValue
 .bss               0x3bbc          0x8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o

.data               0x3bc4          0x6
 .data              0x3bc4          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
                    0x3bc4                  _app_aacLanguages
                    0x3bc6                  _app_sInstance

.bss                0x3bca          0xc
 .bss               0x3bca          0x6 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
                    0x3bca                  _us_bSwitch1
                    0x3bcb                  _us_bSwitch2
                    0x3bcc                  _us_fSwitch1Set
                    0x3bcd                  _us_fSwitch2Set
 .bss               0x3bd0          0x6 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o

_04E28D2056823d9b
                    0x3bd6          0x6
 _04E28D2056823d9b
                    0x3bd6          0x6 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o

.bss                0x3bdc          0x6
 .bss               0x3bdc          0x6 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
                    0x3bdc                  _SPICON1Value
                    0x3bde                  _SPICON2Value
                    0x3be0                  _SPISTATValue

.bss                0x35fc          0x4
 .bss               0x35fc          0x4 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o

.bss                0x3be2          0x4
 .bss               0x3be2          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o

.data               0x3be6          0x8
 .data              0x3be6          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
 .data              0x3bea          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o

.bss                0x3bee          0xc
 .bss               0x3bee          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
 .bss               0x3bf2          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
 .bss               0x3bf6          0x4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o

.data               0x3bfa          0x4
 .data              0x3bfa          0x4 build/XC16_dsPIC33EP512MU810/debug/main.o
                    0x3bfa                  _ABCC_StateMachineEnabled
                    0x3bfc                  ___C30_UART

.bss                0x3bfe          0x8
 .bss               0x3bfe          0x4 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
 .bss               0x3c02          0x4 build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
                    0x3c02                  _Nb_Octets_Log
                    0x3c04                  _Address_Log_L
                    0x3c05                  _Address_Log_B

.bss.randx          0x3c06          0x4
 .bss.randx         0x3c06          0x4 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)

.bss                0x3c0a          0x2
 .bss               0x3c0a          0x2 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_debug_err.o
                    0x3c0a                  _ErrorReporter

.data               0x3c0c          0x8
 .data              0x3c0c          0x2 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
                    0x3c0c                  _dpv_sInstance
 .data              0x3c0e          0x2 build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
                    0x3c0e                  _rxECANBufferIndex
 .data              0x3c10          0x2 build/XC16_dsPIC33EP512MU810/debug/Process.o
                    0x3c10                  _Demarrage1er
 .data              0x3c12          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o

.pbss               0x3c14          0x2
 .pbss              0x3c14          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o

.data               0x3c16          0x4
 .data              0x3c16          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
 .data              0x3c18          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o

.pbss               0x3c1a          0x2
 .pbss              0x3c1a          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o

.data               0x3c1c          0x2
 .data              0x3c1c          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o

.pbss               0x3c1e          0x2
 .pbss              0x3c1e          0x2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o

.bss                0x3c20          0x4
 .bss               0x3c20          0x2 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
                    0x3c20                  _DmaBufferSwitch
 .bss               0x3c22          0x2 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o

.bss.errno          0x3c24          0x2
 .bss.errno         0x3c24          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(errno.epeo)
                    0x3c24                  _errno

.bss.randf          0x3c26          0x2
 .bss.randf         0x3c26          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(rand.epeo)

.bss.sp.1310        0x3c28          0x2
 .bss.sp.1310       0x3c28          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(strtok.epeo)

.data._Files        0x3c2a          0x2
 .data._Files       0x3c2a          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                    0x3c2a                  __Files

.bss._outdone       0x3c2c          0x2
 .bss._outdone      0x3c2c          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                    0x3c2c                  __outdone

.bss._sibuf         0x3c2e          0x2
 .bss._sibuf        0x3c2e          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                    0x3c2e                  __sibuf

.bss._sobuf         0x3c30          0x2
 .bss._sobuf        0x3c30          0x2 c:/program files (x86)/microchip/xc16/v1.24/bin/bin/../../lib\libc-elf.a(_iob.epeo)
                    0x3c30                  __sobuf

.config_APLK      0xf80010          0x2
 .config_APLK     0xf80010          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_JTAGEN    0xf8000e          0x2
 .config_JTAGEN
                  0xf8000e          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_ALTI2C2
                  0xf8000c          0x2
 .config_ALTI2C2
                  0xf8000c          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_FWDTEN    0xf8000a          0x2
 .config_FWDTEN
                  0xf8000a          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_FCKSM     0xf80008          0x2
 .config_FCKSM    0xf80008          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_IESO      0xf80006          0x2
 .config_IESO     0xf80006          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.config_GSSK      0xf80004          0x2
 .config_GSSK     0xf80004          0x2 build/XC16_dsPIC33EP512MU810/debug/configuration_bits.o

.const              0xc0a4       0x16a6 load address 0x0040a4  
 .const             0xc0a4        0x4c0 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
 .const             0xc564        0x2aa build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
 .const             0xc80e        0x268 build/XC16_dsPIC33EP512MU810/debug/user.o
                    0xc80e                  _DELIMITER
                    0xc812                  _DELIMITER_NULL
 .const             0xca76        0x264 build/XC16_dsPIC33EP512MU810/debug/Process.o
 .const             0xccda        0x18c build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
 .const             0xce66        0x164 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
 .const             0xcfca        0x158 build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
 .const             0xd122        0x14a build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
                    0xd1e5                  _HTML_UP_ARROW
                    0xd1e8                  _HTML_DOWN_ARROW
 .const             0xd26c        0x114 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
 .const             0xd380         0xe6 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
 .const             0xd466         0xa0 build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
 .const             0xd506         0x92 build/XC16_dsPIC33EP512MU810/debug/usb_descriptors.o
                    0xd506                  _device_dsc
                    0xd518                  _configDescriptor1
                    0xd55c                  _sd000
                    0xd560                  _sd001
                    0xd578                  _sd002
                    0xd590                  _USB_CD_Ptr
                    0xd592                  _USB_SD_Ptr
 .const             0xd598         0x50 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
                    0xd598                  _abBitReverseTable16
                    0xd5a8                  _crc_table32
 .const             0xd5e8         0x34 build/XC16_dsPIC33EP512MU810/debug/main.o
 .const             0xd61c         0x2e build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
 .const             0xd64a         0x24 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
 .const             0xd66e         0x24 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
                    0xd66e                  _TCPSocketInitializer
 .const             0xd692         0x1c build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
                    0xd6a6                  _app_sObject
 .const             0xd6ae         0x1c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
 .const             0xd6ca         0x1a build/XC16_dsPIC33EP512MU810/debug/AD7190.o
 .const             0xd6e4         0x18 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
                    0xd6f4                  _dpv1_sObject
 .const             0xd6fc         0x12 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
 .const             0xd70e         0x12 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o
 .const             0xd720         0x10 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
 .const             0xd730          0xe build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
 .const             0xd73e          0x8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
 .const             0xd746          0x4 build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
                    0xd746                  _MPFS_Start

.text             0x00574a       0x63f0
 .text            0x00574a       0x63f0 build/XC16_dsPIC33EP512MU810/debug/ModbusUartServer.o
                  0x00574a                  _ModbusUartServer
                  0x0057f2                  _ProcessMessageRecu
                  0x00589a                  _LectureMots
                  0x0084ca                  _LectureModbus
                  0x008580                  _envoieLongPF
                  0x0085e0                  _envoieLongPf
                  0x00860c                  _envoieReelPF
                  0x0086b8                  _envoieReelPf
                  0x00876a                  _EcritureMots
                  0x00aa38                  _AffectationIO
                  0x00aa76                  _ModifParamMetro
                  0x00b6b0                  _LectureLong
                  0x00b792                  _LectureReel
                  0x00b8bc                  _ValidationCodeMetrologie
                  0x00b9d8                  _ModbusErreur
                  0x00ba06                  _Random
                  0x00ba36                  _ModifieVitesseComm

MPFSData          0x00bb3a       0x51ea
 MPFSData         0x00bb3a       0x51ea build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
                  0x00bb3e                  BEGIN_MPFS

.text             0x010d24      0x13c7c
 .text            0x010d24       0x2e16 build/XC16_dsPIC33EP512MU810/debug/Process.o
                  0x010d24                  _EcrFRAM_Param
                  0x010d6c                  _EcrFRAM
                  0x010db4                  _LecFRAM_Param
                  0x010e18                  _LecFRAM
                  0x010e60                  _InitParams
                  0x01131c                  _gestion_profibus
                  0x011548                  _process_plcd
                  0x0119a0                  _gestion_defauts_BI
                  0x011c38                  _gestion_cycle_BI
                  0x011f42                  _ImpressionTotalisateur
                  0x0122f0                  _ValEntTOR
                  0x012328                  _gestion_vitesse
                  0x0125ba                  _EnvoieSerie1
                  0x0125fe                  _EnvoieSerie
                  0x01270e                  _gestion_totalisateurs
                  0x012b26                  _verif_totaux
                  0x012d9c                  _etatSortieTOR
                  0x012dd2                  _forcageSortiesTOR
                  0x012f20                  _sortiesTOR
                  0x012f70                  _gestion_poids
                  0x013104                  _gestion_debit
                  0x013224                  _envoyer_reel
                  0x013302                  _moyenne_glissante_debit
                  0x013326                  _moyenne_glissante_poids
                  0x013588                  _conversion_poids
                  0x01360e                  _lecture_entrees_TOR
                  0x0136ea                  _EcritSortieAna
 .text            0x013b3a       0x249c build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/TCP.o
                  0x013c02                  _TCPInit
                  0x013cd2                  _TCPOpen
                  0x013e2c                  _TCPWasReset
                  0x013e5a                  _TCPIsConnected
                  0x013e7e                  _TCPDisconnect
                  0x013f1e                  _TCPClose
                  0x013f3e                  _TCPGetRemoteInfo
                  0x013f68                  _TCPFlush
                  0x013f8e                  _TCPIsPutReady
                  0x013fdc                  _TCPPut
                  0x014082                  _TCPPutArray
                  0x014168                  _TCPPutString
                  0x01418c                  _TCPGetTxFIFOFull
                  0x0141b8                  _TCPDiscard
                  0x0141d8                  _TCPIsGetReady
                  0x014210                  _TCPGet
                  0x01428a                  _TCPGetArray
                  0x014356                  _TCPGetRxFIFOFree
                  0x014380                  _TCPPeekArray
                  0x01442a                  _TCPPeek
                  0x014442                  _TCPFindArrayEx
                  0x0146b2                  _TCPFindEx
                  0x0146d6                  _TCPTick
                  0x014bc6                  _TCPProcess
                  0x015dd4                  _TCPAdjustFIFOSize
 .text            0x015fd6       0x1dd8 build/XC16_dsPIC33EP512MU810/debug/B40/ad_obj.o
                  0x015fd6                  _AD_Init
                  0x01616c                  _AD_GetAdiIndex
                  0x0161a2                  _AD_GetAdiInstEntry
                  0x0161c8                  _AD_ProcObjectRequest
                  0x017168                  _AD_GetAdiValue
                  0x017308                  _AD_SetAdiValue
                  0x017882                  _AD_UpdatePdReadData
                  0x0178d4                  _AD_UpdatePdWriteData
                  0x017936                  _AD_NewWrPd
                  0x017940                  _AD_AdiMappingReq
                  0x017d86                  _AD_RemapDone
 .text            0x017dae       0x1a80 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/HTTP2.o
                  0x017dae                  _HTTPPrint
                  0x017ffc                  _HTTPPrint_
                  0x01801a                  _HTTPInit
                  0x0180a8                  _HTTPServer
                  0x0193d6                  _HTTPURLDecode
                  0x0194aa                  _HTTPGetArg
                  0x019500                  _HTTPReadPostName
                  0x01952c                  _HTTPReadPostValue
                  0x019748                  _HTTPIncFile
 .text            0x01982e       0x18ce build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device.o
                  0x01982e                  _USBDeviceInit
                  0x019942                  _USBDeviceTasks
                  0x019ade                  _USBEnableEndpoint
                  0x019b18                  _USBTransferOnePacket
                  0x019c52                  _USBStallEndpoint
                  0x019de0                  _USBCancelIO
                  0x019f72                  _USBDeviceDetach
                  0x019f84                  _USBDeviceAttach
                  0x019fc6                  _USBCtrlEPAllowStatusStage
                  0x01a0fe                  _USBCtrlEPAllowDataStage
 .text            0x01b0fc       0x126a build/XC16_dsPIC33EP512MU810/debug/Pesage.o
                  0x01b0fc                  _GestionCyclePesage
 .text            0x01c366        0xd92 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ENC28J60.o
                  0x01c366                  _MACInit
                  0x01c496                  _MACIsLinked
                  0x01c4ac                  _MACIsTxReady
                  0x01c4c4                  _MACDiscardRx
                  0x01c500                  _MACGetFreeRxSize
                  0x01c58a                  _MACGetHeader
                  0x01c65c                  _MACPutHeader
                  0x01c6b2                  _MACFlush
                  0x01c7f4                  _MACSetReadPtrInRx
                  0x01c826                  _MACSetWritePtr
                  0x01c85c                  _MACSetReadPtr
                  0x01c892                  _MACCalcRxChecksum
                  0x01c8f8                  _CalcIPBufferChecksum
                  0x01c9ae                  _MACMemCopyAsync
                  0x01cbb4                  _MACIsMemCopyDone
                  0x01cbcc                  _MACGet
                  0x01cbfe                  _MACGetArray
                  0x01ccdc                  _MACPut
                  0x01cd14                  _MACPutArray
                  0x01cece                  _ReadPHYReg
                  0x01d016                  _WritePHYReg
                  0x01d06e                  _MACPowerDown
                  0x01d0a2                  _MACPowerUp
                  0x01d0c4                  _SetCLKOUT
                  0x01d0da                  _GetCLKOUT
 .text            0x01d0f8        0xbb4 build/XC16_dsPIC33EP512MU810/debug/user.o
                  0x01d0f8                  _InitApp
                  0x01d114                  _putsUSB
                  0x01d178                  _USB_enqMsg
                  0x01d1c4                  _DeviceCDCInitialize
                  0x01d1e8                  _DeviceCDCTasks
                  0x01d286                  _ProccessCmd
                  0x01d9f6                  _CRC_Init
                  0x01da06                  _CRC_ChecksumWord
                  0x01da6c                  _ResetCounterMillis
                  0x01da76                  _GetCounterMillis
                  0x01da8c                  _UpdateB40ADI
 .text            0x01dcac        0xb5e build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/BerkeleyAPI.o
                  0x01dcac                  _BerkeleySocketInit
                  0x01dcd8                  _socket
                  0x01dd72                  _bind
                  0x01de12                  _listen
                  0x01df2e                  _accept
                  0x01e074                  _connect
                  0x01e1f4                  _send
                  0x01e214                  _sendto
                  0x01e3d8                  _recv
                  0x01e470                  _recvfrom
                  0x01e5d0                  _gethostname
                  0x01e632                  _closesocket
 .text            0x01e80a        0xb08 build/XC16_dsPIC33EP512MU810/debug/CustomHTTPApp.o
                  0x01e80a                  _HTTPNeedsAuth
                  0x01e83e                  _HTTPCheckAuth
                  0x01e870                  _HTTPExecuteGet
                  0x01e8f4                  _HTTPExecutePost
                  0x01ec66                  _HTTPPrint_builddate
                  0x01ecb4                  _HTTPPrint_version
                  0x01ecd4                  _HTTPPrint_btn
                  0x01ed2a                  _HTTPPrint_led
                  0x01ed7e                  _HTTPPrint_ledSelected
                  0x01ede2                  _HTTPPrint_pot
                  0x01ee10                  _HTTPPrint_lcdtext
                  0x01ee4a                  _HTTPPrint_hellomsg
                  0x01ee96                  _HTTPPrint_cookiename
                  0x01eee4                  _HTTPPrint_uploadeImage
                  0x01eeea                  _HTTPPrint_uploadedmd5
                  0x01ef3c                  _HTTPPrintIP
                  0x01efa2                  _HTTPPrint_config_hostname
                  0x01efc0                  _HTTPPrint_config_dhcpchecked
                  0x01efea                  _HTTPPrint_config_ip
                  0x01f018                  _HTTPPrint_config_gw
                  0x01f046                  _HTTPPrint_config_subnet
                  0x01f074                  _HTTPPrint_config_dns1
                  0x01f0a2                  _HTTPPrint_config_dns2
                  0x01f0d0                  _HTTPPrint_config_mac
                  0x01f188                  _HTTPPrint_read_comm
                  0x01f190                  _HTTPPrint_write_comm
                  0x01f198                  _HTTPPrint_reboot
                  0x01f1a0                  _HTTPPrint_rebootaddr
                  0x01f1be                  _HTTPPrint_ddns_user
                  0x01f1c4                  _HTTPPrint_ddns_pass
                  0x01f1ca                  _HTTPPrint_ddns_host
                  0x01f1d0                  _HTTPPrint_ddns_service
                  0x01f1d8                  _HTTPPrint_ddns_status
                  0x01f1f8                  _HTTPPrint_ddns_status_msg
                  0x01f246                  _HTTPPrint_smtps_en
                  0x01f266                  _HTTPPrint_snmp_en
                  0x01f286                  _HTTPPrint_status_ok
                  0x01f2cc                  _HTTPPrint_status_fail
 .text            0x01f312        0xaf2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/MPFS2.o
                  0x01f312                  _MPFSInit
                  0x01f33e                  _MPFSOpen
                  0x01f494                  _MPFSOpenID
                  0x01f51e                  _MPFSClose
                  0x01f544                  _MPFSGet
                  0x01f6d4                  _MPFSGetArray
                  0x01f8fe                  _MPFSGetLong
                  0x01f920                  _MPFSSeek
                  0x01fb32                  _MPFSGetTimestamp
                  0x01fb78                  _MPFSGetMicrotime
                  0x01fbbe                  _MPFSGetFlags
                  0x01fc02                  _MPFSGetSize
                  0x01fc48                  _MPFSGetBytesRem
                  0x01fc86                  _MPFSGetStartAddr
                  0x01fcce                  _MPFSGetEndAddr
                  0x01fd20                  _MPFSGetFilename
                  0x01fd84                  _MPFSGetPosition
                  0x01fdaa                  _MPFSGetID
 .text            0x01fe04        0x9c6 build/XC16_dsPIC33EP512MU810/debug/main.o
                  0x01fe04                  _main
                  0x01ff34                  _ABCCMainStateMachine
                  0x01ffda                  _DisplayIPValue
                  0x020010                  _GestionReponseModbus
                  0x02017c                  _ProcessIO
                  0x0203c0                  _InitTCPIPAppConfig
                  0x02049c                  _InitializeBoard
                  0x02066e                  _SaveAppConfig
                  0x0206a6                  _ADInit
                  0x0206f8                  _LEDUpdateUSBStatus
                  0x020766                  _USER_USB_CALLBACK_EVENT_HANDLER
 .text            0x0207ca        0x8b4 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Helpers.o
                  0x0207ca                  _LFSRSeedRand
                  0x02080c                  _LFSRRand
                  0x02087c                  _GenerateRandomDWORD
                  0x020986                  _StringToIPAddress
                  0x020b00                  _Base64Decode
                  0x020c68                  _uitoa
                  0x020ce8                  _hexatob
                  0x020d52                  _btohexa_high
                  0x020d74                  _btohexa_low
                  0x020d92                  _stricmppgm2ram
                  0x020e2a                  _swaps
                  0x020e46                  _swapl
                  0x020ea6                  _CalcIPChecksum
                  0x020f28                  _strupr
                  0x020f68                  _FormatNetBIOSName
                  0x020fb2                  _strnchr
                  0x021000                  _strncpy_m
 .text            0x02107e        0x896 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/DNS.o
                  0x02107e                  _DNSBeginUsage
                  0x02109e                  _DNSEndUsage
                  0x0210d6                  _DNSResolve
                  0x021116                  _DNSIsResolved
 .text            0x021914        0x87a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/UDP.o
                  0x021914                  _UDPInit
                  0x021934                  _UDPOpenEx
                  0x021a4e                  _UDPTask
                  0x021c90                  _UDPIsOpened
                  0x021cb2                  _UDPClose
                  0x021cf4                  _UDPSetTxBuffer
                  0x021d0a                  _UDPSetRxBuffer
                  0x021d20                  _UDPIsPutReady
                  0x021d56                  _UDPPut
                  0x021d86                  _UDPPutArray
                  0x021dc2                  _UDPPutString
                  0x021de0                  _UDPFlush
                  0x021eda                  _UDPIsGetReady
                  0x021f10                  _UDPGet
                  0x021f44                  _UDPGetArray
                  0x021f90                  _UDPDiscard
                  0x021fb6                  _UDPProcess
 .text            0x02218e        0x866 build/XC16_dsPIC33EP512MU810/debug/UARTsComm.o
                  0x02218e                  _UARTs_Init
                  0x022284                  _BaudrateIsValid
                  0x0222f4                  _UART1_SetBaudrate
                  0x02234a                  _UART2_SetBaudrate
                  0x0223a0                  _UART3_SetBaudrate
                  0x0223f6                  _UART4_SetBaudrate
                  0x02244c                  _UART1_SetStopBit
                  0x02248a                  _UART2_SetStopBit
                  0x0224c8                  _UART1_SetParityNBits
                  0x022520                  _UART2_SetParityNBits
                  0x022578                  _ReceiveUART1
                  0x0225ee                  _ReceiveUART2
                  0x02272c                  _ReceiveUART3
                  0x02285e                  _ReceiveUART4
                  0x022990                  _SendStrUART3
                  0x0229bc                  _SendStrUART4
 .text            0x0229f4        0x748 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_setup.o
                  0x0229f4                  _ABCC_SetupInit
                  0x022a22                  _ABCC_SetupCommands
                  0x022d52                  _ABCC_SetupResponses
                  0x0230dc                  _ABCC_UserInitComplete
                  0x023114                  _ABCC_NetworkType
                  0x02311e                  _ABCC_ModuleType
                  0x023128                  _ABCC_NetFormatType
                  0x023132                  _ABCC_ParameterSupport
 .text            0x02313c        0x6a2 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o
                  0x02316a                  _ABCC_DrvSpiRunDriverTx
                  0x0232a6                  _ABCC_DrvSpiRunDriverRx
                  0x023438                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_spi_drv_DataReceived
                  0x02347e                  build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_spi_drv.o:_drv_WdTimeoutHandler
                  0x02348c                  _ABCC_DrvSpiInit
                  0x023534                  _ABCC_DrvSpiWriteMessage
                  0x0235b0                  _ABCC_DrvSpiWriteProcessData
                  0x0235e6                  _ABCC_DrvSpiIsReadyForWriteMessage
                  0x02360c                  _ABCC_DrvSpiIsReadyForCmd
                  0x02362c                  _ABCC_DrvSpiSetNbrOfCmds
                  0x023638                  _ABCC_DrvSpiSetAppStatus
                  0x023648                  _ABCC_DrvSpiSetPdSize
                  0x0236a4                  _ABCC_DrvSpiSetMsgReceiverBuffer
                  0x0236ec                  _ABCC_DrvSpiGetIntStatus
                  0x023710                  _ABCC_DrvSpiGetAnybusState
                  0x02371e                  _ABCC_DrvSpiReadProcessData
                  0x023736                  _ABCC_DrvSpiReadMessage
                  0x023758                  _ABCC_DrvSpiSetIntMask
                  0x023768                  _ABCC_DrvSpiGetWrPdBuffer
                  0x023778                  _ABCC_DrvSpiGetModCap
                  0x02379c                  _ABCC_DrvSpiGetLedStatus
                  0x0237a6                  _ABCC_DrvSpiIsReadyForWrPd
                  0x0237ba                  _ABCC_DrvSpiIsSupervised
                  0x0237d0                  _ABCC_DrvSpiGetAnbStatus
 .text            0x0237de        0x62a build/XC16_dsPIC33EP512MU810/debug/AD7190.o
                  0x0237de                  _AD7190_SetRegisterValue
                  0x023830                  _AD7190_GetRegisterValue
                  0x0238a2                  _AD7190_Init
                  0x0238d6                  _AD7190_Reset
                  0x023902                  _AD7190_SetPower
                  0x023992                  _AD7190_WaitRdyGoLow
                  0x0239c6                  _AD7190_ChannelSelect
                  0x023a26                  _AD7190_Calibrate
                  0x023ab4                  _AD7190_RangeSetup
                  0x023b3a                  _AD7190_SingleConversion
                  0x023b7a                  _AD7190_ContinuousReadAvg
                  0x023be2                  _AD7190_TemperatureRead
                  0x023c44                  _AD7190_StartContinuousRead
                  0x023cac                  _AD7190_StopContinuousRead
                  0x023cce                  _AD7190_PrintRegisters
 .text            0x023e08        0x628 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_handler.o
                  0x023e08                  _ABCC_SetReadyForCommunication
                  0x023e12                  _ABCC_SetMainStateError
                  0x023e1c                  _ABCC_GetMainState
                  0x023e26                  _ABCC_CheckAnbStatus
                  0x023e46                  _ABCC_CheckSendMessage
                  0x023e50                  _ABCC_StartDriver
                  0x023fe8                  _ABCC_isReadyForCommunication
                  0x024070                  _ABCC_NewWrPdEvent
                  0x02409e                  _ABCC_RdPdEvent
                  0x0240c2                  _ABCC_RdMsgEvent
                  0x02414a                  _ABCC_SendCmdMsg
                  0x02419a                  _ABCC_GetCmdQueueSize
                  0x0241a8                  _ABCC_SendRespMsg
                  0x0241ba                  _ABCC_MsgAlloc
                  0x0241c8                  _ABCC_MsgFree
                  0x0241da                  _ABCC_SetPdSize
                  0x024202                  _ABCC_HWReset
                  0x02421e                  _ABCC_ShutdownDriver
                  0x024240                  _ABCC_ModuleDetect
                  0x02424e                  _ABCC_ModCap
                  0x02425c                  _ABCC_LedStatus
                  0x02426a                  _ABCC_AnbState
                  0x024278                  _ABCC_IsSupervised
                  0x024286                  _ABCC_HWReleaseReset
                  0x024290                  _ABCC_SetAppStatus
                  0x02429e                  _ABCC_ReadModuleId
                  0x0242ac                  _ABCC_RunTimerSystem
                  0x0242ba                  _ABCC_GetNewSourceId
                  0x0242ea                  _ABCC_GetOpmode
                  0x0242f8                  _ABCC_GetAttribute
                  0x024350                  _ABCC_SetByteAttribute
                  0x0243b2                  _ABCC_VerifyMessage
                  0x0243c6                  _SetErrorReporter
                  0x0243d2                  _ABCC_GetDataTypeSize
 .text            0x024430        0x570 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_link.o
                  0x02450e                  _ABCC_LinkInit
                  0x024598                  _ABCC_LinkReadMessage
                  0x024618                  _ABCC_LinkCheckSendMessage
                  0x0246a2                  _ABCC_LinkRunDriverRx
                  0x0246c0                  _ABCC_LinkGetNumCmdQueueEntries
                  0x0246d4                  _ABCC_LinkWriteMessage
                  0x0247f2                  _ABCC_LinkWrMsgWithNotification
                  0x024836                  _ABCC_LinkAlloc
                  0x02484c                  _ABCC_LinkFree
                  0x0248aa                  _ABCC_LinkMapMsgHandler
                  0x0248fe                  _ABCC_LinkGetMsgHandler
                  0x02495c                  _ABCC_LinkIsSrcIdUsed

.dinit            0x0249a0        0x4fa
 .dinit           0x0249a0        0x4fa data_init

.text             0x024e9a       0x4932
 .text            0x024e9a        0x4aa build/XC16_dsPIC33EP512MU810/debug/MemFlash.o
                  0x024e9a                  _Flash_N_Clock
                  0x024eb8                  _Active_Flash
                  0x024ec0                  _Desactive_Flash
                  0x024ece                  _Flash_Ready
                  0x024ef0                  _Wait_Flash_Ready
                  0x024f00                  _Write_Flash
                  0x024f32                  _Charge_Pointeurs
                  0x024f4a                  _Lecture_Byte_In_Flash
                  0x024f66                  _Direct_Byte_Write_In_Page
                  0x024f7e                  _Transfert_Page_To_Buffer
                  0x024f96                  _Read_Flash
                  0x024fd2                  _Incremente_Adresse_FlashDB32
                  0x0250a0                  _Incremente_Adresse_FlashDB64
                  0x02516e                  _MakeAddrDB32
                  0x0251ca                  _MakeAddrDB64
                  0x02522c                  _Ecriture_Memoire_Flash_Ligne_Str
                  0x0252bc                  _Lecture_Memoire_Flash_Ligne_Str
 .text            0x025344        0x44e build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_device_cdc.o
                  0x025344                  _USBCheckCDCRequest
                  0x02548e                  _CDCInitEP
                  0x0254de                  _USBCDCEventHandler
                  0x025524                  _getsUSBUSART
                  0x0255b8                  _putUSBUSART
                  0x0255e4                  _putsUSBUSART
                  0x02563a                  _putrsUSBUSART
                  0x025690                  _CDCTxService
 .text            0x025792        0x440 build/XC16_dsPIC33EP512MU810/debug/B40/app_obj.o
                  0x025792                  _APP_IsResetRequestAllowed
                  0x0257a8                  _APP_ProcResetRequest
                  0x0257d4                  _APP_ProcessCmdMsg
                  0x0257fe                  _app_InstanceCommand
                  0x025a08                  _app_ObjectCommand
 .text            0x025bd2        0x3ae build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/NBNS.o
                  0x025bd2                  _NBNSTask
 .text            0x025f80        0x3a8 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ARP.o
                  0x025f80                  _ARPSendPkt
                  0x026054                  _ARPInit
                  0x026086                  _ARPProcess
                  0x02615e                  _ARPResolve
                  0x026228                  _ARPIsResolved
                  0x0262f0                  _SwapARPPacket
 .text            0x026328        0x358 build/XC16_dsPIC33EP512MU810/debug/SPIFRAM.o
                  0x026328                  _FRAMInit
                  0x026340                  _FRAMBeginRead
                  0x026358                  _FRAMRead
                  0x02639c                  _FRAMReadArray
                  0x026478                  _FRAMBeginWrite
                  0x026490                  _FRAMWrite
                  0x0264d2                  _FRAMWriteArray
                  0x026500                  _FRAMEndWrite
                  0x02660e                  _FRAMIsBusy
 .text            0x026680        0x350 build/XC16_dsPIC33EP512MU810/debug/Depeseur.o
                  0x026680                  _Dep_AttenteDCY
                  0x0266fe                  _Dep_Chargement
                  0x0267d6                  _Dep_AttenteFermVanne
                  0x0268c4                  _Dep_Suspension
                  0x026968                  _gestion_cycle_Depeseur
 .text            0x0269d0        0x336 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/SPIEEPROM.o
                  0x0269d0                  _XEEInit
                  0x0269ee                  _XEEBeginRead
                  0x026a06                  _XEERead
                  0x026a4a                  _XEEEndRead
                  0x026a54                  _XEEReadArray
                  0x026b12                  _XEEBeginWrite
                  0x026b2a                  _XEEWrite
                  0x026b6c                  _XEEWriteArray
                  0x026b9a                  _XEEEndWrite
                  0x026c94                  _XEEIsBusy
 .text            0x026d06        0x300 build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPServer.o
                  0x026d06                  _TestModbus
                  0x026d6a                  _BerkeleyTCPServer
 .text            0x027006        0x2ec build/XC16_dsPIC33EP512MU810/debug/ECAN/ECAN1Drv.o
                  0x027006                  _ECANFilterSID
                  0x027036                  _ECANFilterEID
                  0x027048                  _ECAN1DMAConfig
                  0x027090                  _ECAN1ClockConfig
                  0x0270a0                  _ECAN1InterruptConfig
                  0x0270ca                  _ECAN1TxRxBuffersConfig
                  0x0270d4                  _ECAN1RxFiltersConfig
                  0x027140                  _ECAN1SendPacket
                  0x027176                  _ECAN1SetOPMode
                  0x027192                  _ECANCreateSIDPacket
                  0x0271e6                  _ECANCreateEIDPacket
 .text            0x0272f2        0x2e4 build/XC16_dsPIC33EP512MU810/debug/B40/dpv1.o
                  0x0272f2                  _DPV1_ProcessCmdMsg
                  0x02731c                  _dpv1_InstanceCommand
                  0x027478                  _dpv1_ObjectCommand
 .text            0x0275d6        0x2c2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/ICMP.o
                  0x0275d6                  _ICMPProcess
                  0x0276c2                  _ICMPSendPing
                  0x0276e6                  _ICMPSendPingToHost
                  0x027710                  _ICMPGetReply
                  0x02786a                  _ICMPBeginUsage
                  0x02788a                  _ICMPEndUsage
 .text            0x027898        0x280 build/XC16_dsPIC33EP512MU810/debug/Regul.o
                  0x027898                  _RegulationDoseur
                  0x0279a8                  _RegulationPID
 .text            0x027b18        0x27a build/XC16_dsPIC33EP512MU810/debug/BerkeleyUDPClient.o
                  0x027b18                  _BerkeleyUDPClient
                  0x027d40                  _BerkeleySNTPGetUTCSeconds
 .text            0x027d92        0x252 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_crc32.o
                  0x027d92                  _CRC_Crc32
 .text            0x027fe4        0x23c build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o
                  0x027fe4                  _US_Init
                  0x027fee                  _US_RunUserInitStateMachine
                  0x0280e4                  build/XC16_dsPIC33EP512MU810/debug/B40/user_setup.o:_US_ProcessRespMsg
                  0x0281fc                  _US_SetSwitch1
                  0x02820e                  _US_SetSwitch2
 .text            0x028220        0x1f4 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_timer.o
                  0x028220                  _ABCC_TimerInit
                  0x028242                  _ABCC_TimerCreate
                  0x0282b4                  _ABCC_TimerStart
                  0x028332                  _ABCC_TimerStop
                  0x028374                  _ABCC_TimerTick
 .text            0x028414        0x1d8 build/XC16_dsPIC33EP512MU810/debug/BdC.o
                  0x028414                  _BdC_VerifContacts
                  0x02841a                  _BdC_AttenteDCY
                  0x028480                  _BdC_InitChargement
                  0x0285aa                  _BdC_Chargement
                  0x0285cc                  _gestion_cycle_BdC
 .text            0x0285ec        0x1ca build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/IP.o
                  0x0285ec                  _IPGetHeader
                  0x0286b6                  _IPPutHeader
                  0x028768                  _IPSetRxBuffer
 .text            0x0287b6        0x1c2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Announce.o
                  0x0287b6                  _AnnounceIP
                  0x028860                  _DiscoveryTask
 .text            0x028978        0x1c2 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/StackTsk.o
                  0x028978                  _StackInit
                  0x0289b0                  _StackTask
                  0x028b24                  _StackApplications
 .text            0x028b3a        0x16a build/XC16_dsPIC33EP512MU810/debug/B40/abcc_cbf.o
                  0x028b3a                  _ABCC_CbfUserInitReq
                  0x028b48                  _ABCC_CbfAdiMappingReq
                  0x028b5a                  _ABCC_CbfRemapDone
                  0x028b64                  _ABCC_CbfUpdateWriteProcessData
                  0x028b76                  _ABCC_CbfNewReadPd
                  0x028b84                  _ABCC_CbfDriverError
                  0x028ba6                  _ABCC_CbfReceiveMsg
                  0x028c16                  _ABCC_CbfWdTimeout
                  0x028c2c                  _ABCC_CbfWdTimeoutRecovered
                  0x028c42                  _ABCC_CbfEvent
                  0x028c7c                  _ABCC_CbfAnbStatusChanged
 .text            0x028ca4        0x160 build/XC16_dsPIC33EP512MU810/debug/MODBUSTCPServer.o
                  0x028ca4                  _MODBUSTCPServer
                  0x028d42                  _ProcessReceivedMessage
                  0x028dd6                  _ModbusError
 .text            0x028e04        0x15a build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Tick.o
                  0x028e04                  _TickInit
                  0x028e96                  _TickGet
                  0x028ec8                  _TickGetDiv256
                  0x028efa                  _TickGetDiv64K
                  0x028f2c                  _TickConvertToMilliseconds
                  0x028f46                  __T1Interrupt
 .text            0x028f5e        0x12e build/XC16_dsPIC33EP512MU810/debug/BerkeleyTCPClient.o
                  0x028f5e                  _BerkeleyTCPClient
 .text            0x02908c        0x118 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_sys_adapt.o
                  0x02908c                  _ABCC_SYS_Init
                  0x0290b6                  _ABCC_SYS_Close
                  0x0290c0                  _ABCC_SYS_SetOpmode
                  0x0290c8                  _ABCC_SYS_GetOpmode
                  0x0290d2                  _ABCC_SYS_HWReset
                  0x0290da                  _ABCC_SYS_HWReleaseReset
                  0x0290e2                  _ABCC_SYS_ReadModuleId
                  0x0290ec                  _ABCC_SYS_ModuleDetect
                  0x029104                  _ABCC_SYS_AbccInterruptEnable
                  0x029110                  _ABCC_SYS_AbccInterruptDisable
                  0x029118                  _ABCC_SYS_EnterCriticalImpl
                  0x02911e                  _ABCC_SYS_ExitCriticalImpl
                  0x029124                  _ABCC_SYS_UseCriticalImpl
                  0x02912a                  _ABCC_SYS_SpiRegDataReceived
                  0x029136                  _ABCC_SYS_SpiSendReceive
 .text            0x0291a4        0x118 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Reboot.o
                  0x0291a4                  _RebootTask
 .text            0x0292bc        0x116 build/XC16_dsPIC33EP512MU810/debug/ADC10bitsDrv.o
                  0x0292bc                  _InitAdc1
                  0x02931c                  _InitTmr3
                  0x029330                  _InitDma0
                  0x029368                  _ProcessADCSamples
 .text            0x0293d2        0x100 build/XC16_dsPIC33EP512MU810/debug/ADComm.o
                  0x0293d2                  _ADSPI_Init
                  0x0293f8                  _SPI_Read
                  0x02946a                  _SPI_Write
 .text            0x0294d2         0xc8 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_mem.o
                  0x0294d2                  _ABCC_MemCreatePool
                  0x02951e                  _ABCC_MemAlloc
                  0x02955a                  _ABCC_MemFree
 .text            0x02959a         0x86 build/XC16_dsPIC33EP512MU810/debug/B40/spi/abcc_handler_spi.o
                  0x02959a                  _ABCC_SpiRunDriver
                  0x0295f6                  _ABCC_SpiISR
 .text            0x029620         0x7e build/XC16_dsPIC33EP512MU810/debug/system.o
                  0x029620                  _ConfigureOscillator
 .text            0x02969e         0x78 build/XC16_dsPIC33EP512MU810/debug/TCPIPStack/Delay.o
                  0x02969e                  _DelayMs
                  0x0296da                  _Delay10us
 .text            0x029716         0x56 build/XC16_dsPIC33EP512MU810/debug/usb/src/usb_hal_dspic33e.o
                  0x029716                  _USBSleepOnSuspend
 .text            0x02976c         0x42 build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o
                  0x02976c                  build/XC16_dsPIC33EP512MU810/debug/B40/abcc_remap.o:_abcc_RemapRespMsgSent
                  0x029782                  _ABCC_SendRemapRespMsg
 .text            0x0297ae         0x1e build/XC16_dsPIC33EP512MU810/debug/B40/user_adi.o
                  0x0297ae                  _AD_GetNumAdi
                  0x0297b8                  _ADI_GetDefaultMap
                  0x0297c2                  _ADI_GetADIEntryList

MPFSHelpers       0x0297cc          0xe
 MPFSHelpers      0x0297cc          0xe build/XC16_dsPIC33EP512MU810/debug/MPFSImg2.o
                  0x0297cc                  _ReadProgramMemory
