This is a library for the Adafruit HX8357 display products

This library works with the Adafruit 3.5" Breakout
  ----> http://www.adafruit.com/products/2050
 
Check out the links above for our tutorials and wiring diagrams.
These displays use SPI to communicate, 4 or 5 pins are required
to interface (RST is optional).

Adafruit invests time and resources providing this open source code,
please support Adafruit and open-source hardware by purchasing
products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.
MIT license, all text above must be included in any redistribution

To download. click the DOWNLOADS button in the top right corner, rename the uncompressed folder Adafruit_HX8357. Check that the Adafruit_HX8357 folder contains Adafruit_HX8357.cpp and Adafruit_HX8357.

Place the Adafruit_HX8357 library folder your arduinosketchfolder/libraries/ folder. You may need to create the libraries subfolder if its your first library. Restart the IDE

Also requires the Adafruit_GFX library for Arduino.
