;
; VAG-COM Label File
;
; Audi A4 (8E) / Audi A6 (4B) / Audi A8 (4D) / Skoda Superb (3U) / VW Passat (3B)
;
; Component: J431 - Dynamic Headlight Aim Control (#55)
;
; P/N: 4Z7-907-357-???
;
; includes measuring blocks, basic setting and coding
;
; created on 27/Sep/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 27/Nov/2005 by Jose Carlos Fernandez (josecarlosfernandez@terra.es)
; updated on 10/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 02/Sep/2006
;
; requires VAG-COM 607.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage Supply,(Terminal 15)
001,2,Light Switch,Status,Display Range:\n\n 1 = ON\n 2 = OFF
001,3,Vehicle Speed
001,4,Acceleration
;
B001,0,Adjustment Position
B001,1,Status
B001,2,,,
B001,3,,,
B001,4,,,
;
002,1,Voltage level,sensor front,Specification (Basic Setting): 1.7...3.5 V\n\n0 Volt  => Level Sensor faulty\n+5 Volts => Wiring faulty
002,2,Voltage level,sensor rear,Specification (Basic Setting): 1.7...3.5 V\n\n0 Volt  => Level Sensor faulty\n+5 Volts => Wiring faulty
002,3,Actuator Motor,Activation
002,4,Time Constant
;
B002,0,Adjustment Learning
B002,1,Status
B002,2,,,
B002,3,,,
B002,4,,,
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Dynamic Headlight Aim Control (J431) Coding
C01,00001 = Audi A8 (4D - Facelift)
C02,00005 = Skoda Superb (3U) FWD
C03,00006 = Skoda Superb (3U) AWD
C04,00007 = VW Passat (3B) FWD
C05,00008 = VW Passat (3B) AWD
C06,00020 = Audi A6 V8 (4B)
C07,00030 = Audi A6 Allroad (4B)
C08,00040 = Audi A6 FWD (4B - Facelift)
C09,00050 = Audi A6 Quattro (4B - Facelift)
C10,00060 = Audi A4 (8E)
C11,00070 = Audi A4 Cabrio/Coupé (8E)
;
