;
; VAG-COM Label File
;
; Audi A3 (8P)
;
; Component: J393 - Comfort System (#46)
;
; P/N: 8P0-959-433-??? (14 Byte)
;
; includes long coding
;
; created on 13/Sep/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 18/Oct/2007
;
; requires VAG-COM 708.0 / LCode 709.0 or newer
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,0,Selective Central Locking (Single Door Opening)
LC,00,3,Auto-Unlock (unlocking after removing key from ignition)
LC,00,4,Auto-Lock (automatic locking from 15 km/h)
LC,02,1,Central Locking (Rear Lid) "Security Lock"
LC,05,0,Comfort Function inactive
LC,05,1,Comfort Function Power Windows/Sunroof via Drivers Door Lock inactive
LC,05,2,Comfort Function Power Windows/Sunroof via Passengers Door Lock inactive
LC,05,3,Comfort Function Power Windows/Sunroof via Rear Lid Door Lock inactive
LC,05,4,Comfort Function Power Windows/Sunroof via Power Window Switch inactive
LC,05,5,Comfort Function Power Windows/Sunroof via Remote Control inactive
LC,05,6,Comfort Function automatic Closing
LC,05,7,Power Windows/Sunroof disabled after door Opening
LC,06,0,Comfort Opening Power Windows via Door Lock active
LC,06,1,Comfort Opening Power Windows via Power Window Switch active
LC,06,2,Comfort Opening Power Windows via Remote Control active
LC,06,3,Comfort Closing Power Windows via Door Lock active
LC,06,4,Comfort Closing Power Windows via Power Window Switch active
LC,06,5,Comfort Closing Power Windows via Remote Control active
LC,06,6,Comfort Function after authorized Access only for a limited Time
LC,07,0,Comfort Opening Sunroof via Door Lock active
LC,07,1,Comfort Opening Sunroof via Power Window Switch active
LC,07,2,Comfort Opening Sunroof via Remote Control active
LC,07,3,Comfort Closing Sunroof via Door Lock active
LC,07,4,Comfort Closing Sunroof via Power Window Switch active
LC,07,5,Comfort Closing Sunroof via Remote Control active
LC,08,0,Unlocking Confirmation (Blink) via Door Locks
LC,08,1,Unlocking Confirmation (Horn) via Door Locks
LC,08,2,Unlocking Confirmation (Blink) via Remote Control
LC,08,3,Unlocking Confirmation (Horn) via Remote Control
LC,08,7,Horn Confirmation Configuration blocked
LC,09,0,Locking Confirmation (Blink) via Door Locks
LC,09,1,Locking Confirmation (Horn) via Door Locks
LC,09,2,Locking Confirmation (Blink) via Remote Control
LC,09,3,Locking Confirmation (Horn) via Remote Control
LC,10,0,Remote Control inactive
LC,10,1,Remote Control with "Terminal 15 ON" inactive
LC,10,2,Remote Control Range Limitation active
LC,10,3,Manual Remote Control learning/unlearning active
LC,10,6,Anti-Theft-System Activation Confirmation (Blink)
LC,10,7,Anti-Theft-System Activation Confirmation (Horn)
LC,11,0,Doors (0 = 2-doors / 1 = 4-doors)
LC,11,1,Front Power Windows installed
LC,11,2,Rear Power Windows installed
LC,11,3,Central Locking installed
LC,11,4,Model (0 = Left-Hand-Drive/ 1 = Right-Hand-Drive)
LC,11,6,Synchronised Mirror Adjustment
LC,11,7,Mirror Lowering with Reverse Rear (only with Memory Seats)
LC,12,0,Anti-Theft System deactivated
LC,12,1,Anti-Theft System disarming only via Remote Control or Immobilizer
LC,12,2,Anti-Theft active with intentional de-safe / Interior Monitoring inactive
LC,12,3,Anti-Theft Alarm Delay (15 sec) inactive (Thatcham)
LC,12,5,Anti-Theft System passive arming
LC,12,6,Inclination Sensor installed
LC,12,7,Interior Monitoring installed
LC,13,4,Siren installed
LC,13,5,Siren Tone Type (0 = frequency modulated / 1 = discontinuoud)
LC,13,6,Siren Alarm Type (0 = 10 Alarms (GB/Irland) / 1 = 1 Alarm (RoW))
LC,13,7,Siren Configuration blocked
;
