;
; VAG-COM Label File
;
; Audi A3 (8P) / Audi R8 (42) / Audi TT (8J)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 8P0-953-549-???
;
; includes measuring blocks, coding and selective output test
;
; created on 23/Apr/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 23/Apr/2007
;
; requires VAG-COM 606.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Blinker,,Range: n. operated/left/right
001,2,Headlamp Flasher,,Range: n. operated/operated
001,3,High Beam,,Range: n. operated/operated
001,4,Front Wiper,,Range: n. operated/level/Stage Int./Stage 1/Stage 2
;
002,1,Interval Stages,,Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Range: n. operated/operated
002,3,Wiping Rear,,Range: n. operated/operated/not installed
002,4,Washing Rear,,Range: n. operated/operated/not installed
;
003,1,Terminal Status,,?xxxx = P-Contact\nx?xxx = S-Contact\nxx?xx = Terminal 75\nxxx?x = Terminal 15\nxxxx? = Terminal 50
003,2,Horn,,Range: n. operated/operated
003,3,Board Computer,Lever,Range: n. installed/n. operated/Reset/Up/Down
;
004,0,Cruise Control System (CCS)
004,1,Cruise Control,Main Switch,Display Range: n. installed/off/on
004,2,Cruise Control,Activation,Range: n. operated/operated
004,3,Cruise Control,Status,Display Range: n. operated/decelerate/accelerate/Reset
;
005,1,Park Position in,Selector Lever,Display Range: n. installed/n.Ok/on/recognized
005,2,Selector Lever,Information (Pos. P),Display Range: n. defined/recognized/on
005,3,Key,Removal Lock,Display Range: n. installed/on/off
005,4,Status Key,Removal Lock,Display Range: n. installed/Ok/n.Ok
;
006,0,Multifunction Steering Wheel
006,1,Communication,,Range: n. intalled/Ok/n.Ok
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Range: yes/no
;
007,0,Multifunction Steering Wheel
007,1,Buttons pressed
007,2,Buttons pressed
007,3,Thumb Button,Left,Range: n. operated/operated/not installed
007,4,Thumb Button,Right,Range: n. operated/operated/not installed
;
008,0,Multifunction Steering Wheel
008,1,Thumb Wheel,Left,Range: n. operated/operated/not installed/up/down
008,2,Thumb Wheel,Right,Range: n. operated/operated/not installed/up/down
008,3,Tiptronic Down,,Range: n. operated/operated/not installed
008,4,Tiptronic Up,,Range: n. operated/operated/not installed
;
009,1,Dimming,,Range: 0.0...100.0 %
009,2,Calculated,Dimming (LIN),Range: 0.0...100.0 %
;
010,0,Steering Wheel Heating
010,1,Steering Wheel,Heating,Range: n. installed/off/on
010,2,Temprature,Sensor,Range: n. installed/Temperature
010,3,St.Wheel Heat.,Output
010,4,Seat Heating,Driver,Range: OFF/Stage
;
080,0,Advanced Control Module Identification I
;
080,0,Advanced Control Module Identification II
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,00?xxxx: Transmission
C02,0 = Manual Transmission
C03,1 = Automatic Transmission
C04,00x?xxx: Steering Wheel
C05,0 = Spoke Steering Wheel without Tiptronic without Multifunction
C06,1 = Spoke Steering Wheel with Tiptronic without Multifunction
C07,2 = Multifunction Steering Wheel for Radio Operation
C08,3 = Multifunction Steering Wheel for Radio/Telephone Operation
C09,4 = Multifunction Steering Wheel for Radio/Telephone/Voice Control Operation
C10,5 = Multifunction Steering Wheel for Radio/Voice Control Operation
C11,00xx?xx: Additional Equipment
C12,+1 = Tiptronic (Shift Paddels)
C13,00xxx?x: Board Computer / Cruise Control System (CCS)
C14,0 = w/o Board Computer and w/o Cruise Control System (CCS)
C15,1 = with Board Computer and w/o Cruise Control System (CCS)
C16,2 = w/o Board Computer and with Cruise Control System (CCS)
C17,4 = with Board Computer and with Cruise Control System (CCS)
C18,00xxxx?: Rear Wiper
C19,1 = Rear Wiper not installed
C20,2 = Rear Wiper installed
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T194,Ignition Key Removal Lock
;
