;
; VCDS Label File
;
; Copyright © 2008-2009 Ross-Tech, LLC
;
; Audi A3/Cabriolet (8P) / Seat Altea/Toledo (5P) / Seat Leon (1P)
; Skoda Octavia (1Z) / VW Caddy (2K) / VW Eos (1F) / VW Golf/Jetta (1K)
; VW Golf Plus (5M) / VW Passat (3C) /  VW Tiguan (5N) / VW Touran (1T)
;
; Component: J345 - Trailer (#69)
;
; P/N: 1K0-907-383-D/E
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-69.LBL
; 1K0-907-383-MY7.LBL
; 1K0-907-383-MY8.LBL
;
; includes measuring blocks, long coding and selective output tests
;
; created on 15/Mar/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 24/Mar/2009
;
; requires VCDS 805.1 / LCode 804.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltage Supply I
001,1,Voltage,(Terminal 30)
001,3,Status Term. 15,(Emergency Run),Range: ON/OFF
;
002,0,Voltage Supply II
002,1,Status,Terminal 30L,Range: ON/OFF\nSignal Type: Input
002,2,Status,Terminal 30R,Range: ON/OFF\nSignal Type: Input
;
003,0,Input Signals I
003,2,Brake Light Switch,,Range: ON/OFF\nSignal Type: Input
003,3,Control Module,Temperature
;
004,0,Output Signals I
004,1,Turn Signal,Rear Left,Range: ON/OFF\nSignal Type: Output
004,2,Turn Signal,Rear Right,Range: ON/OFF\nSignal Type: Output
004,3,Tail Light,Rear Left,Range: ON/OFF\nSignal Type: Output
004,4,Tail Light,Rear Right,Range: ON/OFF\nSignal Type: Output
;
005,0,Output Signals II
005,1,Brake Lights,Rear,Range: ON/OFF\nSignal Type: Output
005,2,Back-Up Lights,Rear,Range: ON/OFF\nSignal Type: Output
005,3,Rear Fog Lights,,Range: ON/OFF\nSignal Type: Output
;
006,0,Input Signals II (CAN)
006,1,Status,Terminal 15,Range: ON/OFF\nSignal Type: Input/CAN
006,2,Status,Terminal X,Range: ON/OFF\nSignal Type: Input/CAN
006,4,Trailer,attached,Range: ON/OFF\nSignal Type: Input/CAN
;
007,0,Input Signals III (CAN)
007,1,Turn Signal,Left,Range: ON/OFF\nSignal Type: Input/CAN
007,2,Turn Signal,Right,Range: ON/OFF\nSignal Type: Input/CAN
007,3,Emergency Flasher,Warning Lights,Range: ON/OFF\nSignal Type: Input/CAN
;
008,0,Input Signals IV (CAN)
008,1,Brake Light Switch,,Range: ON/OFF\nSignal Type: Input/CAN
008,2,Brake Test Switch,,Range: ON/OFF\nSignal Type: Input/CAN
;
009,0,Input Signals V (CAN)
009,1,Side Marking,Lights,Range: ON/OFF\nSignal Type: Input/CAN
009,2,Parking Light,Left,Range: ON/OFF\nSignal Type: Input/CAN
009,3,Parking Light,Right,Range: ON/OFF\nSignal Type: Input/CAN
;
010,0,Input Signals VI (CAN)
010,1,Rear Fog Light,,Range: ON/OFF\nSignal Type: Input/CAN
010,2,Back-Up Light,,Range: ON/OFF\nSignal Type: Input/CAN
;
011,0,Input Signals VII (CAN)
011,1,Rear Lid,,Range: Open/Closed\nSignal Type: Input/CAN
011,2,Vehicle Speed,,Signal Type: Input/CAN
011,3,Rear Windshield,,Range: Open/Closed\nSignal Type: Input/CAN
;
012,0,CAN-Databus Communication (Comfort)
012,1,Central Electronics,(J519),Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
012,3,Gateway,(J533),Range: Gateway 1/Gateway 0\nSpecification: Gateway 1
012,4,Comfort System,(J393)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1019,Relay (Terminal 30G)
T2562,Trailer Brake Lights
T2564,Trailer Tail Light Left (M60)
T2563,Trailer Tail Light Right (M61)
T2566,Trailer Turn Signals Left (M62)
T2565,Trailer Turn Signals Right (M63)
T2567,Trailer Rear Fog Lights (M64)
T2568,Trailer Back-Up Lights
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,0~7,00,Control Module not coded
LC,00,0~7,01,Country: Rest of World (RoW)
LC,00,0~7,02,Country: North American Region (NAR)
LC,00,0~7,03,Country: Australia
;
;LC,03,1,Unknown (Standard?)
;
