;
; VCDS Label File
;
; Copyright © 2006-2009 Ross-Tech, LLC
;
; VW Jetta (1K) / VW Passat (3C) / VW Eos (1F)
;
; Component: J345 - Trailer (#69)
;
; P/N: 1K0-907-383/A/B/C / 8P0-907-383-???
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-69.LBL
; 1K0-907-383-MY7.LBL
; 1K0-907-383-MY8.LBL
;
; includes measuring blocks, coding and selective output tests
;
; created on 02/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 07/Feb/2009
;
; requires VCDS 805.1 or newer
;
;
;---------------------------------------------------
;
; measuring block
;
;---------------------------------------------------
;
;
001,0,Inputs
001,1,Voltage,(Terminal 30)
001,3,Status Term. 15,(Emergency Run),Range: ON/OFF
;
002,0,Inputs
002,2,Brake Light Switch,,Range: ON/OFF
;
003,0,Outputs
003,1,Turn Signal,Rear Left,Range: ON/OFF
003,2,Turn Signal,Rear Right,Range: ON/OFF
003,3,Tail Light,Left,Range: ON/OFF
003,4,Tail Light,Right,Range: ON/OFF
;
004,0,Outputs
004,1,Brake Lights,,Range: ON/OFF
004,2,Back-Up Lights,,Range: ON/OFF
004,3,Rear Fog Lights,,Range: ON/OFF
;
008,0,Input Signals
008,1,Status,Terminal 15,Range: ON/OFF
008,2,Status,Terminal X,Range: ON/OFF
008,4,Trailer,attached,Range: ON/OFF
;
009,0,Input Signals
009,1,Turn Signal,Left,Range: ON/OFF
009,2,Turn Signal,Right,Range: ON/OFF
009,3,Emergency Flasher,Warning Lights,Range: ON/OFF
;
010,0,Input Signals
010,1,Brake Light Switch,,Range: ON/OFF
;
011,0,Input Signals
011,1,Side Marking,Lights,Range: ON/OFF
011,2,Parking Light,Left,Range: ON/OFF
011,3,Parking Light,Right,Range: ON/OFF
;
012,0,Input Signals
012,1,Rear Fog Light,,Range: ON/OFF
012,2,Back-Up Light,,Range: ON/OFF
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
130,0,CAN-Databus Communication (Comfort)
130,1,Central Electronics,(J519),Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
130,2,Electrical,Ignition Lock,Range: El.Ign.Lock 1/El.Ign.Lock 0\nSpecification: El.Ign.Lock 1
130,3,CAN-Gateway,(J533),Range: Gateway 1/Gateway 0\nSpecification: Gateway 1
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1019,Relay (Terminal 30G)
T2562,Trailer Brake Lights
T2564,Trailer Tail Light Left (M60)
T2563,Trailer Tail Light Right (M61)
T2566,Trailer Turn Signals Left (M62)
T2565,Trailer Turn Signals Right (M63)
T2567,Trailer Rear Fog Lights (M64)
T2568,Trailer Back-Up Lights
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Trailer (J345) Coding
C01,0000001 = Rest of World (RoW)
C02,0000002 = North America (USA/Canada)
C03,0000003 = Australia
;
