;
; VAG-COM Label File
;
; Seat Ibiza/Cordoba (6L) / Skoda Fabia (6Y) / VW Polo (9N)
;
; Component: J519 - Central Electronics I (#09) (through Index B)
;
; P/N: 6Q?-937-049-???
;
; includes measuring blocks, coding, login and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6Q-09.LBL
; 6Qx-937-049-B.LBL (through Index B)
; 6Qx-937-049-C.LBL (from Index C)
;
; created on 07/29/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 07/29/2007
;
; requieres VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Terminal Status
001,1,Terminal S,Status,Range: operated/inactive
001,2,Terminal 50,Status,Range: ON/OFF
001,3,Terminal X,Status,Range: ON/OFF
001,4,Terminal 15,Status,Range: ON/OFF
;
002,1,Voltage,(Terminal 30)
002,2,Load Managem.,Intervention,Range: active/inactive
002,3,Blinker Switch,,Range: ON/OFF
002,4,Emergency,Flasher Button,Range: ON/OFF
;
003,0,Wiper (Front)
003,1,Wiper,,Range: ON/OFF
003,2,Wiper,Stage 1,Range: ON/OFF
003,3,Wiper,Stage 2,Range: ON/OFF
003,4,Wiper,Potentiometer,Range: Not Recognized/Stage 1/Stage 2/Stage 3/Stage 4
;
004,1,Windshield,Washer Pump,Range: ON/OFF
004,2,Rear Windshield,Heating,Range: Not Operated/Operated
004,3,Horn,,Range: Not Operated/Operated
004,4,Hood Contact,Switch,Range: ON/OFF
;
005,0,Door Status
005,1,Driver's Door,Contact Switch,Range: Door open/Door closed
005,2,Passenger Door,Contact Switch,Range: Door open/Door closed
005,3,Rear Left,Contact Switch,Range: Door open/Door closed
005,4,Rear Right,Contact Switch,Range: Door open/Door closed
;
006,0,Trunk Lid Status (II)
006,1,Trunk Contact,Switch (Locking),Range: ON/OFF
006,2,Trunk Contact,Switch (Light),Range: ON/OFF
;
007,0,Trunk Lid Status (II)
007,1,Trunk Lid Handle,Push-Button,Range: Not Operated/Operated
007,2,Trunk Lid Interior,Push-Button,Range: Not Operated/Operated
007,3,Lock,Service Position,,Range: ON/OFF
;
008,1,Headlight Washers,,Range: ON/OFF/Not Installed
008,2,Heated Mirrors,,Range: ON/OFF
008,3,Reverse Gear,,Range: Reverse OFF/Reverse ON
008,4,Heated Front,Windshield,,Range: ON/OFF/Not Installed
;
009,0,Cruise Control System (CCS)
009,1,CCS Main Switch,,Range: Not Operated/Operated
009,2,CCS Main Switch,,Range: Not Operated/Operated
009,3,CCS Switch,SET/(-),Range: Not Operated/Operated
009,4,CCS Switch,RES/(+),Range: Not Operated/Operated
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics (J519) Coding
C01,+00001 = Trailer Hitch installed
C02,+00002 = Trunk Lid Remote Unlocking installed
C03,+00004 = Electric Load Management active
C04,+00008 = Interior Light Control
C05,+00016 = 4-door Chassis
C06,+00032 = Heated Front Seats installed
C07,+00064 = Heated Front Windshield installed
C08,+00128 = Heated Mirrors installed
C09,+00256 = Headlight Washers installed
C10,+00512 = Rain Sensor installed
C11,+01024 = Trunk Lid Remote Unlocking impulse driven
C12,+08192 = Rear Windshield Wiper with Comfort Function installed
C13,+16384 = Electric Fuel Pump Releay installed
C14,Note: The coding is the sum of the individual options.
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Central Electronics (J519) Login
L01,21343 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Terminal 30G Deactivation/Reset
A001,5,Terminal 30G Deactivation/Reset
A001,6,Range: 1-253 (0.66...173 min)
A001,7,Standard: 44 (30 min)
;
A002,0,Front Windshield Heating Activation Time
A002,5,Front Windshield Heating Activation Time
A002,6,Range: 1...253 (0.66...173 min)
A002,7,Special: 254 (infinite)
A002,8,Standard: 29 (20 min)
;
A003,0,Mirror Heating Activation Time
A003,5,Mirror Heating Activation Time
A003,6,Range: 1...253 (0.66...173 min)
A003,7,Standard (through 04/2002): 29 (20 min)
A003,8,Standard (from 05/2002): 254 (infinite)
;
A004,0,Rear Windshield Heating Activation Time
A004,5,Rear Windshield Heating Activation Time
A004,6,Range: 1...253 (0.66...173 min)
A004,7,Standard: 29 (20 min)
A004,8,Special: 254 (infinite)
;
A005,0,Trunk Lid Remote Unlocking
A005,5,Trunk Lid Remote Unlocking
A005,6,Range: 1...253 (0.32-81.6 s)
A005,7,Standard: 3 (1 s)
;
A006,0,Comfort Blinking (Time)
A006,5,Comfort Blinking (Time)
A006,6,Range: 40 ms...10 s
A006,7,Standard: 25 (1 s)
;
A007,0,Comfort Blinking (Cycles)
A007,5,Comfort Blinking (Cycles)
A007,6,Range: 0...5
A007,7,Standard: 3
;
A008,5,Tear Wiping
A008,6,Tear Wiping
A008,7,Range: 0...255 s
A008,8,Standard: 5 s
;
A009,0,Headlight Washer Activation
A009,5,Headlight Washer Activation
A009,6,Range: 0...255 s
A009,7,Standard: 5 s
;
