;
; VAG-COM Label File
;
; Audi Q7 (4L)
;
; Component: J393 - Comfort System (#46)
;
; P/N: 4L0-910-289-???
;
; includes measuring blocks, coding, adaptation and selective output test
;
; created on 29/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 30/May/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Status - Driver's Door
001,1,Door Contact,Switch,Range: Door Open/Door Closed/no communication
001,2,Central Locking,Interior Button,Range: locking/unlocking/not operated/no communication
001,3,Lock Feedback,,Range: locked/unlocked/no communication
001,4,Safe Feedback,,Range: safe/not safe/no communication
;
002,0,Status - Passenger Door
002,1,Door Contact,Switch,Range: Door Open/Door Closed/no communication
002,2,Central Locking,Interior Button,Range: locking/unlocking/not operated/no communication
002,3,Lock Feedback,,Range: locked/unlocked/no communication
002,4,Safe Feedback,,Range: safe/not safe/no communication
;
003,0,Status - Rear Left Door
003,1,Door Contact,Switch,Range: Door Open/Door Closed/no communication
003,2,Central Locking,Interior Button,Range: locking/unlocking/not operated/no communication
003,3,Lock Feedback,,Range: locked/unlocked/no communication
003,4,Safe Feedback,,Range: safe/not safe/no communication
;
004,0,Status - Rear Right Door
004,1,Door Contact,Switch,Range: Door Open/Door Closed/no communication
004,2,Central Locking,Interior Button,Range: locking/unlocking/not operated/no communication
004,3,Lock Feedback,,Range: locked/unlocked/no communication
004,4,Safe Feedback,,Range: safe/not safe/no communication
;
005,0,Window Regulators && Shut-Off Buttons
005,1,Window Regulator,standardized,1 = standardized\n0 = not standardized\n\n?xxx - Driver's Door\nx?xx - Passenger Door\nxx?x - Rear Left Door\nxxx? - Rear Right Door
005,2,Window Regulator,Thermal Protection,1 = active\n0 = not active\n\n?xxx - Driver's Door\nx?xx - Passenger Door\nxx?x - Rear Left Door\nxxx? - Rear Right Door
005,3,Interior Monitoring,Shut-Off Button,Range: operated/not operated/no communication
005,4,Inclination Sensor,Shut-Off Button,Range: operated/not operated/no communication
;
006,0,Rear Lid && Rear Window
006,1,Rear Lid Switch,(Driver's Door),Range: operated/not operated/no communication
006,2,Rear Lid,Contact Switch,Range: lid open/lid closed
006,3,Rear Lid,Soft Touch,Range: operated/not operated
006,4,Rear Window,Break,Anti-Theft-System\n\nRange: not recognized/recognized/not installed
;
007,2,Luggage,Compartment Light,Range: ON/OFF
007,3,Interior Light,,Range: ON/OFF
007,4,Rear Lid,Key Switch,Range: open/closed/not operated
;
008,0,Basic Functions
008,1,Speed Signal
008,2,Engine Speed
008,3,Interior,Temperature
008,4,Fuel Filler,Flap Detection,Range: not recognized/recognized/not installed
;
009,0,Terminal Status
009,1,S-Terminal,,Range: on/off/no communication
009,2,Terminal 15,(hardware input),Range: Term. 15 On/Term. 15 Off
009,3,Terminal 15,(CAN),Range: Term. 15 On/Term. 15 Off/no communication
;
010,1,Terminal 30,(right),Specification: 8.5...15.5 V
010,2,Terminal 30,(left),Specification: 8.5...15.5 V
010,3,Rear Window,Heater,Range: heater on/heater off
010,4,Hood Contact,Switch,Range: lid open/lid closed/no communication
;
011,0,Light Status
011,1,Back-Up Light,,?x - left\nx? - right
011,2,Turn Signal,,?x - left\nx? - right
011,3,Fog Light,,?x - left\nx? - right
011,4,Tail Light,,?x - left\nx? - right
;
012,1,Terminal 54,,?xx - Hardware Terminal 54\nx?x - Terminal 54 CAN\nxx? - Brake Test Switch
012,2,Brake ESP,,?x - Hardware ECD Brake\nx? - CAN ECD Brake
012,3,Brake light,,?xx - left\nx?x - center\nxx? - right
012,4,Garage Door,Opener,Range: ON/OFF
;
013,1,Rear Window,Shaded,Range: ON/OFF/not installed
013,2,Luggage Compartment,Closing Aid,Range: locked/unlocked/not insalled
013,3,Crash,Recognized,Range: Yes/No
013,4,Energy Manager,Shut-Off Stage,Range: 0...6
;
014,0,Interior Monitoring Sensor
014,1,Interior Monitoring,Sensor Status,Range: not installed/no communication/activated/inactive
;
015,0,Alarm Horn
015,1,Alarm Horn,Status,Range: not installed/no communication/activated/inactive
;
016,0,Alarm Sources
;   0 = Door Contact (Driver's Door)
;   1 = Door Contact (Passenger Door)
;   2 = Door Contact (Rear Left)
;   3 = Door Contact (Rear Right)
;   4 = Hood Contact
;   5 = Rear Lid Contact
;   6 = Rear Window Breakage
;   7 = Interior Monitoring
;   8 = Immobilizer (Key not authorized)
;   9 = Intelligent Siren
;  10 = Inclination Sensor
;  11 = Driver Door Control Module
;  12 = Passenger Door Control Module
;  13 = Rear Left Door Control Module
;  14 = Rear Right Door Control Module
;  15 = Terminal 15
; 255 = No Alarm
016,1,Last,Alarm Source
016,2,2nd last,Alarm Source
016,3,3rd last,Alarm Source
016,4,4th last,Alarm Source
;
018,0,Horn - Alarm Trigger
; 0 = No Alarm
; 1 = Comfort Control Module (J393)
; 2 = Communication Break (Ground/Open Circuit)
; 3 = Voltage Supply (Open Circuit)
; 4 = Smart Battery Analysis
018,1,Last,Alarm Trigger
018,2,2nd last,Alarm Trigger
018,3,3rd last,Alarm Trigger
018,4,Alarm Trigger,Counter,Range: 0...15
;
019,0,Interior Monitoring - Alarm Trigger
; 0 = No Alarm
; 1 = Alarm with Vehicle Closed
; 2 = Alarm with open Window
; 3 = Alarm with Fan Operation
019,1,1st Alarm Trigger
019,2,2nd Alarm Trigger
019,3,3rd Alarm Trigger
019,4,4th Alarm Trigger
;
020,1,FPI User ID
020,2,Key Number,(Keyless Entry)
020,3,Rear Lid,Position,Range: 0...100 % / not installed
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,+0000001 = Reserved (always)
C02,+0000002 = 10 Tamper Alarms (PR-B09)
C03,+0000004 = Thatcham inactive (PR-7AA/A8U)
C04,+0000008 = Selective Central Locking (PR-4K2/4K7/4K8)
C05,+0000016 = Anti-Theft Warning System (PR-7AN/7AL)
C06,+0000032 = Inclination Sensor installed (PR-7AN/7AL)
C07,+0000064 = Interior Monitoring (PR-7AL)
C08,+0000128 = Comfort Function via Remote (NOT PR-B29/B30/B34/B35)
C09,+0002048 = Confirmation Anti-Theft System via Horn (PR-A8U)
C10,+0004096 = SAE Rear Lights (PR-A8U)
C11,+0008192 = Light Package (PR-QQ1)
C12,+0016384 = SAFE-Function deactivated (PR-A8U)
C13,+0065536 = No Anti-Theft Delay (0 Seconds)
C14,+0262144 = Sunroof / Open Sky System (PR-3FU)
C15,+1048576 = Luggage Compartment Closing Assistance (PR-4E7/4E9)
C16,+2097152 = Rear Lid Control Module (PR-4E7/4E9)
C17,+4194304 = Fuel Lid Unlock via Driver Door Button
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Personalization - Key 1
A001,5,Personalization - Key 1
A001,6,+00001 = Passenger Door
A001,7,+00002 = Rear Left Door
A001,8,+00004 = Rear Right Door
A001,9,+00008 = Luggage Compartment
A001,10,+00016 = Auto-Lock/Unlock
A001,11,+00032 = Comfort Opening of Front Window Regulators
A001,12,+00064 = Comfort Opening of Rear Window Regulators
A001,13,+00128 = Comfort Opening of Sunroof
A001,14,+00256 = Rear Shade automatic
A001,15,+00512 = Interior Light Dimming 1 %
A001,16,+01024 = Interior Light Dimming 2 %
A001,17,+02048 = Interior Light Dimming 4 %
A001,18,+04096 = Interior Light Dimming 8 %
A001,19,+08192 = Interior Light Dimming 16 %
A001,20,+16384 = Interior Light Dimming 32 %
A001,21,+32768 = Interior Light Dimming 64 %
;
A002,0,Personalization - Key 2
A002,5,Personalization - Key 2
A002,6,+00001 = Passenger Door
A002,7,+00002 = Rear Left Door
A002,8,+00004 = Rear Right Door
A002,9,+00008 = Luggage Compartment
A002,10,+00016 = Auto-Lock/Unlock
A002,11,+00032 = Comfort Opening of Front Window Regulators
A002,12,+00064 = Comfort Opening of Rear Window Regulators
A002,13,+00128 = Comfort Opening of Sunroof
A002,14,+00256 = Rear Shade automatic
A002,15,+00512 = Interior Light Dimming 1 %
A002,16,+01024 = Interior Light Dimming 2 %
A002,17,+02048 = Interior Light Dimming 4 %
A002,18,+04096 = Interior Light Dimming 8 %
A002,19,+08192 = Interior Light Dimming 16 %
A002,20,+16384 = Interior Light Dimming 32 %
A002,21,+32768 = Interior Light Dimming 64 %
;
A003,0,Personalization - Key 3
A003,5,Personalization - Key 3
A003,6,+00001 = Passenger Door
A003,7,+00002 = Rear Left Door
A003,8,+00004 = Rear Right Door
A003,9,+00008 = Luggage Compartment
A003,10,+00016 = Auto-Lock/Unlock
A003,11,+00032 = Comfort Opening of Front Window Regulators
A003,12,+00064 = Comfort Opening of Rear Window Regulators
A003,13,+00128 = Comfort Opening of Sunroof
A003,14,+00256 = Rear Shade automatic
A003,15,+00512 = Interior Light Dimming 1 %
A003,16,+01024 = Interior Light Dimming 2 %
A003,17,+02048 = Interior Light Dimming 4 %
A003,18,+04096 = Interior Light Dimming 8 %
A003,19,+08192 = Interior Light Dimming 16 %
A003,20,+16384 = Interior Light Dimming 32 %
A003,21,+32768 = Interior Light Dimming 64 %
;
A004,0,Personalization - Key 4
A004,5,Personalization - Key 4
A004,6,+00001 = Passenger Door
A004,7,+00002 = Rear Left Door
A004,8,+00004 = Rear Right Door
A004,9,+00008 = Luggage Compartment
A004,10,+00016 = Auto-Lock/Unlock
A004,11,+00032 = Comfort Opening of Front Window Regulators
A004,12,+00064 = Comfort Opening of Rear Window Regulators
A004,13,+00128 = Comfort Opening of Sunroof
A004,14,+00256 = Rear Shade automatic
A004,15,+00512 = Interior Light Dimming 1 %
A004,16,+01024 = Interior Light Dimming 2 %
A004,17,+02048 = Interior Light Dimming 4 %
A004,18,+04096 = Interior Light Dimming 8 %
A004,19,+08192 = Interior Light Dimming 16 %
A004,20,+16384 = Interior Light Dimming 32 %
A004,21,+32768 = Interior Light Dimming 64 %
;
A015,0,Interior Monitoring Sensitivity
A015,5,Interior Monitoring Sensitivity
A015,6,200 = 100 %
A015,7,180 = 90 %
A015,8,160 = 80 %
A015,9,140 = 70 %
A015,10,120 = 60 %
A015,11,100 = 50 %
;
A050,0,Adaptive Brake Light
A050,5,Adaptive Brake Light
A050,6,+1 = Emergency Brake Blinking
A050,7,+4 = Brake Light Surface Amplification
;
A061,0,Comfort Functions
A061,5,Comfort Functions
A061,6,+001 = Comfort Closing: Window Regulators via Remote Control
A061,7,+002 = Comfort Opening: Window Regulators via Remote Control
A061,8,+004 = Comfort Closing: Sunroof via Remote Control
A061,9,+008 = Comfort Opening: Sunroof via Remote Control
A061,10,+016 = Comfort Closing: Window Regulator via Switch Drivers Door
A061,11,+032 = Comfort Opening: Window Regulator via Switch Drivers Door
A061,12,+064 = Comfort Closing: Sunroof via Switch Drivers Door
A061,13,+128 = Comfort Opening: Sunroof via Switch Drivers Door
A061,14,+256 = Comfort Closing: Window Regulators via Lock Cylinder
A061,15,+512 = Comfort Closing: Sunroof via Lock Cylinder
;
A062,0,Central Locking Functions
A062,5,Central Locking Functions
A062,6,+1 = Central Locking Closing Confirmation (Blink)
A062,7,+2 = Central Locking Opening Confirmation (Blink)
A062,8,+4 = Terminal 87 USA Logic
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
T42,Parking Light Left (M43)
T43,Parking Light Right (M44)
T834,Signal for Activation of Heated Rear Window
T959,Indicator Lamp for Central Locking: Safe (K133)
T987,Left Brake Light (M9)
T988,Right Brake Light (M10)
T1503,3rd Brake Light (M25)
T1148,Activation of Safety/Deadbolt Locks in Doors
T1223,Central Locking: Unlock
T1551,Central Locking: Lock
T1483,Rear Lid Remote Unlocking
T1501,Blinker Rear Left (M6)
T1505,Blinker Rear Right (M8)
T1504,License-Plate Light (X)
T1565,Luggage Compartment Light (W3)
T1696,Footwell Lighting Rear Left (W45)
T1697,Footwell Lighting Rear Right (W46)
T1828,Tail-Lamp Left
T1829,Tail-Lamp Right
T2570,Interior Illumination
T2615,Fuel Tank Cap: Lock
T2616,Fuel Tank Cap: Unlock
T2899,Comfort Opening
T2900,Comfort Closing
T2956,Trunk/Hatch Lid Lamp Left
T2957,Trunk/Hatch Lid Lamp Right
T2960,Bumper Lamp Rear Left
T2961,Bumper Lamp Rear Right
;
