;
; VCDS Label File
;
; Copyright © 2004-2009 Ross-Tech, LLC
;
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Touran (1T)
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
;
; Component: J519 - Central Electronics I (#09)
;
; P/N: 1K0-937-049-???
;
; includes measuring blocks, adaptation, selective output test and long coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-09.LBL
; 1T-09.LBL
; 3C-09.LBL
; 1K0-937-049-21-B.LBL
; 3C0-937-049-23-H.LBL
; 3C0-937-049-23-M.LBL
; 3C0-937-049-30-H.LBL
; 3C0-937-049-30-M.LBL
;
; created on 01/Jan/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 24/Jan/2009
;
; requires VCDS 805.0 / LCode 804.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Parking Lights
001,1,Left Front,Parking Light,Specification: 0...100 %
001,2,Right Front,Parking Light,Specification: 0...100 %
001,3,Left Rear,Parking Light,Specification: 0...100 %
001,4,Right Rear,Parking Light,Specification: 0...100 %
;
002,0,Fog Lights/Low Beams
002,1,Left Low Beam,Headlight,Specification: 0...100 %
002,2,Right Low Beam,Headlight,Specification: 0...100 %
002,3,Left Fog Light,,Specification: 0...100 %
002,4,Right Fog Light,,Specification: 0...100 %
;
003,0,Turn Signals
003,1,Left Front,Turn Signal,Specification: 0...100 %
003,2,Right Front,Turn Signal,Specification: 0...100 %
003,3,Left Rear,Turn Signal,Specification: 0...100 %
003,4,Right Rear,Turn Signal,Specification: 0...100 %
;
004,1,Left Side,Turn Signal,Specification: 0...100 %
004,2,Right Side,Turn Signal,Specification: 0...100 %
004,3,Left/Right,High Beam,Specification: 0...100 %
004,4,Xenon-Shutter,,Specification: on/off
;
005,0,Brake Lights
005,1,Left,Brake Light,Specification: 0...100 %
005,2,Right,Brake Light,Specification: 0...100 %
005,3,Center,Brake Light,Specification: 0...100 %
005,4,License Plate,Illumination,Specification: 0...100 %
;
006,0,Back-Up Lights
006,1,Instrument,Illumination,Terminal 58d (Specification: 0...100 %)
006,2,Left,Back-Up Light,Specification: 0...100 %
006,3,Right,Back-Up Light,Specification: 0...100 %
006,4,Left Rear,Fog Light,Specification: 0...100 %
;
007,1,Activation Relay,Terminal 50,Display Range: on/off
007,2,Activation Relay,Terminal 15,cockpit/engine (Display Range: on/off)
007,3,Activation Relay,Terminal 75,Display Range: on/off
007,4,Enabling SAD,,Display Range: active/inactive
;
008,1,Brightness,,Specification: 0...7
008,2,Rain Quantity,,Specification: 0...7
008,3,Right Rear,Fog Light,Specification: 0...100 %
008,4,Footwell,Lighting,Specification: 0...100 %
;
009,1,Terminal 30g,Relay,Display Range: on/off
009,2,Dual Washer,Pump +,Display Range: on/off
009,3,Dual Washer,Pump -,Display Range: on/off
009,4,Heated Rear,Windshield,Display Range: on/off
;
010,1,Horn,,Display Range: operated/n. oprated
010,2,Enabling of,Seat Heating,Display Range: active/inactive
010,3,Electric Fuel,Pump (FP) Relay,Display Range: on/off
010,4,Headlight Washer,System Relay,Display Range: on/off
;
011,1,LED Heated Rear,Windshield,Display Range: on/off
011,2,LED Emergency,Flasher Button,Specification: 0...100 %
011,3,LED Heated,Outside Mirror,Specification: on/off
011,4,Interior,Light Dimmed,Specification: 0...100 %
;
012,1,Coming Home,LED,Display Range: on/off
012,2,Heated Outside,Mirror,Display Range: on/off
012,3,Rate Action 1,Relay Driver 1,Display Range: on/off
012,4,Rate Action 2,Relay Driver 2,Display Range: on/off
;
013,0,Terminals
013,1,Terminal 30,(left),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,2,Terminal 30,(right),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,3,Terminal 30,(ref.),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,4,Terminal 31,(ref.),Range: 0.00...12.75 V\nSpecification: 0.0...1.00 V
;
014,1,Dimming,Potentiometer,Specification: 0...100 %
014,2,Coming Home,Potentiometer,Specification: 0...100 %
;
015,0,Terminals
015,1,Terminal 15,(input),Display Range: on/off
015,2,Terminal 50,(input),Display Range: on/off
015,3,Enabling P/N,,Display Range: on/off
015,4,Terminal L,(input),Display Range: on/off
;
016,1,Light dark,,Display Range: dark = on/bright = off
016,2,Lights on (RLS),,Display Range: on/off
016,3,Front Wiper on
016,4,Wiper turn-around,Position Signal,Display Range: reached/not active
;
017,1,Light Switch,(Light off),Display Range: on/off
017,2,Parking Light,Switch,Display Range: on/off
017,3,Low Beam,Headlight Switch,Display Range: on/off
017,4,AFL Light Switch,,Display Range: on/off
;
018,1,Fog Light Switch,,Display Range: on/off
018,2,Light Switch,Rear Fog Light,Display Range: on/off
018,3,Brake Light Switch,,Display Range: on/off
018,4,Back-Up,Light Switch,Display Range: on/off
;
019,1,Emergency,Flasher Button,Display Range: operated/n. oprated
019,2,Engine Hood,,Display Range: open/closed
019,3,Heated Rear,Windshield Button,Display Range: operated/n. oprated
019,4,Heated Outside,Mirror,Display Range: operated/n. oprated
;
020,0,Backrest Recognition
020,3,Backrest,Left,Display Range: on/off
020,4,Backrest,Right,Display Range: on/off
;
021,0,Rotary Traps
021,1,Rotary Trap LF,,Display Range: on/off
021,2,Rotary Trap RF,,Display Range: on/off
021,3,Rotary Trap LR,,Display Range: on/off
021,4,Rotary Trap RR,,Display Range: on/off
;
022,1,Rear Lid,Main Catch,Display Range: on/off
;
023,1,Rotary Light Switch,Position
023,2,Coming Home,Condition
023,3,Leaving Home,Condition
023,4,AFL Condition
;
024,1,Steering Column,Switch Information,via LIN-Databus
024,2,Terminal 15,(via LIN),Display Range: on/off
024,3,Terminal 50,(via LIN),Display Range: on/off
024,4,Wiper Cycle,Number (via LIN)
;
030,1,Load Management,,Display Range: active/inactive
030,2,Short-Distance,Operations
030,3,Critical,Time Fraction
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Reset Adaptation Channels
A000,5,Reset Adaptation Channels
A000,6,Reset all adaptation channels back
A000,7,to the original factory values.
;
A001,0,Coming-Home Time
A001,5,Coming-Home Time
A001,6,Time which the Coming-Home function will be active.
A001,7,Range: 10...60 Seconds
A001,8,Resolution: 10 Seconds
A001,9,Note: Only active if Byte 00 Bit 7 of Long Coding active.
;
A002,0,Leaving-Home Time
A002,5,Leaving-Home Time
A002,6,Time which the Leaving-Home function will be active.
A002,7,Range: 10...60 Seconds
A002,8,Resolution: 10 Seconds
A002,9,Note: Only active if Byte 00 Bit 5 of Long Coding active.
;
A003,0,Rear Window & Outside Mirror Heater Activation Time
A003,5,Rear Window & Outside Mirror Heater Activation Time
A003,6,Time which the Rear Window and Outside Mirror Heater will be active.
A003,7,Range: 1...254 Minutes
A003,8,Resolution: 1 Minute
;
A004,0,Headlight Washer Activation Time
A004,5,Headlight Washer Activation Time
A004,6,Range: 50...10000 ms
A004,7,Resolution: 50 ms (Adaptation Value * Resolution = Actual Value)
A004,8,Note: Only active if Byte 01 Bit 1 of Long Coding active.
;
A005,0,Footwell Lighting Dimming
A005,5,Footwell Lighting Dimming
A005,6,Range: 20...100 %
A005,7,Resolution: 1 %
A005,8,Note: Only active if Byte 00 Bit 1 of Long Coding active.
;
A006,0,Load Management
A006,5,Load Management
A006,6,Range: 0...3
A006,7,Note: Only active if Byte 02 Bit 3 of Long Coding active.
;
A007,0,Highbeam with Assistance Driving Light
A007,5,Highbeam with Assistance Driving Light
A007,6,0 = inactive
A007,7,1 = active
;
A008,0,Assistance Driving Light Activation/Deactivation Delay
A008,5,Assistance Driving Light Activation/Deactivation Delay
A008,6,Range: 0...10200 ms
A008,7,Resolution: 40 ms
;
;
;---------------------------------------------------
;
; selektive output tests
;
;---------------------------------------------------
;
;
T977,Abblendlicht links/rechts
T2486,Fernlicht links/rechts
T967,Blinker links (vorne/mitte/hinten)
T968,Blinker rechts (vorne/mitte/hinten)
T1064,Instrumentenbeleuchtung (Klemme 58d) und LED Warnblinktaster
T1504,Kennzeichenbeleuchtung (X)
T1701,Innenbeleuchtung mit Dimmung
T1755,Standlicht vorne links/rechts und hinten links/rechts
T1758,Bremslicht links/rechts/mitte
T1830,Nebelschlussleuchte links/rechts
T901,Back-Up Lamps
T59,Interior Lighting
T156,Dual-Waschpumpe (+) - Frontscheibe
T2398,Dual-Waschpumpe (-) - Heckscheibe
T906,Hupe (H1)
T909,Scheibenwischeranlage (V)
T924,Relais für Scheinwerferwaschanlage (J39)
T975,Beheizbare Heckscheibe (Z1) und LED
T1259,Fuel Pump Relay (J17)
T2092,Enabling Heated Seat
T80,Freischaltung Schiebedach
T2377,Scheibenwischer auf Richtungsänderungsposition
T61,Beleuchtung Fußraum
T920,Beheizbarer Außenspiegel und LED
T1483,Fernentriegelung für Heckklappe
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,3,Daytime Running Lights (Scandinavia) active
LC,00,4,Daytime Running Lights (North America)
LC,01,2,Electronic Fuelpump Relay installed (Gasoline only)
LC,01,3,Rear Wiper installed
LC,01,4,Heated Side Mirrors installed
LC,01,5,Rear Lid Remote Opening
LC,01,6,Rear Lid Remote Opening - Release
LC,01,7,Rear Wiper with Front Wiper continiously active
LC,02,0,Rear Wiper with Front Wiper intermittent active
LC,02,1,Comfort Turn Signals
LC,02,2,Cold Lamp Diagnosis active
LC,02,3,Load Management active
LC,02,5,Rear Lid Remote Openening	(0 = Impuls activated / 1 = Contact activated)
LC,02,6,Side Turn Signal Lights installed
LC,02,7,Seat Heating installed
LC,03,0,Relay Terminal 15 installed
LC,03,5,Teardrop Wiping for Rear Window active
LC,04,0,Auxiliary Heater installed
LC,05,0-7,50,Headlight Washer Delay
LC,05,0-7,50,Decimal Value (Resolution 50 ms) (Example: 20 is 20 x 50 = 1000 ms)
LC,06,0-7,50,Headlight Washer Activation Time
LC,06,0-7,50,Decimal Value (Resolution 50 ms) (Example: 16 is 16 x 50 = 800 ms)
LC,07,0-7,1,Turn Signal Front left/right as Parking Light Front left/right (USA and Canada)
LC,07,0-7,1,Decimal Value (Resolution: 1%)
LC,08,0-7,1,Daytime Running Light Dimming
LC,08,0-7,1,Decimal Value (Resolution: 1%)
LC,09,0-7,1,Rear Brake Light as Parking Light
LC,09,0-7,1,Decimal Value (Resolution: 1%)
LC,10,0-7,1,Rear Fog Light as Parking Light
LC,10,0-7,1,Decimal Value (Resolution: 1%)
LC,11,0-7,1,Front Parking Light Dimming
LC,11,0-7,1,Decimal Value (Resolution: 1%)
LC,12,0-7,1,Rear Parking Light Dimming
LC,12,0-7,1,Decimal Value (Resolution: 1%)
LC,13,0-7,1,Backup Function: Rear Side Turn Signal as Parking/Brake Light
LC,13,0-7,1,Decimal Value (Resolution: 1%)
LC,14,0-7,1,Backup Function: Front Parking Light as Side Turn Signals
LC,14,0-7,1,Decimal Value (Resolution: 1%)
LC,15,0-7,1,Backup Function: Rear Parking Light as Side Turn Signals
LC,15,0-7,1,Decimal Value (Resolution: 1%)
LC,16,0-7,1,Backup Function: Front Fog Lights as Low Beam Headlight
LC,16,0-7,1,Decimal Value (Resolution: 1%)
LC,17,0,Emergency Brake Flash Light active
LC,17,3,Diagnosis Terminal 50 active
LC,18,0,Cold Diagnosis License Plate Lights active
LC,18,4,Cold Diagnosis High Beam active
LC,18,5,Cold Diagnosis Turn Signals active
LC,18,7,Cold Diagnosis Side Turn Signals active
LC,19,1,Cold Diagnosis Front Parking Lights active
LC,19,2,Cold Diagnosis Rear Parking Lights active
LC,19,3,Diagnosis Rear Parking Lights active
LC,20,0-7,1,Front Fog Light Dimming (Standard 5C)
LC,20,0-7,1,Decimal Value (Resolution: 1%)
;
