;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Component: R - Radio (#56) - DELTA 6/Premium 6
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3B-56.LBL
; 3B7-035-1xx-56.LBL
;
; includes measuring blocks and coding
;
; created on 02/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 25/Feb/2013
;
; requires VCDS 11.11.5 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Supply Voltage,(Terminal 30),Specification: 5...18 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Telephone-Mute
001,4,Telephone-Mute,Status,Range: ON/OFF
;
002,0,Speaker/Line-Out (Front)
002,1,Location/Type
002,2,Status
002,3,Location/Type
002,4,Status
;
003,0,Speaker/Line-Out (Rear)
003,1,Location/Type
003,2,Status
003,3,Location/Type
003,4,Status
;
004,0,Remote Feed Antenna
004,1,Antenna,Type
004,2,Component
004,3,Antenna,Status
;
005,0,IF-Output
005,1,Component
005,2,IF-Output,Status
;
007,0,Communication Status CD-Changer (R41)
007,1,Component
007,2,CD-Changer,Status
;
008,0,Signal Strength
008,1,Signal Strength
008,2,Signal Strength,Tuner
;
025,0,Internal Control Module Malfunctions
025,1,Control Module,Status,01 = Button(s) Jam\n02 = Checksum Error ROM/EPROM/Flash-ROM\n03 = Writing Error EEPROM\n04 = CC-Drive (Casette) Error\n05 = CD/DVD-Drive Error
; 01 = Button(s) Jam
; 02 = Checksum Error ROM/EPROM/Flash-ROM
; 03 = Writing Error EEPROM
; 04 = CC-Drive (Casette) Error
; 05 = CD/DVD-Drive Error
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,000?xxx: Radio Configuration I
C02,+1 = IF-Output
C03,+2 = Telephone (via CAN)
C04,+4 = Multi-Function Steering Wheel (via CAN)
C05,000x?xx: Speaker Channels
C06,0 = No passive Speakers (Sound System)
C07,2 = 2 passive Speakers (Front)
C08,4 = 4 passive Speakers (Front & Rear)
C09,000xx?x: Sound System Correction
C10,0 = No Sound System (No Correction)
C11,1 = Sound System with Cloth Interior
C12,2 = Sound System with Leather Interior
C13,3 = Monsoon (USA only)
C14,000xxx?: Radio Configuration II
C15,+1 = Active/Remote Supplied Antenna
C16,+2 = CD-Changer
C17,+4 = CAN-Secondary Display (Board Computer/large Display)
;
