;
; VAG-COM Labelfile
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia (1Z)
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Golf Plus (5M) / VW Touran (1T)
;
; Component: Radio-/Navigation System (#56) - MFD2-CD
;
; P/N: 1T0-035-095-??? / 1Z0-035-194-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1Z-56.LBL
; 1T0-035-095.LBL
;
; created on 27/Mar/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 18/Feb/2008
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Battery Voltage,(Terminal 30),Specification: 5...18 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Input,Telephone-Mute
001,4,Input,Telephone-Mute,CAN-Databus signal (Display Range: on/off)
; 
002,0,Speakers/Line-Out (Front)
002,1,Location/Type
002,2,Condition
002,3,Location/Type
002,4,Condition
;
003,0,Speakers/Line-Out (Rear)
003,1,Location/Type
003,2,Condition
003,3,Location/Type
003,4,Condition
;
004,0,Remote Feed Antenna
004,1,Type
004,2,Antenna
004,3,Condition
;
005,1,IF-Output
005,2,IF-Output,Status
005,3,CD-Connection
005,4,CD-Connection,Status,Display Range: OK/not OK
;
006,0,CAN-Databus Infotainment (Communication)
006,1,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
006,2,Telephone,,Display Range: Telephone 1/Telephone 0
006,3,Steering Wheel,Electronics,Specification: St. Wheel 1\nDisplay Range: St. Wheel 1/St. Wheel 0
006,4,TV-Tuner,,Display Range: TV-Tuner 1/TV-Tuner 0
;
025,0,Internal Control Module Malfunctions
025,1,Control Module,Status
; 01 = Button(s) Jam
; 02 = Checksum Error ROM/EPROM/Flash-ROM
; 03 = Writing Error EEPROM
; 04 = CC-Drive (Casette) Error
; 05 = CD/DVD-Drive Error
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00,Radio/Navigation System MFD2-CD (J503) Coding
C01,00?xxxx: Configuration I
C02,+1 = TV-Tuner
C03,00x?xxx: Configuration II
C04,+1 = IF-Output
C05,+2 = Telephone Control (CAN)
C06,+4 = Multi-Function Steering Wheel (CAN)
C07,00xx?xx: Speaker Channels
C08,0 = Sound System (active Speakers)
C09,2 = 2 passive Speakers (Front)
C10,4 = 4 passive Speakers (Front & Rear)
C11,00xxx?x: Sound System Correction
C12,0 = No Sound System (No Correction)
C13,1 = Sound System with Cloth Interior (with Open Circuit Recognition)
C14,2 = Sound System with Leather Interior (with Open Circuit Recognition)
C15,3 = Sound System with Cloth Interior (without Open Circuit Recognition)
C16,00xxxx?: Configuration III
C17,+1 = Active/Remote feed Antenna
C18,+2 = CD-Changer
;
