;
; VAG-COM label file - 3D0-919-887.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
;
; component: Control Module for Navigation with CD Mechanism - J401 - (#37)
;
;       p/n: 3D0 919 887 A  Component: NAVIGATION 0147 Coding: 0400000 (2004 Phaeton - North America)
;       p/n: 3D0 919 887 B  Component: NAVIGATION 0168 Coding: 0500735 (2004 Phaeton - ROW) - Daniel, with DVD player
;       p/n: 3D0 919 887 E  Component: NAVIGATION 0168 Coding: 0000000 (2004 Phaeton - ROW) - DD AM 2662
;       p/n: 3D0 919 887 F  Component: NAVIGATION 0168 Coding: 0400000 (2005 Phaeton - North America)
;
; NOTE: A CD ROM is available to flash upgrade this controller to 0168 status, VW part number 3D0 919 278,
;       release 136 ZAB.
;
;       Part Numbers for Other Platforms (it is not known whether this label file will work with these)
;          7L6 919 887 A Component: Navigation 0627 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 A Component: Navigation 0634 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 B Component: Navigation 0627 Coding: 0000002 (Touareg - North America)
;          7L6 919 887 D Component: Navigation 0628 Coding: 0000002 (Touareg - North America)
;          3W0 919 887 A Component: NAVIGATION 0168 Coding: 0400000 (Bentley Continental GT - North America)
;
;
; includes coding & measured value blocks
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; Modification History
;
; 20/March/2005 - Michael - additional MVB data added
; 23/November/2005 - Michael - note added about CD ROM available for flash upgrade.
; 29/November/2005 - Michael - all MVB and adaptation channels mapped,
;                            - additional MVBs identified and labelled.
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Phaeton Control Module for Navigation with CD Mechanism - J401
C1,x?xxxxx
C2,4 - Byte Code Valid
C3,0 - No Byte Code
C4, 
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
; REMARK: VAG-COM can be very slow to read some of these blocks, be patient.
;
001,0,General Vehicle Information
001,1,Filtered voltage,supply T30
;
002,0,Inputs used by Navigation System
002,1,Unknown
002,2,Unknown
002,3,Reverse signal,for dead reckoning,
;
003,0,GPS Antenna Status (On-glass Rear Window Antenna - not the OnStar shark-fin)
003,1,
003,2,GPS Antenna
003,3,Gyro Voltage
;
004,0,Satellite Related Information
004,1,GPS Reception,status
004,2,Satellites,in view now,0 to 8 possible
004,3,Satellites,available,typically between 25 and 35
;
005,0,Wheel circumference used for measuring distance travelled when satellite reception is lost.
005,1,
005,2,Tire,circumference
;
006,0,Navigation CD Player Status
006,1,Eject Button,Status
006,2,CD ROM,Drive Status
;
007,0,*Next MVB used is 080
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
;
081,0,Expanded Control Module Identification
;
082,0,Expanded Control Module Identification
;
083,0,*Next MVB used is 247
; 
247,0,Present Vehicle Position (Latitude and Longitude)
;
248,0,Vehicle Speed - Day of Week - UTC Time (from satellites)
;
249,0,Unknown
;
250,0,Temperature of Controller Components and Blower Status
250,2,Fan Status
;
251,0,Unknown
;
252,0,Unknown
;
253,0,Unknown
;
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;Remark: A Security access code is required to adapt this controller.
;
;


