;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi A6 (4B)
;
; Component: J255 - Heating/Air Conditioning (#08) (< MY 2001)
;
; P/N: 4B0-820-043-???
;
; includes measuring blocks, basic setting coding and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4B-08.LBL
; 4B0-820-043-MY1.LBL (> MY 2001)
; 4B0-820-043-MY2.LBL (MY 2002 >)
;
; created on 10/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Apr/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
B001,0,Potentiometer && Flap Alignment
B001,1, , , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Heating/Air Conditioning (J255) Coding
C01,00?xx: Country
C02,0 = Rest of World (RoW)
C03,1 = Nort American Region (NAR)
C04,2 = Japan (JP)
C05, 
C06,00x?x: Engine (Cylinder)
C07,4 = 4-Cylinder Engine
C08,6 = 6-Cylinder Engine
C09,8 = 8-Cylinder Engine
C10, 
C11,00xx?: Vehicle & Engine (Type)
C12,0 = Gasoline Engine with Left-Hand-Drive (LHD)
C13,1 = Gasoline Engine with Right-Hand-Drive (RHD)
C14,3 = Diesel Engine with Left-Hand-Drive (LHD)
C15,4 = Diesel Engine with Right-Hand-Drive (RHD)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;

;
