;
; VCDS Label File
;
; Copyright © 2007-2011 Ross-Tech, LLC
;
; Seat Ibiza (6L) / Skoda Fabia (6Y) / VW Polo (9N)
;
; Component: J104 - Brake Electronics (#03) -  Bosch 5.7 ABS/ASR/EDS/ESP
;
; P/N: 6Q0-907-37?-???
;
; Includes measuring blocks, basic setting, login, coding and misc
;
; This File is part of a Label File Package,
; make sure you have all of the following Files.
;
; 6Q-03.LBL
; 6R-03.LBL
; 6Q0-907-37x-ABS.LBL  (ABS/EDS 5.7)
; 6Q0-907-37x-ABS2.LBL (ABS/EDS MK60)
; 6Q0-907-37x-ASR.LBL  (ABS/EDS/ASR 5.7)
; 6Q0-907-37x-ESP.LBL  (ABS/EDS/ASR/ESP 5.7)
; 6R0-907-37x-ABS.LBL  (ABS/EDS 8.0)
; 6R0-907-37x-ASR.LBL  (ABS/EDS/ASR 8.0)
; 6R0-907-37x-ESP.LBL  (ABS/EDS/ASR/ESP 8.0)
; 
; created on 22/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 20/Jun/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0...255 km/h
001,2,Wheel Speed,Front Right,Display Range: 0...255 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0...255 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0...255 km/h
;
B001,0,Steering Angel Sensor (G85) Alignment
B001,1,Steering Angel,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,0,Switches && Buttons
002,1,Brake Test Switch,,Display Range: 0/operated
002,2,Brake Light Switch,,Display Range: 0/operated
002,3,Parking Brake,Button,Display Range: 0/operated
002,4,ESP-Passive,Button,Display Range: 0/operated
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
B003,0,System Function Test Activation
B003,1,Status, , 
B003,2, , , 
B003,3, , , 
B003,4, , , 
;
004,0,Standing Time && EDL-T Flag
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,Sensor (G85),Display Range: -720.0...+720.0 °\nTolerance: +/- 5.0 °
005,2,Turn Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n\n-41.0 bar = short to ground\n290 bar = short to plus
005,4,Lateral,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Voltage Supply,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON/OFF\nSpecification: ON
006,3,Return Flow Pump,Status,Display Range: ON/OFF\nSpecification (Ignition ON/Engine OFF): OFF
006,4,Workshop Code
;
B010,0,Brake System Bleeding
B010,1,Status, , 
B010,2, , , 
B010,3, , , 
B010,4, , , 
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor,Specification: Steer. ang. 1
125,2,Automatic,Transmission,Specification: Transm. 1
125,3,Engine,,Specification: Engine 1
125,4,Instrument Cluster,,Specification: Instruments 1
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Brake Electronics (J104) Login
L01,40168 = Basic Setting Enabling
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104/Bosch 5.7 ABS/ASR/ESP) Coding
C01,Refer to the Factory Repair Manual for Coding Details.
C02, 
C03,If a Factory Repair Manual is not available or does not
C04,contain Coding Information please contact Ross-Tech or
C05,your local VCDS Reseller/Distributor for Assistance.
C06, 
C07,http://www.ross-tech.com/contact.html
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,ABS/ASR/ESP Bosch 5.7
;
