;
; VCDS Label File
;
; Copyright © 2012+ Ross-Tech, LLC
;
; Audi Cabriolet (8G) / Audi A8 (4D)
;
; Component: J362 - Immobilizer (#25)
;
; P/N: 4B0-953-234-???
;
; includes measuring blocks, adaptation, login and misc
;
; created on 19/Jul/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 19/Jul/2012
;
; requires VCDS 11.11.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
022,0,System Status
022,1,Engine Start,permitted,Specification: Yes\nRange: Yes/No
022,2,Engine (ECU),responds,Specification: Yes\nRange: Yes/No
022,3,Key Status,OK,Specification: Yes\nRange: Yes/No
022,4,Number of,adapted Keys,Specification: 1...8

023,0,Key && Adaptation Status
023,1,Variable Code,authorized,Specification: Yes\nRange: Yes/No
023,2,Key Status,(Transponder Lock),Range: Yes/No
023,3,Fixed Code,authorized,Specification: Yes\nRange: Yes/No
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A021,0,Immobilizer (Key Adaptation)
A021,3,Key Count
A021,5,Immobilizer (Key Adaptation)
A021,6,Prior to Adapting new Keys the Adaptation has to be enabled by
A021,7,logging in using the Immobilizer PIN/SKC. The Adaptation Value
A021,8,is the number of all Keys to be adapted (Max. 4). After Saving
A021,9,the Adaptation Value the first Key is adapted. The Learning of
A021,10,all Keys should not exceed 30 Seconds.
A021,11,Proceed until all Keys are adapted:
A021,12,- Switch the Ingnition OFF and take out the Key.
A021,13,- Switch the Ignition ON using the next Key.
A021,14,- The Immobilizer Lamp should light up for 2 Seconds and then switch OFF.
A021,15,- The Key is now adapted.
;
;
;---------------------------------------------------
;
; Login
;
;---------------------------------------------------
;
;
L00,Immobilizer (J362) Login
L01,Prior to Key Learning or adapting a new USED Immobilizer
L02,Control Module the Vehicle specific PIN/SKC (IMMO-Login)
L03,of the new USED Immobilizer Control Module has to be used
L04,to enable the adaptation.
L05,You'll find the PIN/SKC on the Key Tag of the additional
L06,Key (of the Donor Car) or you can acquire it through your
L07,responsible Distribution Center or Importer.
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,IMMO II
;
