;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Touran (1T)
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
;
; Component: J104 - Brake Electronics (#03) - ABS MK60 (FWD)
;
; P/N: 1K0-907-37?-???
;
; includes measuring blocks, basic setting, coding, adaptation and security access
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-03.LBL
; 1K0-907-379-MK60-A.LBL (MK60 AWD)
; 1K0-907-379-MK60-F.LBL (MK60 FWD)
; 1K0-907-379-MK70.LBL  (MK70)
;
; created on 31/Mar/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 08/Jun/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
002,0,Starting Wheel Speed
002,1,Speed Sensor,Front Left (G47),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,2,Speed Sensor,Front Right (G45),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,3,Speed Sensor,Rear Left (G46),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,4,Speed Sensor,Rear Right (G44),Range: 0.0...254.0 km/h (255.0 km/h = standing)
;
003,0,Switches and Warning Lights
003,1,Brake Light,Switch (F),Range: Not Oper./Operated
003,2,Brake System,Warning L. (K118),Range: ON/OFF
003,3,ABS,Warning L. (K47),Range: ON/OFF
003,4,ASR/ESP,Warning L. (K155),Range: ON/OFF
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
004,2,Lateral Acc.,Sensor (G200),Specification: ± 1.5 m/s²
004,3,Rotation Rate,,Specification: ± 2.5 °/s
;
005,0,Brake Pressure
005,1,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
005,2,Steering Angle,Sensor Condition,Display Range: Initialised/N. Initialised/Implausible
;
007,0,ASR Button
007,1,ASR Button,,Display Range: operated/n. operated
;
010,0,Additional Functions
010,1,Trailer,Stabilisation
010,2,Brake Wiping,(Front)
;
011,0,Speed Encoder Errors (Front Left)
;
012,0,Speed Encoder Errors (Front Right)
;
013,0,Speed Encoder Errors (Rear Left)
;
014,0,Speed Encoder Errors (Rear Right)
;
016,0,Tire Pressure Monitoring (TPMS) I
016,1,Mileage at,last Warning
;
017,0,Tire Pressure Monitoring (TPMS) II
017,1,Mileage at,last Initialization
;
018,0,Tire Pressure Monitoring (TPMS) III
018,1,TPMS Button,Status,Range: Operated/Not Oper.
018,2,Parking Brake,Status,Range: Operated/Not Oper.
;
031,0,Tire Pressure Monitoring (TPMS) IV
; 0 = Nothing Learned
; 1 = Only 1st Threshold powered
; 2 = Only 2nd Threshold powered
; 3 = Only 1st Threshold rolling
; 4 = Only 2nd Threshold rolling
; 5 = 1st Threshold powered and rolling
; 6 = 1st Threshold powered and 2nd Threshold rolling
; 7 = 2nd Threshold powered and 1st Threshold rolling
; 8 = 2nd Threshold powered and rolling (Optimal)
031,1,Speed Ranges I
; 5?xxx = Speed Range 1 ( 15 -  70 km/h)
; 5x?xx = Speed Range 2 ( 70 - 100 km/h)
; 5xx?x = Speed Range 3 (100 - 130 km/h)
; 5xxx? = Speed Range 4 (130 - 160 km/h)
031,2,Speed Ranges II
; 5?xxx = Speed Range 5 (160 - 190 km/h)
; 5x?xx = Speed Range 6 (190 - 220 km/h)
; 5xx?x = Speed Range 7 (220 - 250 km/h)
031,3,Curve/Wheel,Recognition
; 5?x00 = Curve Recognition (0 = No Curve / 1 = Left or Right Curve learned / 2 = Complete Curve learned)
; 5x?00 = Wheel Recognition (0 = inactive / 1 = activ)
;
B042,0,Tire Pressure Monitoring System (TPMS) Reset
B042,1,Tire Pressure,Monitoring System
B042,2, , , 
B042,3,Reset Status
B042,4, , , 
;
B060,0,Adjustment of Steering Angle Sensor (G85)
B060,1,Adjustment
B060,2,Adjustment,Status
B060,3,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
;
B063,0,Adjustment of Lateral Acceleration Sensor (G200)
B063,1,Adjustment
B063,2,Adjustment,Status
B063,3,Lateral Acc.,Sensor (G200),Specification: ± 1.5 m/s²
;
B066,0,Adjustment of Brake Pressure Sensor (G201)
B066,1,Adjustment
B066,2,Adjustment,Status
B066,3,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
;
080,0,Advanced Control Module Identification I
;
B093,0,Initiation of ESP Driving Test
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine
125,2,Steering Angle,Sensor (G85)
125,3,All-Wheel-Drive
125,4,Transmission
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Instrument,Cluster (J285)
126,2,CAN-Gateway,(J533)
126,3,Immobilizer
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
C01,Model:
C02,+0000000 = Audi A3 (8P) / Seat Leon (1P) / VW Golf/Jetta (1K)
C03,+0000064 = VW Touran (1T)
C04,+0000080 = VW Caddy (2K)
C05,+0000096 = VW Eos (1F)
C06,+0000112 = Seat Altea/Toledo (5P) / VW Golf Plus (5M)
C07,Frontbrakes (Sensor Cluster OLD - ONLY VW Caddy (2K) & VW Touran (1T) & Audi A3 (8P) <MY2005):
C08,+0000005 = FS III 54 15" (PR-1ZF/1ZM/1ZC)
C09,+0000006 = FN III 54 15"/16" (PR-1ZE/1LJ/1ZP/1ZD/1LL)
C10,+0000009 = FRNG 57 17" (PR-1LK)
C11,Frontbrakes (Sensor Cluster NEW - All Others & Audi A3 (8P) MY2006>):
C12,+0000001 = FS III 54 15" (PR-1ZF/1ZM/1ZC)
C13,+0000002 = FN III 54 15"/16" (PR-1ZE/1LJ/1ZP/1ZD/1LL)
C14,+0000008 = FRNG 57 17" (PR-1LK)
C15,Suspension:
C16,+0000640 = Standard/Sport Suspension (PR-2UA/2UC OR PR-UA0/UA1/UA9)
C17,+0001152 = Rough Road/Comfort Suspension (PR-2UB/2UD OR PR-UA2)
C18,Engine:
C19,+0002048 = 1.4l MPI / 1.6l & 1.6l FSI
C20,+0004096 = All Other Engines & All Engines with Automatic Transmission
C21,+0006144 = 2.0l TDI PD
C22,Tire Pressure Monitoring (TPMS):
C23,+0000000 = with Tire Pressure Monitoring (PR-7K1/7K6)
C24,+0016384 = without Tire Pressure Monitoring (PR-7K0)
C25,Notes: See production codes on car data plate. Coding is the sum of the individual options.
;
;Sensor Cluster OLD: Installed behind glove compartment (ONLY VW Caddy (2K) & VW Touran (1T) & Audi A3 (8P) <MY2005).
;Sensor Cluster NEW: Installed under passenger seat (All Others & Audi A3 (8P) MY2006>).
;
;
;---------------------------------------------------
;
; login/coding-ii
;
;---------------------------------------------------
;
; Older versions use 11 instead of 16!
L00,Brake Electronics (J104) Coding-II
L01,40168 = Basic Setting Enabling
;
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
; Newer versions use 16 instead of 11!
S00,Brake Electronics (J104) Security Access
S01,15082 = Adaptation Enabling
S02,40168 = Basic Setting Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A056,0,Trailer Stabilization
A056,3,Stabilization,Status
A056,5,Trailer Stabilization
A056,6,0 = Trailer Stabilization inactive
A056,7,1 = Trailer Stabilization active
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,ABS/ESP MK60 FWD
;
