Technical Specifications

# Electrical

> Perfection 1260 and 1260 Photo
> Perfection 1660 Photo
> Perfection 2400 Photo

## Perfection 1260 and 1260 Photo

Input voltage range | DC 15.2 V
Rated current | 1.2 A
Power consumption | 20 W

| Note:

Check the label on the back of the scanner for voltage information.

[Top]

## Perfection 1660 Photo

Input voltage range | DC 24 V
Rated current | 0.8 A
Power consumption | 17 W

| Note:

Check the label on the back of the scanner for voltage information.

[Top]

## Perfection 2400 Photo

Input voltage range | DC 24 V
Rated current | 0.8 A
Power consumption | 17 W

| Note:

Check the label on the back of the scanner for voltage information.

### ENERGY STAR Compliance

As an ENERGY STAR® Partner, EPSON has determined that this product meets the ENERGY STAR guidelines for energy efficiency.

The International ENERGY STAR Office Equipment Program is a voluntary partnership with the computer and office equipment industry to promote the introduction of energy-efficient personal computers, monitors, printers, fax machines, copiers, and scanners, in an effort to reduce air pollution caused by power generation.

[Top]

Previous | Next